InS_StArT
OCE2XODI.COM
1.0
^Olicom OC-2232 Ethernet PCMCIA Card,OCE2XODI.COM,IEM
!OIEM(PORT)I/O port
?If you want to specify a specific IO Port Base Address for the OC-2232, use this parameter. If no value is entered, the driver will search for an OC-2231 at the IO Port adresses shown above, starting at the top of the list (300h).
300
320
340
360
240
260
280
2A0
2C0
2E0
200
220
380
3A0
3C0
3E0
$OIE0(NODE ADDRESS)Node address
0
FFFFFFFFFFFF
*OIE0(FRAME)Media frame type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
