InS_StArT
OCE3XODI.COM
1.0
^Olicom Ethernet MCA 10/100 Adapter,OCE3XODI.COM,IE0
^Olicom Ethernet ISA 10/100 Adapter,OCE3XODI.COM,00M
!O00M(PORT)I/O Port
?If you want to specify a specific IO Port Base Address for the MCA 10/100, use this parameter. If no value is entered, the driver will search for an OC-2335 at the IO Port adresses shown above, starting at the top of the list (300h).
300
340
380
3C0
200
240
280
2C0
!OIE0(PORT)I/O Port
?If you want to specify a specific IO Port Base Address for the ISA 10/100, use this parameter. If no value is entered, the driver will search for an OC-2375 at the IO Port adresses shown above, starting at the top of the list (300h).
300
320
340
360
240
260
280
2A0
2C0
2E0
200
220
380
3A0
3C0
3E0
$OIEM(NODE ADDRESS)Node address
0
FFFFFFFFFFFF
*OIEM(FRAME)Media frame type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIEM(SPEED)Media speed
?Media speed used by adapter. AUTO is default and is automatic media detection.
AUTO
10
100
!OIEM(DUPLEX)Duplex mode
?Duplex mode used by adapter. AUTO is default and is automatic media detection.
AUTO
HALF
FULL
InS_EnD

