InS_StArT
OCE4XODI.COM
1.0
^Olicom Ethernet PCI/II 10/100 Adapter,OCE4XODI.COM,IEM
!OIEM(PORT)I/O Port
?If more than one Ethernet adapter is present, use this parameter to identify the adapter. If omitted, the driver will use the first it finds. The 1st PCI adapter is selected by the entering the (fake) Port address FFF0. FFF1 selects the 2nd etc.
FFF0
FFF1
FFF2
FFF3
FFF4
FFF5
FFF6
FFF7
$OIEM(NODE ADDRESS)Node address
0
FFFFFFFFFFFF
*OIEM(FRAME)Media frame type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIEM(SPEED)Media speed
?Media speed used by adapter. AUTO is default and is automatic media detection.
AUTO
10
100
!OIEM(DUPLEX)Duplex mode
?Duplex mode used by adapter. AUTO is default and is automatic media detection.
AUTO
HALF
FULL
InS_EnD

