InS_StArT
ILANPCI.COM
1.0
^Racal InterLan PCI Ethernet MLID,ILANPCI.COM,000
?The driver is self-configuring.
!O000(BUSTYPE)PCI Mechanism
?If you know the PCI mechanism type, you can specify it here.  The driver assumes mechanism 2.
PCI1
PCI2
$OIE0(NODE ADDRESS)
0
7FFFFFFFFFFF
*RIE0(FRAME)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
