InS_StArT
NI6510.COM
1.01
^Racal InterLan XLerator/EB/NI6510 Ethernet MLID,NI6510.COM,IEO
!OIE0(PORT)
?Driver is self-configuring. If multiple NI6510 cards are in the system, IO Base Addr. must be specified.
300
320
340
360
$OIE0(NODE ADDRESS)
0
7FFFFFFFFFFF
*OIE0(FRAME)
?NOTE: Ethernet_802.2 is the default frame type for ODI drivers.
Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD
