InS_StArT
DC21040.COM
1.0
^Digital Equipment Corporation EB40,DC21040.COM,0E0
^Digital Equipment Corporation DE425,DC21040.COM,0E0
?This driver supports both EISA and PCI machines
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*O0E0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
Ethernet_802.2
Ethernet_802.3
@Ethernet_II
Ethernet_SNAP
!O0E0()Media Access Type
?NOTE: Media access type will be autodetected on driver's load
TP
TP_NO_LINK_TEST
TP_FULL_DUPLEX
AUI
BNC
@AUTODETECT 
InS_EnD




 
