InS_StArT
ES3210.COM
1.0
^Racal InterLan ES3210 Ethernet MLID,ES3210.COM,0E0,RII0102
?Driver is self-configuring.
$O0E0(NODE ADDRESS)
0
7FFFFFFFFFFF
*O0E0(FRAME)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
@Ethernet_II
InS_EnD

