InS_StArT
ILANAT.COM
1.0
^Racal InterLan AT/NI6610 Ethernet MLID,ILANAT.COM,IE0
!OIE0(PORT)
?The driver is self-configuring.  If multiple InterLan AT network boards are installed in the system, the Base I/O Port must be specified.
300
320
340
360
380
3A0
3C0
3E0
$OIE0(NODE ADDRESS)
0
7FFFFFFFFFFF
*OIE0(FRAME)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
@Ethernet_II
InS_EnD
