InS_StArT
NE1000.COM
1.1
^Novell Ethernet NE1000,NE1000.COM,IE0000
?Please select the options that match your board's jumper settings.
!RIE0000(IRQ)Hardware Interrupt
2
@3
5
7
!RIE0000(PORT)Base I/O Port
@300
320
340
360
$OIE0000(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
@Ethernet_II
Ethernet_SNAP
InS_EnD
