InS_StArT
PCNTNW.COM
1.0
^HP PC LAN Adapter NC/16 (J2405B),PCNTNW.COM,IE0
?Please select the options that match your board's configuration.
!RIE0 (INT) Hardware Interrupt
?Select the interrupt that matches the value chosen in HPNCSET.
@3
4
5
9
10
11
12
15
!RIE0 (DMA) Hardware DMA Channel
?Select the DMA channel value that matches the value chosen in HPNCSET.
3
@5
6
7
!RIE0 (PORT) Base I/O Port
?Select the I/O base address that matches the value chosen in HPNCSET. 
200
220
240
260
280
2A0
2C0
2E0
@300
320
340
360
380
3A0
3C0
3E0
$OIE0 (NODE ADDRESS) Node Address Override
0
7fffffffffff
*RIE0 (FRAME) Media Frame Type(s)
?Note: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
@Ethernet_II
Ethernet_SNAP
InS_EnD
