InS_StArT
SMC8000.COM
1.0
^SMC Ethernet LAN Adapter,SMC8000.COM,IEM
?Please select the options that match your boards settings
!RIE0 (PORT) I/O Base Port
200
220
240
260
@280
2A0
2C0
2E0
300
320
340
360
380
3A0
3C0
3E0
!R00M (SLOT) Microchannel Slot
1
2
3
4
5
6
7
8
!OIE0 (INT) Hardware Interrupt
? This value is required for older (8003 style) cards
2
@3
4
5
7
10
11
14
15
!OIE0 (MEM) Memory Base
? This value is required for older (8003 style) cards
c0000
c2000
c4000
c6000
c8000
ca000
cc000
ce000
@d0000
d2000
d4000
d6000
d8000
da000
dc000
de000
e0000
e2000
e4000
e6000
e8000
ea000
ec000
ee000
!OIEM (NODE ADDRESS) Override Node Address
0
7FFFFFFFFFFF
*RIEM (FRAME) Frame Types
Ethernet_802.2
Ethernet_802.3
@Ethernet_II
Ethernet_SNAP
InS_EnD
