InS_StArT
SMCPWR.COM
1.0
^SMC 8432/PCI,SMCPWR.COM,0E0
?Help line was intentionally left blank
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*O0E0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
Ethernet_802.2
Ethernet_802.3
@Ethernet_II
Ethernet_SNAP
!O0E0()Media Access Type
?NOTE: Twisted Pair connector is the default media access type
@TP
TP_FULL_DUPLEX
AUI
AUTOSENSE 
InS_EnD




 
