InS_StArT
OC212X.COM
1.0
^Olicom OC212X Ethernet adapter,OC212X.COM,IE0
?The adapter configuration program is used to set the I/O address, interrupt level and connector type: 10BaseT, BNC(Thin coax) or AUI(Thick coax). These settings will be read from the adapter and cannot be specified in the NET.CFG file.
!OIEM(PORT)I/O port
?If more than one OC212X adapter is installed in the workstation, use this parameter to identify the adapter. If no value is entered, the driver will search for an adapter and use the one at the lowest I/O port address.
300
320
340
360
240
280
2C0
!OIE0(MEM)Optional shared RAM address
?If not specified, shared RAM will not be used. If specified, the driver will use 16K shared RAM mapped at the specified location. Applications sending (writing) data may run faster with this option. The 16K area is then not available to memory managers such as EMM386 and should be properly 'excluded'. If more than one OC212X adapter is installed, they may all use the same address.
D0000
D4000
D8000
DC000
C8000
CC000
C0000
C4000
E0000
E4000
E8000
EC000
$OIE0(NODE ADDRESS)Node address
0
FFFFFFFFFFFF
*OIE0(FRAME)Media frame type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
