InS_StArT
ODIPKT.COM
1.0
^ShineNet LCS-8834P Pocket Ethernet card,ODIPKT.COM,IE0
?The Pocket lan card is auto-detected.
$OIE0(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
