InS_StArT
PCNTNW.COM
1.0
^AMD PCNet Family (EtherTeam PCI/ISA) Adapter,PCNTNW.COM,IE0
?The "PCNTNW.COM" driver supports AMD PCNet family chips.
!OIE0(BUSTYPE)PCNet Device
?If you know the device type, you can specify here.
PCI
PCI1
PCI2
VESA
PNP
ISA
!OIE0(PORT)Base I/O Port
?You can specify the I/O port address, or let the driver scan for you.
200
220
240
260
280
2A0
2C0
2E0
300
320
340
360
380
3A0
3C0
3E0
!OIE0(INT)Hardware Interrupt
?If you use PCNetISA, you must select a interrupt number.
3
4
5
9
10
11
15
!OIE0(DMA)DMA Channel
?If you use PCNetISA, you must select a DMA channel.
3
5
6
7
$OIE0(LED0 Value)Optional LED0 value
0
FFFF
$OIE0(LED1 Value)Optional LED1 value
0
FFFF
$OIE0(LED2 Value)Optional LED2 value
0
FFFF
$OIE0(LED3 Value)Optional LED3 value
0
FFFF
!OIE0()Optional Keyword
TP
FASTISA
DMAROTATE
$OIE0(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
