InS_StArT
MADGEODI.COM
1.0,MDGDOS26.BIN
^Madge Smart 16 Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 PC Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 PCMCIA Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 AT Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 AT Plus Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 ISA Client Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 ISA Client Plus Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 ISA Client PnP Ringnode,MADGEODI.COM,IE0
^Madge Smart 16/4 MC Ringnode,MADGEODI.COM,00M
^Madge Smart 16/4 MC32 Ringnode,MADGEODI.COM,00M
^Madge Smart 16/4 EISA Ringnode,MADGEODI.COM,0E0
^Madge Smart 16/4 PCI Ringnode,MADGEODI.COM,IE0
?This board may be used with source routing. If your network is using Source Routing please load the ROUTE.COM file after the MADGEODI.COM file.
!OIE0(PORT) Base I/O Port
0920
0940
0960
0A20
0A40
0A60
0B20
0B40
0B60
0E20
1A20
2A20
3A20
4A20
1E20
2E20
3E20
4E20
1000
2000
3000
4000
5000
6000
7000
!O00M(SLOT) Slot location
1
2
3
4
5
6
7
8
!OIEM(FRAME) Frame Type
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
$OIEM(NODE ADDRESS) Node Address
400000000000
7FFFFFFFFFFF
!OIEM(MAX FRAME SIZE) Maximum frame size
?Select the maximum packet size for your network. The packet sizes include protocol headers and represent 1/2k, 1k, 2k and 4k frames, respectively. Default is 4K.
626
1138
2162
4210
8200
InS_EnD
