InS_StArT
smart.exe
1.0,odi.smt
^Madge Smart 16 Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 PC Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 PCMCIA Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 AT Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 AT Plus Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 ISA Client Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 ISA Client Plus Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 ISA Client PnP Ringnode (Smart.exe),smart.exe,IE0
^Madge Smart 16/4 MC Ringnode (Smart.exe),smart.exe,00M
^Madge Smart 16/4 MC32 Ringnode (Smart.exe),smart.exe,00M
^Madge Smart 16/4 EISA Ringnode (Smart.exe),smart.exe,0E0
^Madge Smart 16/4 PCI Ringnode (Smart.exe),smart.exe,IE0
?For more details on this driver, including multiprotocol support, consult the SMART.INF file on your Madge Install disk.
!OIE0(PORT) Base I/O Port
0920
0940
0960
0A20
0A40
0A60
0B20
0B40
0B60
0E20
1A20
2A20
3A20
4A20
1E20
2E20
3E20
4E20
1000
2000
3000
4000
5000
6000
7000
!O00M(SLOT) Slot location
1
2
3
4
5
6
7
8
!OIEM(FRAME) Frame Type
TOKEN-RING 
TOKEN-RING_SNAP
$OIEM(NODE ADDRESS) Node Address
400000000000
7FFFFFFFFFFF
!OIEM(MAX FRAME SIZE) Maximum frame size
?Select the maximum packet size for your network. The packet sizes include protocol headers and represent 1/2K, 1K, 2K and 4K frames, respectively.  Default: 4K.
626
1138
2162
4210
InS_EnD
