InS_StArT
TOKEN.COM
1.1
^IBM Token-Ring Network Adapter II & 16/4 Adapter,TOKEN.COM,IE0000
^IBM Token-Ring Network Adapter/A,TOKEN.COM,00M,E000000
^IBM Token-Ring Network 16/4 Adapter/A,TOKEN.COM,00M000,E001
^IBM Token-Ring 16/4 ISA-16 Adapter,TOKEN.COM,IE0000
^IBM Token-Ring 16/4 MC Adapter,TOKEN.COM,00M000,E001
^IBM Auto 16/4 Token-Ring ISA Adapter,TOKEN.COM,IE0000
^IBM Auto 16/4 Token-Ring MC Adapter,TOKEN.COM,00M000,E001
!OIE0000(PORT)
?This keyword is only required when using more than one adapter of this type.
A20
A24
!R00M000(SLOT)
1
2
3
4
5
6
7
8
$OIEM000(NODE ADDRESS)
0
FFFFFFFFFFFF
$OIEM000(NIC UAA)NIC UAA Keyword
?If there is more than one adapter of this type installed in the system, this keyword may be used to specify which adapter is to be associated with this driver.
0
FFFFFFFFFFFF
$OIEM000(MAX FRAME SIZE)Maximum Frame Size
?The maximum frame size must be a multiple of 8.
632
17960
@4208
*RIEM000(FRAME)
@TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
InS_EnD
