InS_StArT
ND5200.COM
1.0
^NDC ND5200,ND5200.COM,IE0
?This setting may not work properly since PCI is not supported yet.
!OIE0()SIA
?I would suggest AUTODETECT if all possible.
BNC
TP
TP_FULL_DUPLEX
@AUTODETECT
TP_No_Link_Test
!OIE0()Turbo Mode
?Disable PCI post write buffer in Intel PCI chip, which gives PCI higher priority.
TURBO
*RIE0(FRAME)MediaFrame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs
may be using Ethernet_802.2.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
