InS_StArT
ne100tx.COM
1.0
^NDC 10/100 Auto PCI Fast Ethernet Adapter,ne100tx.COM,0E0
?This driver supports PCI machines
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*O0E0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!O0E0()Media Access Type
?NOTE: Media access type will be autodetected on driver's load
@AUTOSENSE 
InS_EnD




 
