InS_StArT
TR2KODI.COM
1.0
^TI-2000 16/4 Token-Ring,TR2KODI.COM,IE0
$OIE0 (PORT) Base I/O Port
?NOTE: Select the Base I/O Port address that corresponds to the port address setting on the adapter.
100
8000
@A20
!OIE0 (INT) Interrupt Level
?NOTE: Select the Interrupt Level that corresponds to the interrupt setting on the adapter.
2
3
4
5
6
7
@9
10
11
12
14
15
!OIE0 (DMA) DMA Channel
?NOTE: Select the DMA Channel that corresponds to the DMA setting on the adapter. Please consult your adapter's documentation to see if the adapter supports DMA Bus Mastering. Omit value if 8 or 16 bit Pseudo DMA is desired.
0
1
2
3
5
6
7
8
9
10
11
12
13
14
$OIE0 (NODE ADDRESS) Node Address
?NOTE:
0
FFFFFFFFFFFF
*OIE0 (FRAME) Frame Type
?NOTE: Select the frame type required by your network. The driver defaults to TOKEN-RING MSB frame type. You may select either or both frame types for MSB or LSB. Do not select a combination of MSB and LSB frames types. Client and Server must be configured to use the same frame type.
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
$OIE0 (MAX FRAME SIZE) Maximum Frame Size
?NOTE: Set the MAX FRAME SIZE to the largest frame size expected on the network. The driver host memory requirements will change respectively.
632
17960
@4208
!OIE0 (SPEED) Ring Speed
?NOTE: The Ring Speed for the adapter must match the speed of the network.
4
@16
!OIE0 () 16-Bit Pseudo DMA
?NOTE: This keyword selects 16-bit pseudo DMA mode. Please note that not all adapters support this mode. Consult the adapter documentation. Do not use the 0 WS 8-Bit Pseudo DMA keyword with this option; unpredictable results may occur.
BIT16
!OIE0 () 0 Wait State 8-Bit Pseudo DMA
?NOTE: This parameter is only valid when the adapter is operating in the 8-bit pseudo DMA mode. Please note that not all adapters support this parameter. This parameter increases performance on slower host computers.
WS0
!OIE0 () No Configuration Register
?NOTE: Select this option only if you want to disable the configuration register on the adapter or if your adapter does not have one.
NOCONFIG
InS_EnD