InS_StArT
TRODI.COM
1.0
^Xircom Token Ring Adapter,TRODI.COM,IEM
?Note: It is not necessary to select a parallel port configuration (INT or PORT).
!OIEM(INT) Parallel Port Interrupt
?It is not necessary to select a value, the driver will attempt to automatically configure if no value is given.
0
5
7
!OIEM(PORT) Parallel Port Address
?It is not necessary to select a value, the driver will attempt to automatically configure if no value is given.
278
378
3BC
$OIEM(NODE ADDRESS) Node Address
?When this parameter is not specified, the node address in the hardware is used.
0
FFFFFFFFFFFF
!OIEM(FRAME) Frame Type
@TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
$OIEM(MAX FRAME SIZE) Maximum frame size
626
4210
InS_EnD
