InS_StArT
E31ODI.COM
1.0
^Cabletron Systems Ethernet E31,E31ODI.COM,00M,5608
^Cabletron Systems Ethernet E31-X,E31ODI.COM,00M,5609
?Select the options you will use.
!O00M(SLOT) Slot Number
?Note: If you don't select a slot number, the first E31 board found will be used.
1
2
3
4
5
6
7
8
$O00M(NODE ADDRESS) Node Address
0
FFFFFFFFFFFF
*R00M(FRAME) Frame Type
?Note: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
