InS_StArT
EXP16ODI.COM
1.0
^Intel EtherExpress ISA Family,EXP16ODI.COM,IE0
^Intel EtherExpress MCA Family,EXP16ODI.COM,00M
?This is the DOS ODI driver for the Intel EtherExpress adapter. It can be used with the EtherExpress 16 in ISA and EISA systems, or with the EtherExpress MCA in microchannel systems.
!RIE0(PORT) I/O Address
?EtherExpress adapters support the following I/O addresses: 200, 210, 220, 230, 240, 250, 260, 270, 300, 310, 320, 330, 340, 350, 360, 370.  To change the I/O address setting, run SOFTSET.
200
210
220
230
240
250
260
270
@300
310
320
330
340
350
360
370
!R00M(SLOT)
?Specify the slot number that the EtherExpress MCA adapter is installed in.
1
2
3
4
5
6
7
8
*RIEM(FRAME)
?Note: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$OIEM(NODE ADDRESS)
?Warning: Entering an incorrect value for the node address can cause serious network problems. If you are uncertain, leave the node address blank.
0
FFFFFFFFFFFF
InS_EnD
