InS_StArT
HPMCAODI.COM
1.0
^Hewlett-Packard MC Adapter 16,HPMCAODI.COM,00M,63CA
!O00M (PORT) Base I/O Port
@400
1400
2400
3400
4400
5400
6400
7400
!O00M (INT) Hardware Interrupt
@3
4
5
7
9
10
11
12
!O00M (SLOT) Expansion Slot
1
2
3
4
5
6
7
8
$O00M (NODE ADDRESS) Node Address
0
7FFFFFFFFFFF
*O00M (FRAME) Frame Type
?Note: Ethernet_802.3 is the default frame type for many NetWare servers.  Newer servers default to Ethernet_802.2 frame type. Check with your administrator for the correct frame type for your network.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
