InS_StArT
NCRWL05.COM
1.0
^NCR WaveLAN,NCRWL05.COM,IEM,6A14
?You can use this driver in an ISA (AT bus), EISA, or microchannel client. In case of ISA, the card must be in a 16-bits slot. You can have a maximum of four WaveLAN network boards in your machine.
!RIE0(PORT)Base I/O Port
?You must select the option that matches your board's I/O jumper setting. The 3C0 setting may conflict with EGA video cards. The 3E0 setting may conflict with COM3.
@300
390
3C0
3E0
$O00M(SLOT) Slot location
?If 0 is selected, the driver scans for the WaveLAN network boards. It starts at slot 1 and uses the first WaveLAN board found.
0
8
@0
*RIEM(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
