InS_StArT
NI6510.COM
1.0
^Racal-Datacom NI6510 ODI MLID,NI6510.COM,IE0
!OIE0(PORT)
?The driver is self-configuring. If multiple NI6510 cards are in the system, specifiy I/O Base Address.
300
320
340
360
$OIE0(NODE ADDRESS)
0
7FFFFFFFFFFF
*OIE0(FRAME)
?Note: Ethernet_802.2 is the default frame type for ODI drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_SNAP
Ethernet_II
InS_EnD
