InS_StArT
PCMDM.COM
1.0
^NSC Ethernet PCMCIA Card,PCMDM.COM,IE0
?If you wish to override a Card Services INT selection, please select an INT assignment from this list and remove the semicolon from the NET.CFG file.
!OIE0( ;INT)
3
4
5
7
9
10
11
15
!OIE0( ;PORT)
?If you wish to override a Card Services PORT selection, please select a PORT assignment from this list and remove the semicolon from the NET.CFG file.
300
320
340
360
380
240
280
2C0
!OIE0(MEM)
?If you wish to override a Card Services MEM selection, please select a MEM assignment from this list.
@FFFFFFFF
D0000
D4000
D8000
DC000
C0000
C4000
C8000
CC000
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!RIE0(PCMCIA)
@
InS_EnD
