;-----------------------------------------------------------------------
;STPCB V3.01B CONFIGURATION FILE, ANYTHING AFTER ; IS A COMMENT

;This is a SAMPLE config file.  After you have made any changes for
;your desired setup, you MUST copy or rename this file to STPCB.CFG

;For fastest operation, remove all comment lines.
;-----------------------------------------------------------------------

MESSAGE_SECURITY=0

;Minimum security level to allow user to capture the report in a message.
;Users with security LESS THAN THIS NUMBER will not be allowed to capture
;the reports to a message.  Valid range is 0 - 255, corresponding to the
;security levels defined in PCBoard.  A value of 256 will prevent ANYONE,
;even the Sysop, from capturing to a message.  Default is 0.

;-----------------------------------------------------------------------

MESSAGE_CONF=65536

;If set to 65536, then all captured report messages will be left in the
;conference the user was in when the report was generated.  If set to a
;number from 0 - 65535, the message will be forced into that conference,
;regardless of what conference the user was in at the time the report
;was generated.  (Conference  0 is the 'Main Board' area.)
;Default is 65536.

;-----------------------------------------------------------------------

MESSAGE_ADDRESS=USERNAME

;If set to USERNAME, then all captured report messages will be addressed
;to the actual name of the user that generated the report.  If set to
;anything other than USERNAME, the message will be addressed to that
;name, like SYSOP or TECH SUPPORT.  Default is USERNAME.

;-----------------------------------------------------------------------

FORCE_MESSAGES_PRIVATE=N

;If set to Y, then all captured report messages will be marked as
;'Receiver-only' in the PCBoard message base.  This will prevent cluttering
;up the message bases on very active systems.   If set to N, all messages
;will be marked as 'Public' in the message base, so that anyone can view
;them, although the user does still have the option of making the message
;private at run-time.  Default is N.

;-----------------------------------------------------------------------

MESSAGE_LIFE=0

;The message pack-out date is set for the number of days indicated.
;Range is 1-32767 days.  A value of 0 indicates no automatic packout
;date will be applied.   Default is 0 days.

;-----------------------------------------------------------------------

COPY_ALL_REPORTS=N

;If set to Y, then ALL reports will be captured to a message in the
;'COPY_MESSAGE_CONF',  WHETHER THE USER REQUESTED A MESSAGE OR NOT!
;Default is N.

;-----------------------------------------------------------------------

COPY_MESSAGE_CONF=65536

;If set to a number from 0 - 65535, then all captured report messages
;will be copied into the indicated conference number.   If set to 65536,
;then no copying of report messages will occur.  Default is 65536.

;-----------------------------------------------------------------------

EXEMPT_CONF=0

;List of conferences to be exempted from the action of the MESSAGE_CONF,
;FORCE_MESSAGES_PRIVATE, and MESSAGE_ADDRESS options.  For example, if
;you had MESSAGE_CONF=0 to force all messages to the main board area,
;but you wanted messages generated in conferences 17 and 18 to remain
;in place, you could enter a line like this:   EXEMPT_CONF=17 18
;Valid numbers are 1-65535 corresponding to the PCBoard conference
;numbers, 0 means 'none'.  Default is 0.

;-----------------------------------------------------------------------

NODE_LOCKOUT=256

;This is a list of node numbers that you do NOT want the program to run on.
;For example, if you wanted to prevent the program from being used on nodes
;3, 8, and 10, you would enter NODE_LOCKOUT=3 8 10
;Setting this option to 256 will allow operation on all nodes, and that is
;the Default value.

;-----------------------------------------------------------------------

RETRAIN_SECURITY=0

;Minimum security level to allow user to force a modem re-train. Users
;with security LESS THAN THIS NUMBER will not be allowed to force a
;a retrain.  Valid range is 0 - 255, corresponding to the security levels
;defined in PCBoard.  A value of 256 will prevent ANYONE, even the
;Sysop, from using the retrain option.  Default is 0.

;-----------------------------------------------------------------------

INCLUDE_SETTINGS=N

;If set to Y, then the report will include the current modem settings.
;If set to N, the settings will not be shown.  Default is N.

;-----------------------------------------------------------------------

MODEM_DELAY=4

;This is the number of clock ticks to pause between issuing modem commands
;inside the program.   There are 18.2 ticks per second.   Valid range is
;1 - 36, default is 4.  Lowering this value may speed operation of the
;program, but may result in glitches or missing information.  If you are
;running a slower system, or have trouble with information missing from
;the display, you may try increasing this value to a maximum of 36.

;-----------------------------------------------------------------------

ESCAPE_CHAR=128

;This is the value of the character used to put the modem into on-line
;command mode, corresponding to the setting of the modem's S2 register.
;If set to 128, then the escape character will not be used, and the
;program will assume that the modem is set to &D1 to allow DTR toggling
;to get into command mode.  Valid values are 0-127 for escape character
;mode, and 128 for DTR toggle mode.   Default is 128.

;-----------------------------------------------------------------------

DELETE_TEMPFILES=Y

;If set to N, the temporary files created during execution will be
;retained for debugging purposes.  If set to Y, the temporary files
;will be deleted when the user exits the program.  Default is Y.

;-----------------------------------------------------------------------
;END OF CONFIG FILE
;-----------------------------------------------------------------------
