This is gdbint.info, produced by makeinfo version 4.2 from
gdbint.texinfo.

INFO-DIR-SECTION Programming & development tools.
START-INFO-DIR-ENTRY
* Gdb-Internals: (gdbint).	The GNU debugger's internals.
END-INFO-DIR-ENTRY

   This file documents the internals of the GNU debugger GDB.
Copyright 1990,1991,1992,1993,1994,1996,1998,1999,2000,2001,2002
Free Software Foundation, Inc.  Contributed by Cygnus Solutions.
Written by John Gilmore.  Second Edition by Stan Shebs.

   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.1 or
any later version published by the Free Software Foundation; with no
Invariant Sections, with the Front-Cover Texts being "A GNU Manual,"
and with the Back-Cover Texts as in (a) below.

   (a) The FSF's Back-Cover Text is: "You have freedom to copy and
modify this GNU Manual, like GNU software.  Copies published by the Free
Software Foundation raise funds for GNU development."


File: gdbint.info,  Node: Top,  Next: Requirements,  Up: (dir)

Scope of this Document
**********************

   This document documents the internals of the GNU debugger, GDB.  It
includes description of GDB's key algorithms and operations, as well as
the mechanisms that adapt GDB to specific hosts and targets.

* Menu:

* Requirements::
* Overall Structure::
* Algorithms::
* User Interface::
* libgdb::
* Symbol Handling::
* Language Support::
* Host Definition::
* Target Architecture Definition::
* Target Vector Definition::
* Native Debugging::
* Support Libraries::
* Coding::
* Porting GDB::
* Releasing GDB::
* Testsuite::
* Hints::

* GNU Free Documentation License::  The license for this documentation
* Index::


File: gdbint.info,  Node: Requirements,  Next: Overall Structure,  Prev: Top,  Up: Top

Requirements
************

   Before diving into the internals, you should understand the formal
requirements and other expectations for GDB.  Although some of these
may seem obvious, there have been proposals for GDB that have run
counter to these requirements.

   First of all, GDB is a debugger.  It's not designed to be a front
panel for embedded systems.  It's not a text editor.  It's not a shell.
It's not a programming environment.

   GDB is an interactive tool.  Although a batch mode is available,
GDB's primary role is to interact with a human programmer.

   GDB should be responsive to the user.  A programmer hot on the trail
of a nasty bug, and operating under a looming deadline, is going to be
very impatient of everything, including the response time to debugger
commands.

   GDB should be relatively permissive, such as for expressions.  While
the compiler should be picky (or have the option to be made picky),
since source code lives for a long time usually, the programmer doing
debugging shouldn't be spending time figuring out to mollify the
debugger.

   GDB will be called upon to deal with really large programs.
Executable sizes of 50 to 100 megabytes occur regularly, and we've
heard reports of programs approaching 1 gigabyte in size.

   GDB should be able to run everywhere.  No other debugger is
available for even half as many configurations as GDB supports.


File: gdbint.info,  Node: Overall Structure,  Next: Algorithms,  Prev: Requirements,  Up: Top

Overall Structure
*****************

   GDB consists of three major subsystems: user interface, symbol
handling (the "symbol side"), and target system handling (the "target
side").

   The user interface consists of several actual interfaces, plus
supporting code.

   The symbol side consists of object file readers, debugging info
interpreters, symbol table management, source language expression
parsing, type and value printing.

   The target side consists of execution control, stack frame analysis,
and physical target manipulation.

   The target side/symbol side division is not formal, and there are a
number of exceptions.  For instance, core file support involves symbolic
elements (the basic core file reader is in BFD) and target elements (it
supplies the contents of memory and the values of registers).  Instead,
this division is useful for understanding how the minor subsystems
should fit together.

The Symbol Side
===============

   The symbolic side of GDB can be thought of as "everything you can do
in GDB without having a live program running".  For instance, you can
look at the types of variables, and evaluate many kinds of expressions.

The Target Side
===============

   The target side of GDB is the "bits and bytes manipulator".
Although it may make reference to symbolic info here and there, most of
the target side will run with only a stripped executable available--or
even no executable at all, in remote debugging cases.

   Operations such as disassembly, stack frame crawls, and register
display, are able to work with no symbolic info at all.  In some cases,
such as disassembly, GDB will use symbolic info to present addresses
relative to symbols rather than as raw numbers, but it will work either
way.

Configurations
==============

   "Host" refers to attributes of the system where GDB runs.  "Target"
refers to the system where the program being debugged executes.  In
most cases they are the same machine, in which case a third type of
"Native" attributes come into play.

   Defines and include files needed to build on the host are host
support.  Examples are tty support, system defined types, host byte
order, host float format.

   Defines and information needed to handle the target format are target
dependent.  Examples are the stack frame format, instruction set,
breakpoint instruction, registers, and how to set up and tear down the
stack to call a function.

   Information that is only needed when the host and target are the
same, is native dependent.  One example is Unix child process support;
if the host and target are not the same, doing a fork to start the
target process is a bad idea.  The various macros needed for finding the
registers in the `upage', running `ptrace', and such are all in the
native-dependent files.

   Another example of native-dependent code is support for features that
are really part of the target environment, but which require `#include'
files that are only available on the host system.  Core file handling
and `setjmp' handling are two common cases.

   When you want to make GDB work "native" on a particular machine, you
have to include all three kinds of information.


File: gdbint.info,  Node: Algorithms,  Next: User Interface,  Prev: Overall Structure,  Up: Top

Algorithms
**********

   GDB uses a number of debugging-specific algorithms.  They are often
not very complicated, but get lost in the thicket of special cases and
real-world issues.  This chapter describes the basic algorithms and
mentions some of the specific target definitions that they use.

Frames
======

   A frame is a construct that GDB uses to keep track of calling and
called functions.

   `FRAME_FP' in the machine description has no meaning to the
machine-independent part of GDB, except that it is used when setting up
a new frame from scratch, as follows:

     create_new_frame (read_register (FP_REGNUM), read_pc ()));

   Other than that, all the meaning imparted to `FP_REGNUM' is imparted
by the machine-dependent code.  So, `FP_REGNUM' can have any value that
is convenient for the code that creates new frames.
(`create_new_frame' calls `INIT_EXTRA_FRAME_INFO' if it is defined;
that is where you should use the `FP_REGNUM' value, if your frames are
nonstandard.)

   Given a GDB frame, define `FRAME_CHAIN' to determine the address of
the calling function's frame.  This will be used to create a new GDB
frame struct, and then `INIT_EXTRA_FRAME_INFO' and `INIT_FRAME_PC' will
be called for the new frame.

Breakpoint Handling
===================

   In general, a breakpoint is a user-designated location in the program
where the user wants to regain control if program execution ever reaches
that location.

   There are two main ways to implement breakpoints; either as
"hardware" breakpoints or as "software" breakpoints.

   Hardware breakpoints are sometimes available as a builtin debugging
features with some chips.  Typically these work by having dedicated
register into which the breakpoint address may be stored.  If the PC
(shorthand for "program counter") ever matches a value in a breakpoint
registers, the CPU raises an exception and reports it to GDB.

   Another possibility is when an emulator is in use; many emulators
include circuitry that watches the address lines coming out from the
processor, and force it to stop if the address matches a breakpoint's
address.

   A third possibility is that the target already has the ability to do
breakpoints somehow; for instance, a ROM monitor may do its own
software breakpoints.  So although these are not literally "hardware
breakpoints", from GDB's point of view they work the same; GDB need not
do nothing more than set the breakpoint and wait for something to
happen.

   Since they depend on hardware resources, hardware breakpoints may be
limited in number; when the user asks for more, GDB will start trying
to set software breakpoints.  (On some architectures, notably the
32-bit x86 platforms, GDB cannot always know whether there's enough
hardware resources to insert all the hardware breakpoints and
watchpoints.  On those platforms, GDB prints an error message only when
the program being debugged is continued.)

   Software breakpoints require GDB to do somewhat more work.  The
basic theory is that GDB will replace a program instruction with a
trap, illegal divide, or some other instruction that will cause an
exception, and then when it's encountered, GDB will take the exception
and stop the program.  When the user says to continue, GDB will restore
the original instruction, single-step, re-insert the trap, and continue
on.

   Since it literally overwrites the program being tested, the program
area must be writable, so this technique won't work on programs in ROM.
It can also distort the behavior of programs that examine themselves,
although such a situation would be highly unusual.

   Also, the software breakpoint instruction should be the smallest
size of instruction, so it doesn't overwrite an instruction that might
be a jump target, and cause disaster when the program jumps into the
middle of the breakpoint instruction.  (Strictly speaking, the
breakpoint must be no larger than the smallest interval between
instructions that may be jump targets; perhaps there is an architecture
where only even-numbered instructions may jumped to.)  Note that it's
possible for an instruction set not to have any instructions usable for
a software breakpoint, although in practice only the ARC has failed to
define such an instruction.

   The basic definition of the software breakpoint is the macro
`BREAKPOINT'.

   Basic breakpoint object handling is in `breakpoint.c'.  However,
much of the interesting breakpoint action is in `infrun.c'.

Single Stepping
===============

Signal Handling
===============

Thread Handling
===============

Inferior Function Calls
=======================

Longjmp Support
===============

   GDB has support for figuring out that the target is doing a
`longjmp' and for stopping at the target of the jump, if we are
stepping.  This is done with a few specialized internal breakpoints,
which are visible in the output of the `maint info breakpoint' command.

   To make this work, you need to define a macro called
`GET_LONGJMP_TARGET', which will examine the `jmp_buf' structure and
extract the longjmp target address.  Since `jmp_buf' is target
specific, you will need to define it in the appropriate `tm-TARGET.h'
file.  Look in `tm-sun4os4.h' and `sparc-tdep.c' for examples of how to
do this.

Watchpoints
===========

   Watchpoints are a special kind of breakpoints (*note breakpoints:
Algorithms.) which break when data is accessed rather than when some
instruction is executed.  When you have data which changes without your
knowing what code does that, watchpoints are the silver bullet to hunt
down and kill such bugs.

   Watchpoints can be either hardware-assisted or not; the latter type
is known as "software watchpoints."  GDB always uses hardware-assisted
watchpoints if they are available, and falls back on software
watchpoints otherwise.  Typical situations where GDB will use software
watchpoints are:

   * The watched memory region is too large for the underlying hardware
     watchpoint support.  For example, each x86 debug register can
     watch up to 4 bytes of memory, so trying to watch data structures
     whose size is more than 16 bytes will cause GDB to use software
     watchpoints.

   * The value of the expression to be watched depends on data held in
     registers (as opposed to memory).

   * Too many different watchpoints requested.  (On some architectures,
     this situation is impossible to detect until the debugged program
     is resumed.)  Note that x86 debug registers are used both for
     hardware breakpoints and for watchpoints, so setting too many
     hardware breakpoints might cause watchpoint insertion to fail.

   * No hardware-assisted watchpoints provided by the target
     implementation.

   Software watchpoints are very slow, since GDB needs to single-step
the program being debugged and test the value of the watched
expression(s) after each instruction.  The rest of this section is
mostly irrelevant for software watchpoints.

   GDB uses several macros and primitives to support hardware
watchpoints:

`TARGET_HAS_HARDWARE_WATCHPOINTS'
     If defined, the target supports hardware watchpoints.

`TARGET_CAN_USE_HARDWARE_WATCHPOINT (TYPE, COUNT, OTHER)'
     Return the number of hardware watchpoints of type TYPE that are
     possible to be set.  The value is positive if COUNT watchpoints of
     this type can be set, zero if setting watchpoints of this type is
     not supported, and negative if COUNT is more than the maximum
     number of watchpoints of type TYPE that can be set.  OTHER is
     non-zero if other types of watchpoints are currently enabled (there
     are architectures which cannot set watchpoints of different types
     at the same time).

`TARGET_REGION_OK_FOR_HW_WATCHPOINT (ADDR, LEN)'
     Return non-zero if hardware watchpoints can be used to watch a
     region whose address is ADDR and whose length in bytes is LEN.

`TARGET_REGION_SIZE_OK_FOR_HW_WATCHPOINT (SIZE)'
     Return non-zero if hardware watchpoints can be used to watch a
     region whose size is SIZE.  GDB only uses this macro as a
     fall-back, in case `TARGET_REGION_OK_FOR_HW_WATCHPOINT' is not
     defined.

`TARGET_DISABLE_HW_WATCHPOINTS (PID)'
     Disables watchpoints in the process identified by PID.  This is
     used, e.g., on HP-UX which provides operations to disable and
     enable the page-level memory protection that implements hardware
     watchpoints on that platform.

`TARGET_ENABLE_HW_WATCHPOINTS (PID)'
     Enables watchpoints in the process identified by PID.  This is
     used, e.g., on HP-UX which provides operations to disable and
     enable the page-level memory protection that implements hardware
     watchpoints on that platform.

`target_insert_watchpoint (ADDR, LEN, TYPE)'
`target_remove_watchpoint (ADDR, LEN, TYPE)'
     Insert or remove a hardware watchpoint starting at ADDR, for LEN
     bytes.  TYPE is the watchpoint type, one of the possible values of
     the enumerated data type `target_hw_bp_type', defined by
     `breakpoint.h' as follows:

           enum target_hw_bp_type
             {
               hw_write   = 0, /* Common (write) HW watchpoint */
               hw_read    = 1, /* Read    HW watchpoint */
               hw_access  = 2, /* Access (read or write) HW watchpoint */
               hw_execute = 3  /* Execute HW breakpoint */
             };

     These two macros should return 0 for success, non-zero for failure.

`target_remove_hw_breakpoint (ADDR, SHADOW)'
`target_insert_hw_breakpoint (ADDR, SHADOW)'
     Insert or remove a hardware-assisted breakpoint at address ADDR.
     Returns zero for success, non-zero for failure.  SHADOW is the
     real contents of the byte where the breakpoint has been inserted;
     it is generally not valid when hardware breakpoints are used, but
     since no other code touches these values, the implementations of
     the above two macros can use them for their internal purposes.

`target_stopped_data_address ()'
     If the inferior has some watchpoint that triggered, return the
     address associated with that watchpoint.  Otherwise, return zero.

`DECR_PC_AFTER_HW_BREAK'
     If defined, GDB decrements the program counter by the value of
     `DECR_PC_AFTER_HW_BREAK' after a hardware break-point.  This
     overrides the value of `DECR_PC_AFTER_BREAK' when a breakpoint
     that breaks is a hardware-assisted breakpoint.

`HAVE_STEPPABLE_WATCHPOINT'
     If defined to a non-zero value, it is not necessary to disable a
     watchpoint to step over it.

`HAVE_NONSTEPPABLE_WATCHPOINT'
     If defined to a non-zero value, GDB should disable a watchpoint to
     step the inferior over it.

`HAVE_CONTINUABLE_WATCHPOINT'
     If defined to a non-zero value, it is possible to continue the
     inferior after a watchpoint has been hit.

`CANNOT_STEP_HW_WATCHPOINTS'
     If this is defined to a non-zero value, GDB will remove all
     watchpoints before stepping the inferior.

`STOPPED_BY_WATCHPOINT (WAIT_STATUS)'
     Return non-zero if stopped by a watchpoint.  WAIT_STATUS is of the
     type `struct target_waitstatus', defined by `target.h'.

x86 Watchpoints
---------------

   The 32-bit Intel x86 (a.k.a. ia32) processors feature special debug
registers designed to facilitate debugging.  GDB provides a generic
library of functions that x86-based ports can use to implement support
for watchpoints and hardware-assisted breakpoints.  This subsection
documents the x86 watchpoint facilities in GDB.

   To use the generic x86 watchpoint support, a port should do the
following:

   * Define the macro `I386_USE_GENERIC_WATCHPOINTS' somewhere in the
     target-dependent headers.

   * Include the `config/i386/nm-i386.h' header file _after_ defining
     `I386_USE_GENERIC_WATCHPOINTS'.

   * Add `i386-nat.o' to the value of the Make variable `NATDEPFILES'
     (*note NATDEPFILES: Native Debugging.) or `TDEPFILES' (*note
     TDEPFILES: Target Architecture Definition.).

   * Provide implementations for the `I386_DR_LOW_*' macros described
     below.  Typically, each macro should call a target-specific
     function which does the real work.

   The x86 watchpoint support works by maintaining mirror images of the
debug registers.  Values are copied between the mirror images and the
real debug registers via a set of macros which each target needs to
provide:

`I386_DR_LOW_SET_CONTROL (VAL)'
     Set the Debug Control (DR7) register to the value VAL.

`I386_DR_LOW_SET_ADDR (IDX, ADDR)'
     Put the address ADDR into the debug register number IDX.

`I386_DR_LOW_RESET_ADDR (IDX)'
     Reset (i.e. zero out) the address stored in the debug register
     number IDX.

`I386_DR_LOW_GET_STATUS'
     Return the value of the Debug Status (DR6) register.  This value is
     used immediately after it is returned by `I386_DR_LOW_GET_STATUS',
     so as to support per-thread status register values.

   For each one of the 4 debug registers (whose indices are from 0 to 3)
that store addresses, a reference count is maintained by GDB, to allow
sharing of debug registers by several watchpoints.  This allows users
to define several watchpoints that watch the same expression, but with
different conditions and/or commands, without wasting debug registers
which are in short supply.  GDB maintains the reference counts
internally, targets don't have to do anything to use this feature.

   The x86 debug registers can each watch a region that is 1, 2, or 4
bytes long.  The ia32 architecture requires that each watched region be
appropriately aligned: 2-byte region on 2-byte boundary, 4-byte region
on 4-byte boundary.  However, the x86 watchpoint support in GDB can
watch unaligned regions and regions larger than 4 bytes (up to 16
bytes) by allocating several debug registers to watch a single region.
This allocation of several registers per a watched region is also done
automatically without target code intervention.

   The generic x86 watchpoint support provides the following API for the
GDB's application code:

`i386_region_ok_for_watchpoint (ADDR, LEN)'
     The macro `TARGET_REGION_OK_FOR_HW_WATCHPOINT' is set to call this
     function.  It counts the number of debug registers required to
     watch a given region, and returns a non-zero value if that number
     is less than 4, the number of debug registers available to x86
     processors.

`i386_stopped_data_address (void)'
     The macros `STOPPED_BY_WATCHPOINT' and
     `target_stopped_data_address' are set to call this function.  The
     argument passed to `STOPPED_BY_WATCHPOINT' is ignored.  This
     function examines the breakpoint condition bits in the DR6 Debug
     Status register, as returned by the `I386_DR_LOW_GET_STATUS'
     macro, and returns the address associated with the first bit that
     is set in DR6.

`i386_insert_watchpoint (ADDR, LEN, TYPE)'
`i386_remove_watchpoint (ADDR, LEN, TYPE)'
     Insert or remove a watchpoint.  The macros
     `target_insert_watchpoint' and `target_remove_watchpoint' are set
     to call these functions.  `i386_insert_watchpoint' first looks for
     a debug register which is already set to watch the same region for
     the same access types; if found, it just increments the reference
     count of that debug register, thus implementing debug register
     sharing between watchpoints.  If no such register is found, the
     function looks for a vacant debug register, sets its mirrored
     value to ADDR, sets the mirrored value of DR7 Debug Control
     register as appropriate for the LEN and TYPE parameters, and then
     passes the new values of the debug register and DR7 to the
     inferior by calling `I386_DR_LOW_SET_ADDR' and
     `I386_DR_LOW_SET_CONTROL'.  If more than one debug register is
     required to cover the given region, the above process is repeated
     for each debug register.

     `i386_remove_watchpoint' does the opposite: it resets the address
     in the mirrored value of the debug register and its read/write and
     length bits in the mirrored value of DR7, then passes these new
     values to the inferior via `I386_DR_LOW_RESET_ADDR' and
     `I386_DR_LOW_SET_CONTROL'.  If a register is shared by several
     watchpoints, each time a `i386_remove_watchpoint' is called, it
     decrements the reference count, and only calls
     `I386_DR_LOW_RESET_ADDR' and `I386_DR_LOW_SET_CONTROL' when the
     count goes to zero.

`i386_insert_hw_breakpoint (ADDR, SHADOW'
`i386_remove_hw_breakpoint (ADDR, SHADOW)'
     These functions insert and remove hardware-assisted breakpoints.
     The macros `target_insert_hw_breakpoint' and
     `target_remove_hw_breakpoint' are set to call these functions.
     These functions work like `i386_insert_watchpoint' and
     `i386_remove_watchpoint', respectively, except that they set up
     the debug registers to watch instruction execution, and each
     hardware-assisted breakpoint always requires exactly one debug
     register.

`i386_stopped_by_hwbp (void)'
     This function returns non-zero if the inferior has some watchpoint
     or hardware breakpoint that triggered.  It works like
     `i386_stopped_data_address', except that it doesn't return the
     address whose watchpoint triggered.

`i386_cleanup_dregs (void)'
     This function clears all the reference counts, addresses, and
     control bits in the mirror images of the debug registers.  It
     doesn't affect the actual debug registers in the inferior process.

*Notes:*
  1. x86 processors support setting watchpoints on I/O reads or writes.
     However, since no target supports this (as of March 2001), and
     since `enum target_hw_bp_type' doesn't even have an enumeration
     for I/O watchpoints, this feature is not yet available to GDB
     running on x86.

  2. x86 processors can enable watchpoints locally, for the current task
     only, or globally, for all the tasks.  For each debug register,
     there's a bit in the DR7 Debug Control register that determines
     whether the associated address is watched locally or globally.  The
     current implementation of x86 watchpoint support in GDB always
     sets watchpoints to be locally enabled, since global watchpoints
     might interfere with the underlying OS and are probably
     unavailable in many platforms.


File: gdbint.info,  Node: User Interface,  Next: libgdb,  Prev: Algorithms,  Up: Top

User Interface
**************

   GDB has several user interfaces.  Although the command-line interface
is the most common and most familiar, there are others.

Command Interpreter
===================

   The command interpreter in GDB is fairly simple.  It is designed to
allow for the set of commands to be augmented dynamically, and also has
a recursive subcommand capability, where the first argument to a
command may itself direct a lookup on a different command list.

   For instance, the `set' command just starts a lookup on the
`setlist' command list, while `set thread' recurses to the
`set_thread_cmd_list'.

   To add commands in general, use `add_cmd'.  `add_com' adds to the
main command list, and should be used for those commands.  The usual
place to add commands is in the `_initialize_XYZ' routines at the ends
of most source files.

   To add paired `set' and `show' commands, use `add_setshow_cmd' or
`add_setshow_cmd_full'.  The former is a slightly simpler interface
which is useful when you don't need to further modify the new command
structures, while the latter returns the new command structures for
manipulation.

   Before removing commands from the command set it is a good idea to
deprecate them for some time.  Use `deprecate_cmd' on commands or
aliases to set the deprecated flag.  `deprecate_cmd' takes a `struct
cmd_list_element' as it's first argument.  You can use the return value
from `add_com' or `add_cmd' to deprecate the command immediately after
it is created.

   The first time a command is used the user will be warned and offered
a replacement (if one exists). Note that the replacement string passed
to `deprecate_cmd' should be the full name of the command, i.e. the
entire string the user should type at the command line.

UI-Independent Output--the `ui_out' Functions
=============================================

   The `ui_out' functions present an abstraction level for the GDB
output code.  They hide the specifics of different user interfaces
supported by GDB, and thus free the programmer from the need to write
several versions of the same code, one each for every UI, to produce
output.

Overview and Terminology
------------------------

   In general, execution of each GDB command produces some sort of
output, and can even generate an input request.

   Output can be generated for the following purposes:

   * to display a _result_ of an operation;

   * to convey _info_ or produce side-effects of a requested operation;

   * to provide a _notification_ of an asynchronous event (including
     progress indication of a prolonged asynchronous operation);

   * to display _error messages_ (including warnings);

   * to show _debug data_;

   * to _query_ or prompt a user for input (a special case).

This section mainly concentrates on how to build result output,
although some of it also applies to other kinds of output.

   Generation of output that displays the results of an operation
involves one or more of the following:

   * output of the actual data

   * formatting the output as appropriate for console output, to make it
     easily readable by humans

   * machine oriented formatting-a more terse formatting to allow for
     easy parsing by programs which read GDB's output

   * annotation, whose purpose is to help legacy GUIs to identify
     interesting parts in the output

   The `ui_out' routines take care of the first three aspects.
Annotations are provided by separate annotation routines.  Note that use
of annotations for an interface between a GUI and GDB is deprecated.

   Output can be in the form of a single item, which we call a "field";
a "list" consisting of identical fields; a "tuple" consisting of
non-identical fields; or a "table", which is a tuple consisting of a
header and a body.  In a BNF-like form:

`<table> ==>'
     `<header> <body>'

`<header> ==>'
     `{ <column> }'

`<column> ==>'
     `<width> <alignment> <title>'

`<body> ==>'
     `{<row>}'

General Conventions
-------------------

   Most `ui_out' routines are of type `void', the exceptions are
`ui_out_stream_new' (which returns a pointer to the newly created
object) and the `make_cleanup' routines.

   The first parameter is always the `ui_out' vector object, a pointer
to a `struct ui_out'.

   The FORMAT parameter is like in `printf' family of functions.  When
it is present, there must also be a variable list of arguments
sufficient used to satisfy the `%' specifiers in the supplied format.

   When a character string argument is not used in a `ui_out' function
call, a `NULL' pointer has to be supplied instead.

Table, Tuple and List Functions
-------------------------------

   This section introduces `ui_out' routines for building lists, tuples
and tables.  The routines to output the actual data items (fields) are
presented in the next section.

   To recap: A "tuple" is a sequence of "fields", each field containing
information about an object; a "list" is a sequence of fields where
each field describes an identical object.

   Use the "table" functions when your output consists of a list of
rows (tuples) and the console output should include a heading.  Use this
even when you are listing just one object but you still want the header.

   Tables can not be nested.  Tuples and lists can be nested up to a
maximum of five levels.

   The overall structure of the table output code is something like
this:

       ui_out_table_begin
         ui_out_table_header
         ...
         ui_out_table_body
           ui_out_tuple_begin
             ui_out_field_*
             ...
           ui_out_tuple_end
           ...
       ui_out_table_end

   Here is the description of table-, tuple- and list-related `ui_out'
functions:

 - Function: void ui_out_table_begin (struct ui_out *UIOUT, int
          NBROFCOLS, int NR_ROWS, const char *TBLID)
     The function `ui_out_table_begin' marks the beginning of the output
     of a table.  It should always be called before any other `ui_out'
     function for a given table.  NBROFCOLS is the number of columns in
     the table. NR_ROWS is the number of rows in the table.  TBLID is
     an optional string identifying the table.  The string pointed to
     by TBLID is copied by the implementation of `ui_out_table_begin',
     so the application can free the string if it was `malloc'ed.

     The companion function `ui_out_table_end', described below, marks
     the end of the table's output.

 - Function: void ui_out_table_header (struct ui_out *UIOUT, int WIDTH,
          enum ui_align ALIGNMENT, const char *COLHDR)
     `ui_out_table_header' provides the header information for a single
     table column.  You call this function several times, one each for
     every column of the table, after `ui_out_table_begin', but before
     `ui_out_table_body'.

     The value of WIDTH gives the column width in characters.  The
     value of ALIGNMENT is one of `left', `center', and `right', and it
     specifies how to align the header: left-justify, center, or
     right-justify it.  COLHDR points to a string that specifies the
     column header; the implementation copies that string, so column
     header strings in `malloc'ed storage can be freed after the call.

 - Function: void ui_out_table_body (struct ui_out *UIOUT)
     This function delimits the table header from the table body.

 - Function: void ui_out_table_end (struct ui_out *UIOUT)
     This function signals the end of a table's output.  It should be
     called after the table body has been produced by the list and
     field output functions.

     There should be exactly one call to `ui_out_table_end' for each
     call to `ui_out_table_begin', otherwise the `ui_out' functions
     will signal an internal error.

   The output of the tuples that represent the table rows must follow
the call to `ui_out_table_body' and precede the call to
`ui_out_table_end'.  You build a tuple by calling `ui_out_tuple_begin'
and `ui_out_tuple_end', with suitable calls to functions which actually
output fields between them.

 - Function: void ui_out_tuple_begin (struct ui_out *UIOUT, const char
          *ID)
     This function marks the beginning of a tuple output.  ID points to
     an optional string that identifies the tuple; it is copied by the
     implementation, and so strings in `malloc'ed storage can be freed
     after the call.

 - Function: void ui_out_tuple_end (struct ui_out *UIOUT)
     This function signals an end of a tuple output.  There should be
     exactly one call to `ui_out_tuple_end' for each call to
     `ui_out_tuple_begin', otherwise an internal GDB error will be
     signaled.

 - Function: struct cleanup *make_cleanup_ui_out_tuple_begin_end
          (struct ui_out *UIOUT, const char *ID)
     This function first opens the tuple and then establishes a cleanup
     (*note Cleanups: Coding.) to close the tuple.  It provides a
     convenient and correct implementation of the non-portable(1) code
     sequence:
          struct cleanup *old_cleanup;
          ui_out_tuple_begin (uiout, "...");
          old_cleanup = make_cleanup ((void(*)(void *)) ui_out_tuple_end,
                                      uiout);

 - Function: void ui_out_list_begin (struct ui_out *UIOUT, const char
          *ID)
     This function marks the beginning of a list output.  ID points to
     an optional string that identifies the list; it is copied by the
     implementation, and so strings in `malloc'ed storage can be freed
     after the call.

 - Function: void ui_out_list_end (struct ui_out *UIOUT)
     This function signals an end of a list output.  There should be
     exactly one call to `ui_out_list_end' for each call to
     `ui_out_list_begin', otherwise an internal GDB error will be
     signaled.

 - Function: struct cleanup *make_cleanup_ui_out_list_begin_end (struct
          ui_out *UIOUT, const char *ID)
     Similar to `make_cleanup_ui_out_tuple_begin_end', this function
     opens a list and then establishes cleanup (*note Cleanups: Coding.)
     that will close the list.list.

Item Output Functions
---------------------

   The functions described below produce output for the actual data
items, or fields, which contain information about the object.

   Choose the appropriate function accordingly to your particular needs.

 - Function: void ui_out_field_fmt (struct ui_out *UIOUT, char
          *FLDNAME, char *FORMAT, ...)
     This is the most general output function.  It produces the
     representation of the data in the variable-length argument list
     according to formatting specifications in FORMAT, a `printf'-like
     format string.  The optional argument FLDNAME supplies the name of
     the field.  The data items themselves are supplied as additional
     arguments after FORMAT.

     This generic function should be used only when it is not possible
     to use one of the specialized versions (see below).

 - Function: void ui_out_field_int (struct ui_out *UIOUT, const char
          *FLDNAME, int VALUE)
     This function outputs a value of an `int' variable.  It uses the
     `"%d"' output conversion specification.  FLDNAME specifies the
     name of the field.

 - Function: void ui_out_field_core_addr (struct ui_out *UIOUT, const
          char *FLDNAME, CORE_ADDR ADDRESS)
     This function outputs an address.

 - Function: void ui_out_field_string (struct ui_out *UIOUT, const char
          *FLDNAME, const char *STRING)
     This function outputs a string using the `"%s"' conversion
     specification.

   Sometimes, there's a need to compose your output piece by piece using
functions that operate on a stream, such as `value_print' or
`fprintf_symbol_filtered'.  These functions accept an argument of the
type `struct ui_file *', a pointer to a `ui_file' object used to store
the data stream used for the output.  When you use one of these
functions, you need a way to pass their results stored in a `ui_file'
object to the `ui_out' functions.  To this end, you first create a
`ui_stream' object by calling `ui_out_stream_new', pass the `stream'
member of that `ui_stream' object to `value_print' and similar
functions, and finally call `ui_out_field_stream' to output the field
you constructed.  When the `ui_stream' object is no longer needed, you
should destroy it and free its memory by calling `ui_out_stream_delete'.

 - Function: struct ui_stream *ui_out_stream_new (struct ui_out *UIOUT)
     This function creates a new `ui_stream' object which uses the same
     output methods as the `ui_out' object whose pointer is passed in
     UIOUT.  It returns a pointer to the newly created `ui_stream'
     object.

 - Function: void ui_out_stream_delete (struct ui_stream *STREAMBUF)
     This functions destroys a `ui_stream' object specified by
     STREAMBUF.

 - Function: void ui_out_field_stream (struct ui_out *UIOUT, const char
          *FIELDNAME, struct ui_stream *STREAMBUF)
     This function consumes all the data accumulated in
     `streambuf->stream' and outputs it like `ui_out_field_string'
     does.  After a call to `ui_out_field_stream', the accumulated data
     no longer exists, but the stream is still valid and may be used
     for producing more fields.

   *Important:* If there is any chance that your code could bail out
before completing output generation and reaching the point where
`ui_out_stream_delete' is called, it is necessary to set up a cleanup,
to avoid leaking memory and other resources.  Here's a skeleton code to
do that:

      struct ui_stream *mybuf = ui_out_stream_new (uiout);
      struct cleanup *old = make_cleanup (ui_out_stream_delete, mybuf);
      ...
      do_cleanups (old);

   If the function already has the old cleanup chain set (for other
kinds of cleanups), you just have to add your cleanup to it:

       mybuf = ui_out_stream_new (uiout);
       make_cleanup (ui_out_stream_delete, mybuf);

   Note that with cleanups in place, you should not call
`ui_out_stream_delete' directly, or you would attempt to free the same
buffer twice.

Utility Output Functions
------------------------

 - Function: void ui_out_field_skip (struct ui_out *UIOUT, const char
          *FLDNAME)
     This function skips a field in a table.  Use it if you have to
     leave an empty field without disrupting the table alignment.  The
     argument FLDNAME specifies a name for the (missing) filed.

 - Function: void ui_out_text (struct ui_out *UIOUT, const char *STRING)
     This function outputs the text in STRING in a way that makes it
     easy to be read by humans.  For example, the console
     implementation of this method filters the text through a built-in
     pager, to prevent it from scrolling off the visible portion of the
     screen.

     Use this function for printing relatively long chunks of text
     around the actual field data: the text it produces is not aligned
     according to the table's format.  Use `ui_out_field_string' to
     output a string field, and use `ui_out_message', described below,
     to output short messages.

 - Function: void ui_out_spaces (struct ui_out *UIOUT, int NSPACES)
     This function outputs NSPACES spaces.  It is handy to align the
     text produced by `ui_out_text' with the rest of the table or list.

 - Function: void ui_out_message (struct ui_out *UIOUT, int VERBOSITY,
          const char *FORMAT, ...)
     This function produces a formatted message, provided that the
     current verbosity level is at least as large as given by
     VERBOSITY.  The current verbosity level is specified by the user
     with the `set verbositylevel' command.(2)

 - Function: void ui_out_wrap_hint (struct ui_out *UIOUT, char *INDENT)
     This function gives the console output filter (a paging filter) a
     hint of where to break lines which are too long.  Ignored for all
     other output consumers.  INDENT, if non-`NULL', is the string to
     be printed to indent the wrapped text on the next line; it must
     remain accessible until the next call to `ui_out_wrap_hint', or
     until an explicit newline is produced by one of the other
     functions.  If INDENT is `NULL', the wrapped text will not be
     indented.

 - Function: void ui_out_flush (struct ui_out *UIOUT)
     This function flushes whatever output has been accumulated so far,
     if the UI buffers output.

Examples of Use of `ui_out' functions
-------------------------------------

   This section gives some practical examples of using the `ui_out'
functions to generalize the old console-oriented code in GDB.  The
examples all come from functions defined on the `breakpoints.c' file.

   This example, from the `breakpoint_1' function, shows how to produce
a table.

   The original code was:

      if (!found_a_breakpoint++)
        {
          annotate_breakpoints_headers ();
     
          annotate_field (0);
          printf_filtered ("Num ");
          annotate_field (1);
          printf_filtered ("Type           ");
          annotate_field (2);
          printf_filtered ("Disp ");
          annotate_field (3);
          printf_filtered ("Enb ");
          if (addressprint)
            {
              annotate_field (4);
              printf_filtered ("Address    ");
            }
          annotate_field (5);
          printf_filtered ("What\n");
     
          annotate_breakpoints_table ();
        }

   Here's the new version:

       nr_printable_breakpoints = ...;
     
       if (addressprint)
         ui_out_table_begin (ui, 6, nr_printable_breakpoints, "BreakpointTable");
       else
         ui_out_table_begin (ui, 5, nr_printable_breakpoints, "BreakpointTable");
     
       if (nr_printable_breakpoints > 0)
         annotate_breakpoints_headers ();
       if (nr_printable_breakpoints > 0)
         annotate_field (0);
       ui_out_table_header (uiout, 3, ui_left, "number", "Num");		/* 1 */
       if (nr_printable_breakpoints > 0)
         annotate_field (1);
       ui_out_table_header (uiout, 14, ui_left, "type", "Type");		/* 2 */
       if (nr_printable_breakpoints > 0)
         annotate_field (2);
       ui_out_table_header (uiout, 4, ui_left, "disp", "Disp");		/* 3 */
       if (nr_printable_breakpoints > 0)
         annotate_field (3);
       ui_out_table_header (uiout, 3, ui_left, "enabled", "Enb");	/* 4 */
       if (addressprint)
         {
          if (nr_printable_breakpoints > 0)
            annotate_field (4);
          if (TARGET_ADDR_BIT <= 32)
            ui_out_table_header (uiout, 10, ui_left, "addr", "Address");/* 5 */
          else
            ui_out_table_header (uiout, 18, ui_left, "addr", "Address");/* 5 */
         }
       if (nr_printable_breakpoints > 0)
         annotate_field (5);
       ui_out_table_header (uiout, 40, ui_noalign, "what", "What");	/* 6 */
       ui_out_table_body (uiout);
       if (nr_printable_breakpoints > 0)
         annotate_breakpoints_table ();

   This example, from the `print_one_breakpoint' function, shows how to
produce the actual data for the table whose structure was defined in
the above example.  The original code was:

        annotate_record ();
        annotate_field (0);
        printf_filtered ("%-3d ", b->number);
        annotate_field (1);
        if ((int)b->type > (sizeof(bptypes)/sizeof(bptypes[0]))
            || ((int) b->type != bptypes[(int) b->type].type))
          internal_error ("bptypes table does not describe type #%d.",
                          (int)b->type);
        printf_filtered ("%-14s ", bptypes[(int)b->type].description);
        annotate_field (2);
        printf_filtered ("%-4s ", bpdisps[(int)b->disposition]);
        annotate_field (3);
        printf_filtered ("%-3c ", bpenables[(int)b->enable]);
        ...

   This is the new version:

        annotate_record ();
        ui_out_tuple_begin (uiout, "bkpt");
        annotate_field (0);
        ui_out_field_int (uiout, "number", b->number);
        annotate_field (1);
        if (((int) b->type > (sizeof (bptypes) / sizeof (bptypes[0])))
            || ((int) b->type != bptypes[(int) b->type].type))
          internal_error ("bptypes table does not describe type #%d.",
                          (int) b->type);
        ui_out_field_string (uiout, "type", bptypes[(int)b->type].description);
        annotate_field (2);
        ui_out_field_string (uiout, "disp", bpdisps[(int)b->disposition]);
        annotate_field (3);
        ui_out_field_fmt (uiout, "enabled", "%c", bpenables[(int)b->enable]);
        ...

   This example, also from `print_one_breakpoint', shows how to produce
a complicated output field using the `print_expression' functions which
requires a stream to be passed.  It also shows how to automate stream
destruction with cleanups.  The original code was:

         annotate_field (5);
         print_expression (b->exp, gdb_stdout);

   The new version is:

       struct ui_stream *stb = ui_out_stream_new (uiout);
       struct cleanup *old_chain = make_cleanup_ui_out_stream_delete (stb);
       ...
       annotate_field (5);
       print_expression (b->exp, stb->stream);
       ui_out_field_stream (uiout, "what", local_stream);

   This example, also from `print_one_breakpoint', shows how to use
`ui_out_text' and `ui_out_field_string'.  The original code was:

       annotate_field (5);
       if (b->dll_pathname == NULL)
         printf_filtered ("<any library> ");
       else
         printf_filtered ("library \"%s\" ", b->dll_pathname);

   It became:

       annotate_field (5);
       if (b->dll_pathname == NULL)
         {
           ui_out_field_string (uiout, "what", "<any library>");
           ui_out_spaces (uiout, 1);
         }
       else
         {
           ui_out_text (uiout, "library \"");
           ui_out_field_string (uiout, "what", b->dll_pathname);
           ui_out_text (uiout, "\" ");
         }

   The following example from `print_one_breakpoint' shows how to use
`ui_out_field_int' and `ui_out_spaces'.  The original code was:

       annotate_field (5);
       if (b->forked_inferior_pid != 0)
         printf_filtered ("process %d ", b->forked_inferior_pid);

   It became:

       annotate_field (5);
       if (b->forked_inferior_pid != 0)
         {
           ui_out_text (uiout, "process ");
           ui_out_field_int (uiout, "what", b->forked_inferior_pid);
           ui_out_spaces (uiout, 1);
         }

   Here's an example of using `ui_out_field_string'.  The original code
was:

       annotate_field (5);
       if (b->exec_pathname != NULL)
         printf_filtered ("program \"%s\" ", b->exec_pathname);

   It became:

       annotate_field (5);
       if (b->exec_pathname != NULL)
         {
           ui_out_text (uiout, "program \"");
           ui_out_field_string (uiout, "what", b->exec_pathname);
           ui_out_text (uiout, "\" ");
         }

   Finally, here's an example of printing an address.  The original
code:

       annotate_field (4);
       printf_filtered ("%s ",
             local_hex_string_custom ((unsigned long) b->address, "08l"));

   It became:

       annotate_field (4);
       ui_out_field_core_addr (uiout, "Address", b->address);

Console Printing
================

TUI
===

   ---------- Footnotes ----------

   (1) The function cast is not portable ISO C.

   (2) As of this writing (April 2001), setting verbosity level is not
yet implemented, and is always returned as zero.  So calling
`ui_out_message' with a VERBOSITY argument more than zero will cause
the message to never be printed.


File: gdbint.info,  Node: libgdb,  Next: Symbol Handling,  Prev: User Interface,  Up: Top

libgdb
******

libgdb 1.0
==========

   `libgdb' 1.0 was an abortive project of years ago.  The theory was
to provide an API to GDB's functionality.

libgdb 2.0
==========

   `libgdb' 2.0 is an ongoing effort to update GDB so that is better
able to support graphical and other environments.

   Since `libgdb' development is on-going, its architecture is still
evolving.  The following components have so far been identified:

   * Observer - `gdb-events.h'.

   * Builder - `ui-out.h'

   * Event Loop - `event-loop.h'

   * Library - `gdb.h'

   The model that ties these components together is described below.

The `libgdb' Model
==================

   A client of `libgdb' interacts with the library in two ways.

   * As an observer (using `gdb-events') receiving notifications from
     `libgdb' of any internal state changes (break point changes, run
     state, etc).

   * As a client querying `libgdb' (using the `ui-out' builder) to
     obtain various status values from GDB.

   Since `libgdb' could have multiple clients (e.g. a GUI supporting
the existing GDB CLI), those clients must co-operate when controlling
`libgdb'.  In particular, a client must ensure that `libgdb' is idle
(i.e. no other client is using `libgdb') before responding to a
`gdb-event' by making a query.

CLI support
===========

   At present GDB's CLI is very much entangled in with the core of
`libgdb'.  Consequently, a client wishing to include the CLI in their
interface needs to carefully co-ordinate its own and the CLI's
requirements.

   It is suggested that the client set `libgdb' up to be bi-modal
(alternate between CLI and client query modes).  The notes below sketch
out the theory:

   * The client registers itself as an observer of `libgdb'.

   * The client create and install `cli-out' builder using its own
     versions of the `ui-file' `gdb_stderr', `gdb_stdtarg' and
     `gdb_stdout' streams.

   * The client creates a separate custom `ui-out' builder that is only
     used while making direct queries to `libgdb'.

   When the client receives input intended for the CLI, it simply
passes it along.  Since the `cli-out' builder is installed by default,
all the CLI output in response to that command is routed (pronounced
rooted) through to the client controlled `gdb_stdout' et. al. streams.
At the same time, the client is kept abreast of internal changes by
virtue of being a `libgdb' observer.

   The only restriction on the client is that it must wait until
`libgdb' becomes idle before initiating any queries (using the client's
custom builder).

`libgdb' components
===================

Observer - `gdb-events.h'
-------------------------

   `gdb-events' provides the client with a very raw mechanism that can
be used to implement an observer.  At present it only allows for one
observer and that observer must, internally, handle the need to delay
the processing of any event notifications until after `libgdb' has
finished the current command.

Builder - `ui-out.h'
--------------------

   `ui-out' provides the infrastructure necessary for a client to
create a builder.  That builder is then passed down to `libgdb' when
doing any queries.

Event Loop - `event-loop.h'
---------------------------

   `event-loop', currently non-re-entrant, provides a simple event
loop.  A client would need to either plug its self into this loop or,
implement a new event-loop that GDB would use.

   The event-loop will eventually be made re-entrant.  This is so that
{No value for `GDB'} can better handle the problem of some commands
blocking instead of returning.

Library - `gdb.h'
-----------------

   `libgdb' is the most obvious component of this system.  It provides
the query interface.  Each function is parameterized by a `ui-out'
builder.  The result of the query is constructed using that builder
before the query function returns.


File: gdbint.info,  Node: Symbol Handling,  Next: Language Support,  Prev: libgdb,  Up: Top

Symbol Handling
***************

   Symbols are a key part of GDB's operation.  Symbols include
variables, functions, and types.

Symbol Reading
==============

   GDB reads symbols from "symbol files".  The usual symbol file is the
file containing the program which GDB is debugging.  GDB can be
directed to use a different file for symbols (with the `symbol-file'
command), and it can also read more symbols via the `add-file' and
`load' commands, or while reading symbols from shared libraries.

   Symbol files are initially opened by code in `symfile.c' using the
BFD library (*note Support Libraries::).  BFD identifies the type of
the file by examining its header.  `find_sym_fns' then uses this
identification to locate a set of symbol-reading functions.

   Symbol-reading modules identify themselves to GDB by calling
`add_symtab_fns' during their module initialization.  The argument to
`add_symtab_fns' is a `struct sym_fns' which contains the name (or name
prefix) of the symbol format, the length of the prefix, and pointers to
four functions.  These functions are called at various times to process
symbol files whose identification matches the specified prefix.

   The functions supplied by each module are:

`XYZ_symfile_init(struct sym_fns *sf)'
     Called from `symbol_file_add' when we are about to read a new
     symbol file.  This function should clean up any internal state
     (possibly resulting from half-read previous files, for example)
     and prepare to read a new symbol file.  Note that the symbol file
     which we are reading might be a new "main" symbol file, or might
     be a secondary symbol file whose symbols are being added to the
     existing symbol table.

     The argument to `XYZ_symfile_init' is a newly allocated `struct
     sym_fns' whose `bfd' field contains the BFD for the new symbol
     file being read.  Its `private' field has been zeroed, and can be
     modified as desired.  Typically, a struct of private information
     will be `malloc''d, and a pointer to it will be placed in the
     `private' field.

     There is no result from `XYZ_symfile_init', but it can call
     `error' if it detects an unavoidable problem.

`XYZ_new_init()'
     Called from `symbol_file_add' when discarding existing symbols.
     This function needs only handle the symbol-reading module's
     internal state; the symbol table data structures visible to the
     rest of GDB will be discarded by `symbol_file_add'.  It has no
     arguments and no result.  It may be called after
     `XYZ_symfile_init', if a new symbol table is being read, or may be
     called alone if all symbols are simply being discarded.

`XYZ_symfile_read(struct sym_fns *sf, CORE_ADDR addr, int mainline)'
     Called from `symbol_file_add' to actually read the symbols from a
     symbol-file into a set of psymtabs or symtabs.

     `sf' points to the `struct sym_fns' originally passed to
     `XYZ_sym_init' for possible initialization.  `addr' is the offset
     between the file's specified start address and its true address in
     memory.  `mainline' is 1 if this is the main symbol table being
     read, and 0 if a secondary symbol file (e.g. shared library or
     dynamically loaded file) is being read.

   In addition, if a symbol-reading module creates psymtabs when
XYZ_symfile_read is called, these psymtabs will contain a pointer to a
function `XYZ_psymtab_to_symtab', which can be called from any point in
the GDB symbol-handling code.

`XYZ_psymtab_to_symtab (struct partial_symtab *pst)'
     Called from `psymtab_to_symtab' (or the `PSYMTAB_TO_SYMTAB' macro)
     if the psymtab has not already been read in and had its
     `pst->symtab' pointer set.  The argument is the psymtab to be
     fleshed-out into a symtab.  Upon return, `pst->readin' should have
     been set to 1, and `pst->symtab' should contain a pointer to the
     new corresponding symtab, or zero if there were no symbols in that
     part of the symbol file.

Partial Symbol Tables
=====================

   GDB has three types of symbol tables:

   * Full symbol tables ("symtabs").  These contain the main
     information about symbols and addresses.

   * Partial symbol tables ("psymtabs").  These contain enough
     information to know when to read the corresponding part of the full
     symbol table.

   * Minimal symbol tables ("msymtabs").  These contain information
     gleaned from non-debugging symbols.

   This section describes partial symbol tables.

   A psymtab is constructed by doing a very quick pass over an
executable file's debugging information.  Small amounts of information
are extracted--enough to identify which parts of the symbol table will
need to be re-read and fully digested later, when the user needs the
information.  The speed of this pass causes GDB to start up very
quickly.  Later, as the detailed rereading occurs, it occurs in small
pieces, at various times, and the delay therefrom is mostly invisible to
the user.

   The symbols that show up in a file's psymtab should be, roughly,
those visible to the debugger's user when the program is not running
code from that file.  These include external symbols and types, static
symbols and types, and `enum' values declared at file scope.

   The psymtab also contains the range of instruction addresses that the
full symbol table would represent.

   The idea is that there are only two ways for the user (or much of the
code in the debugger) to reference a symbol:

   * By its address (e.g. execution stops at some address which is
     inside a function in this file).  The address will be noticed to
     be in the range of this psymtab, and the full symtab will be read
     in.  `find_pc_function', `find_pc_line', and other `find_pc_...'
     functions handle this.

   * By its name (e.g. the user asks to print a variable, or set a
     breakpoint on a function).  Global names and file-scope names will
     be found in the psymtab, which will cause the symtab to be pulled
     in.  Local names will have to be qualified by a global name, or a
     file-scope name, in which case we will have already read in the
     symtab as we evaluated the qualifier.  Or, a local symbol can be
     referenced when we are "in" a local scope, in which case the first
     case applies.  `lookup_symbol' does most of the work here.

   The only reason that psymtabs exist is to cause a symtab to be read
in at the right moment.  Any symbol that can be elided from a psymtab,
while still causing that to happen, should not appear in it.  Since
psymtabs don't have the idea of scope, you can't put local symbols in
them anyway.  Psymtabs don't have the idea of the type of a symbol,
either, so types need not appear, unless they will be referenced by
name.

   It is a bug for GDB to behave one way when only a psymtab has been
read, and another way if the corresponding symtab has been read in.
Such bugs are typically caused by a psymtab that does not contain all
the visible symbols, or which has the wrong instruction address ranges.

   The psymtab for a particular section of a symbol file (objfile)
could be thrown away after the symtab has been read in.  The symtab
should always be searched before the psymtab, so the psymtab will never
be used (in a bug-free environment).  Currently, psymtabs are allocated
on an obstack, and all the psymbols themselves are allocated in a pair
of large arrays on an obstack, so there is little to be gained by
trying to free them unless you want to do a lot more work.

Types
=====

Fundamental Types (e.g., `FT_VOID', `FT_BOOLEAN').
--------------------------------------------------

   These are the fundamental types that GDB uses internally.
Fundamental types from the various debugging formats (stabs, ELF, etc)
are mapped into one of these.  They are basically a union of all
fundamental types that GDB knows about for all the languages that GDB
knows about.

Type Codes (e.g., `TYPE_CODE_PTR', `TYPE_CODE_ARRAY').
------------------------------------------------------

   Each time GDB builds an internal type, it marks it with one of these
types.  The type may be a fundamental type, such as `TYPE_CODE_INT', or
a derived type, such as `TYPE_CODE_PTR' which is a pointer to another
type.  Typically, several `FT_*' types map to one `TYPE_CODE_*' type,
and are distinguished by other members of the type struct, such as
whether the type is signed or unsigned, and how many bits it uses.

Builtin Types (e.g., `builtin_type_void', `builtin_type_char').
---------------------------------------------------------------

   These are instances of type structs that roughly correspond to
fundamental types and are created as global types for GDB to use for
various ugly historical reasons.  We eventually want to eliminate
these.  Note for example that `builtin_type_int' initialized in
`gdbtypes.c' is basically the same as a `TYPE_CODE_INT' type that is
initialized in `c-lang.c' for an `FT_INTEGER' fundamental type.  The
difference is that the `builtin_type' is not associated with any
particular objfile, and only one instance exists, while `c-lang.c'
builds as many `TYPE_CODE_INT' types as needed, with each one
associated with some particular objfile.

Object File Formats
===================

a.out
-----

   The `a.out' format is the original file format for Unix.  It
consists of three sections: `text', `data', and `bss', which are for
program code, initialized data, and uninitialized data, respectively.

   The `a.out' format is so simple that it doesn't have any reserved
place for debugging information.  (Hey, the original Unix hackers used
`adb', which is a machine-language debugger!)  The only debugging
format for `a.out' is stabs, which is encoded as a set of normal
symbols with distinctive attributes.

   The basic `a.out' reader is in `dbxread.c'.

COFF
----

   The COFF format was introduced with System V Release 3 (SVR3) Unix.
COFF files may have multiple sections, each prefixed by a header.  The
number of sections is limited.

   The COFF specification includes support for debugging.  Although this
was a step forward, the debugging information was woefully limited.  For
instance, it was not possible to represent code that came from an
included file.

   The COFF reader is in `coffread.c'.

ECOFF
-----

   ECOFF is an extended COFF originally introduced for Mips and Alpha
workstations.

   The basic ECOFF reader is in `mipsread.c'.

XCOFF
-----

   The IBM RS/6000 running AIX uses an object file format called XCOFF.
The COFF sections, symbols, and line numbers are used, but debugging
symbols are `dbx'-style stabs whose strings are located in the `.debug'
section (rather than the string table).  For more information, see
*Note Top: (stabs)Top.

   The shared library scheme has a clean interface for figuring out what
shared libraries are in use, but the catch is that everything which
refers to addresses (symbol tables and breakpoints at least) needs to be
relocated for both shared libraries and the main executable.  At least
using the standard mechanism this can only be done once the program has
been run (or the core file has been read).

PE
--

   Windows 95 and NT use the PE ("Portable Executable") format for their
executables.  PE is basically COFF with additional headers.

   While BFD includes special PE support, GDB needs only the basic COFF
reader.

ELF
---

   The ELF format came with System V Release 4 (SVR4) Unix.  ELF is
similar to COFF in being organized into a number of sections, but it
removes many of COFF's limitations.

   The basic ELF reader is in `elfread.c'.

SOM
---

   SOM is HP's object file and debug format (not to be confused with
IBM's SOM, which is a cross-language ABI).

   The SOM reader is in `hpread.c'.

Other File Formats
------------------

   Other file formats that have been supported by GDB include Netware
Loadable Modules (`nlmread.c').

Debugging File Formats
======================

   This section describes characteristics of debugging information that
are independent of the object file format.

stabs
-----

   `stabs' started out as special symbols within the `a.out' format.
Since then, it has been encapsulated into other file formats, such as
COFF and ELF.

   While `dbxread.c' does some of the basic stab processing, including
for encapsulated versions, `stabsread.c' does the real work.

COFF
----

   The basic COFF definition includes debugging information.  The level
of support is minimal and non-extensible, and is not often used.

Mips debug (Third Eye)
----------------------

   ECOFF includes a definition of a special debug format.

   The file `mdebugread.c' implements reading for this format.

DWARF 1
-------

   DWARF 1 is a debugging format that was originally designed to be
used with ELF in SVR4 systems.

   The DWARF 1 reader is in `dwarfread.c'.

DWARF 2
-------

   DWARF 2 is an improved but incompatible version of DWARF 1.

   The DWARF 2 reader is in `dwarf2read.c'.

SOM
---

   Like COFF, the SOM definition includes debugging information.

Adding a New Symbol Reader to GDB
=================================

   If you are using an existing object file format (`a.out', COFF, ELF,
etc), there is probably little to be done.

   If you need to add a new object file format, you must first add it to
BFD.  This is beyond the scope of this document.

   You must then arrange for the BFD code to provide access to the
debugging symbols.  Generally GDB will have to call swapping routines
from BFD and a few other BFD internal routines to locate the debugging
information.  As much as possible, GDB should not depend on the BFD
internal data structures.

   For some targets (e.g., COFF), there is a special transfer vector
used to call swapping routines, since the external data structures on
various platforms have different sizes and layouts.  Specialized
routines that will only ever be implemented by one object file format
may be called directly.  This interface should be described in a file
`bfd/libXYZ.h', which is included by GDB.


File: gdbint.info,  Node: Language Support,  Next: Host Definition,  Prev: Symbol Handling,  Up: Top

Language Support
****************

   GDB's language support is mainly driven by the symbol reader,
although it is possible for the user to set the source language
manually.

   GDB chooses the source language by looking at the extension of the
file recorded in the debug info; `.c' means C, `.f' means Fortran, etc.
It may also use a special-purpose language identifier if the debug
format supports it, like with DWARF.

Adding a Source Language to GDB
===============================

   To add other languages to GDB's expression parser, follow the
following steps:

_Create the expression parser._
     This should reside in a file `LANG-exp.y'.  Routines for building
     parsed expressions into a `union exp_element' list are in
     `parse.c'.

     Since we can't depend upon everyone having Bison, and YACC produces
     parsers that define a bunch of global names, the following lines
     *must* be included at the top of the YACC parser, to prevent the
     various parsers from defining the same global names:

          #define yyparse         LANG_parse
          #define yylex           LANG_lex
          #define yyerror         LANG_error
          #define yylval          LANG_lval
          #define yychar          LANG_char
          #define yydebug         LANG_debug
          #define yypact          LANG_pact
          #define yyr1            LANG_r1
          #define yyr2            LANG_r2
          #define yydef           LANG_def
          #define yychk           LANG_chk
          #define yypgo           LANG_pgo
          #define yyact           LANG_act
          #define yyexca          LANG_exca
          #define yyerrflag       LANG_errflag
          #define yynerrs         LANG_nerrs

     At the bottom of your parser, define a `struct language_defn' and
     initialize it with the right values for your language.  Define an
     `initialize_LANG' routine and have it call
     `add_language(LANG_language_defn)' to tell the rest of GDB that
     your language exists.  You'll need some other supporting variables
     and functions, which will be used via pointers from your
     `LANG_language_defn'.  See the declaration of `struct
     language_defn' in `language.h', and the other `*-exp.y' files, for
     more information.

_Add any evaluation routines, if necessary_
     If you need new opcodes (that represent the operations of the
     language), add them to the enumerated type in `expression.h'.  Add
     support code for these operations in the `evaluate_subexp' function
     defined in the file `eval.c'.  Add cases for new opcodes in two
     functions from `parse.c': `prefixify_subexp' and
     `length_of_subexp'.  These compute the number of `exp_element's
     that a given operation takes up.

_Update some existing code_
     Add an enumerated identifier for your language to the enumerated
     type `enum language' in `defs.h'.

     Update the routines in `language.c' so your language is included.
     These routines include type predicates and such, which (in some
     cases) are language dependent.  If your language does not appear
     in the switch statement, an error is reported.

     Also included in `language.c' is the code that updates the variable
     `current_language', and the routines that translate the
     `language_LANG' enumerated identifier into a printable string.

     Update the function `_initialize_language' to include your
     language.  This function picks the default language upon startup,
     so is dependent upon which languages that GDB is built for.

     Update `allocate_symtab' in `symfile.c' and/or symbol-reading code
     so that the language of each symtab (source file) is set properly.
     This is used to determine the language to use at each stack frame
     level.  Currently, the language is set based upon the extension of
     the source file.  If the language can be better inferred from the
     symbol information, please set the language of the symtab in the
     symbol-reading code.

     Add helper code to `print_subexp' (in `expprint.c') to handle any
     new expression opcodes you have added to `expression.h'.  Also,
     add the printed representations of your operators to
     `op_print_tab'.

_Add a place of call_
     Add a call to `LANG_parse()' and `LANG_error' in `parse_exp_1'
     (defined in `parse.c').

_Use macros to trim code_
     The user has the option of building GDB for some or all of the
     languages.  If the user decides to build GDB for the language
     LANG, then every file dependent on `language.h' will have the
     macro `_LANG_LANG' defined in it.  Use `#ifdef's to leave out
     large routines that the user won't need if he or she is not using
     your language.

     Note that you do not need to do this in your YACC parser, since if
     GDB is not build for LANG, then `LANG-exp.tab.o' (the compiled
     form of your parser) is not linked into GDB at all.

     See the file `configure.in' for how GDB is configured for
     different languages.

_Edit `Makefile.in'_
     Add dependencies in `Makefile.in'.  Make sure you update the macro
     variables such as `HFILES' and `OBJS', otherwise your code may not
     get linked in, or, worse yet, it may not get `tar'red into the
     distribution!


File: gdbint.info,  Node: Host Definition,  Next: Target Architecture Definition,  Prev: Language Support,  Up: Top

Host Definition
***************

   With the advent of Autoconf, it's rarely necessary to have host
definition machinery anymore.  The following information is provided,
mainly, as an historical reference.

Adding a New Host
=================

   GDB's host configuration support normally happens via Autoconf.  New
host-specific definitions should not be needed.  Older hosts GDB still
use the host-specific definitions and files listed below, but these
mostly exist for historical reasons, and will eventually disappear.

`gdb/config/ARCH/XYZ.mh'
     This file once contained both host and native configuration
     information (*note Native Debugging::) for the machine XYZ.  The
     host configuration information is now handed by Autoconf.

     Host configuration information included a definition of
     `XM_FILE=xm-XYZ.h' and possibly definitions for `CC',
     `SYSV_DEFINE', `XM_CFLAGS', `XM_ADD_FILES', `XM_CLIBS',
     `XM_CDEPS', etc.; see `Makefile.in'.

     New host only configurations do not need this file.

`gdb/config/ARCH/xm-XYZ.h'
     This file once contained definitions and includes required when
     hosting gdb on machine XYZ.  Those definitions and includes are now
     handled by Autoconf.

     New host and native configurations do not need this file.

     _Maintainer's note: Some hosts continue to use the `xm-xyz.h' file
     to define the macros HOST_FLOAT_FORMAT, HOST_DOUBLE_FORMAT and
     HOST_LONG_DOUBLE_FORMAT.  That code also needs to be replaced with
     either an Autoconf or run-time test._

Generic Host Support Files
--------------------------

   There are some "generic" versions of routines that can be used by
various systems.  These can be customized in various ways by macros
defined in your `xm-XYZ.h' file.  If these routines work for the XYZ
host, you can just include the generic file's name (with `.o', not
`.c') in `XDEPFILES'.

   Otherwise, if your machine needs custom support routines, you will
need to write routines that perform the same functions as the generic
file.  Put them into `XYZ-xdep.c', and put `XYZ-xdep.o' into
`XDEPFILES'.

`ser-unix.c'
     This contains serial line support for Unix systems.  This is always
     included, via the makefile variable `SER_HARDWIRE'; override this
     variable in the `.mh' file to avoid it.

`ser-go32.c'
     This contains serial line support for 32-bit programs running
     under DOS, using the DJGPP (a.k.a. GO32) execution environment.

`ser-tcp.c'
     This contains generic TCP support using sockets.

Host Conditionals
=================

   When GDB is configured and compiled, various macros are defined or
left undefined, to control compilation based on the attributes of the
host system.  These macros and their meanings (or if the meaning is not
documented here, then one of the source files where they are used is
indicated) are:

`GDBINIT_FILENAME'
     The default name of GDB's initialization file (normally
     `.gdbinit').

`NO_STD_REGS'
     This macro is deprecated.

`NO_SYS_FILE'
     Define this if your system does not have a `<sys/file.h>'.

`SIGWINCH_HANDLER'
     If your host defines `SIGWINCH', you can define this to be the name
     of a function to be called if `SIGWINCH' is received.

`SIGWINCH_HANDLER_BODY'
     Define this to expand into code that will define the function
     named by the expansion of `SIGWINCH_HANDLER'.

`ALIGN_STACK_ON_STARTUP'
     Define this if your system is of a sort that will crash in
     `tgetent' if the stack happens not to be longword-aligned when
     `main' is called.  This is a rare situation, but is known to occur
     on several different types of systems.

`CRLF_SOURCE_FILES'
     Define this if host files use `\r\n' rather than `\n' as a line
     terminator.  This will cause source file listings to omit `\r'
     characters when printing and it will allow `\r\n' line endings of
     files which are "sourced" by gdb.  It must be possible to open
     files in binary mode using `O_BINARY' or, for fopen, `"rb"'.

`DEFAULT_PROMPT'
     The default value of the prompt string (normally `"(gdb) "').

`DEV_TTY'
     The name of the generic TTY device, defaults to `"/dev/tty"'.

`FCLOSE_PROVIDED'
     Define this if the system declares `fclose' in the headers included
     in `defs.h'.  This isn't needed unless your compiler is unusually
     anal.

`FOPEN_RB'
     Define this if binary files are opened the same way as text files.

`GETENV_PROVIDED'
     Define this if the system declares `getenv' in its headers included
     in `defs.h'.  This isn't needed unless your compiler is unusually
     anal.

`HAVE_MMAP'
     In some cases, use the system call `mmap' for reading symbol
     tables.  For some machines this allows for sharing and quick
     updates.

`HAVE_TERMIO'
     Define this if the host system has `termio.h'.

`INT_MAX'
`INT_MIN'
`LONG_MAX'
`UINT_MAX'
`ULONG_MAX'
     Values for host-side constants.

`ISATTY'
     Substitute for isatty, if not available.

`LONGEST'
     This is the longest integer type available on the host.  If not
     defined, it will default to `long long' or `long', depending on
     `CC_HAS_LONG_LONG'.

`CC_HAS_LONG_LONG'
     Define this if the host C compiler supports `long long'.  This is
     set by the `configure' script.

`PRINTF_HAS_LONG_LONG'
     Define this if the host can handle printing of long long integers
     via the printf format conversion specifier `ll'.  This is set by
     the `configure' script.

`HAVE_LONG_DOUBLE'
     Define this if the host C compiler supports `long double'.  This is
     set by the `configure' script.

`PRINTF_HAS_LONG_DOUBLE'
     Define this if the host can handle printing of long double
     float-point numbers via the printf format conversion specifier
     `Lg'.  This is set by the `configure' script.

`SCANF_HAS_LONG_DOUBLE'
     Define this if the host can handle the parsing of long double
     float-point numbers via the scanf format conversion specifier
     `Lg'.  This is set by the `configure' script.

`LSEEK_NOT_LINEAR'
     Define this if `lseek (n)' does not necessarily move to byte number
     `n' in the file.  This is only used when reading source files.  It
     is normally faster to define `CRLF_SOURCE_FILES' when possible.

`L_SET'
     This macro is used as the argument to `lseek' (or, most commonly,
     `bfd_seek').  FIXME, should be replaced by SEEK_SET instead, which
     is the POSIX equivalent.

`MMAP_BASE_ADDRESS'
     When using HAVE_MMAP, the first mapping should go at this address.

`MMAP_INCREMENT'
     when using HAVE_MMAP, this is the increment between mappings.

`NORETURN'
     If defined, this should be one or more tokens, such as `volatile',
     that can be used in both the declaration and definition of
     functions to indicate that they never return.  The default is
     already set correctly if compiling with GCC.  This will almost
     never need to be defined.

`ATTR_NORETURN'
     If defined, this should be one or more tokens, such as
     `__attribute__ ((noreturn))', that can be used in the declarations
     of functions to indicate that they never return.  The default is
     already set correctly if compiling with GCC.  This will almost
     never need to be defined.

`USE_GENERIC_DUMMY_FRAMES'
     Define this to 1 if the target is using the generic inferior
     function call code.  See `blockframe.c' for more information.

`USE_MMALLOC'
     GDB will use the `mmalloc' library for memory allocation for
     symbol reading if this symbol is defined.  Be careful defining it
     since there are systems on which `mmalloc' does not work for some
     reason.  One example is the DECstation, where its RPC library can't
     cope with our redefinition of `malloc' to call `mmalloc'.  When
     defining `USE_MMALLOC', you will also have to set `MMALLOC' in the
     Makefile, to point to the `mmalloc' library.  This define is set
     when you configure with `--with-mmalloc'.

`NO_MMCHECK'
     Define this if you are using `mmalloc', but don't want the overhead
     of checking the heap with `mmcheck'.  Note that on some systems,
     the C runtime makes calls to `malloc' prior to calling `main', and
     if `free' is ever called with these pointers after calling
     `mmcheck' to enable checking, a memory corruption abort is certain
     to occur.  These systems can still use `mmalloc', but must define
     `NO_MMCHECK'.

`MMCHECK_FORCE'
     Define this to 1 if the C runtime allocates memory prior to
     `mmcheck' being called, but that memory is never freed so we don't
     have to worry about it triggering a memory corruption abort.  The
     default is 0, which means that `mmcheck' will only install the heap
     checking functions if there has not yet been any memory allocation
     calls, and if it fails to install the functions, GDB will issue a
     warning.  This is currently defined if you configure using
     `--with-mmalloc'.

`NO_SIGINTERRUPT'
     Define this to indicate that `siginterrupt' is not available.

`SEEK_CUR'
`SEEK_SET'
     Define these to appropriate value for the system `lseek', if not
     already defined.

`STOP_SIGNAL'
     This is the signal for stopping GDB.  Defaults to `SIGTSTP'.
     (Only redefined for the Convex.)

`USE_O_NOCTTY'
     Define this if the interior's tty should be opened with the
     `O_NOCTTY' flag.  (FIXME: This should be a native-only flag, but
     `inflow.c' is always linked in.)

`USG'
     Means that System V (prior to SVR4) include files are in use.
     (FIXME: This symbol is abused in `infrun.c', `regex.c',
     `remote-nindy.c', and `utils.c' for other things, at the moment.)

`lint'
     Define this to help placate `lint' in some situations.

`volatile'
     Define this to override the defaults of `__volatile__' or `/**/'.


File: gdbint.info,  Node: Target Architecture Definition,  Next: Target Vector Definition,  Prev: Host Definition,  Up: Top

Target Architecture Definition
******************************

   GDB's target architecture defines what sort of machine-language
programs GDB can work with, and how it works with them.

   The target architecture object is implemented as the C structure
`struct gdbarch *'.  The structure, and its methods, are generated
using the Bourne shell script `gdbarch.sh'.

Operating System ABI Variant Handling
=====================================

   GDB provides a mechanism for handling variations in OS ABIs.  An OS
ABI variant may have influence over any number of variables in the
target architecture definition.  There are two major components in the
OS ABI mechanism: sniffers and handlers.

   A "sniffer" examines a file matching a BFD architecture/flavour pair
(the architecture may be wildcarded) in an attempt to determine the OS
ABI of that file.  Sniffers with a wildcarded architecture are
considered to be "generic", while sniffers for a specific architecture
are considered to be "specific".  A match from a specific sniffer
overrides a match from a generic sniffer.  Multiple sniffers for an
architecture/flavour may exist, in order to differentiate between two
different operating systems which use the same basic file format.  The
OS ABI framework provides a generic sniffer for ELF-format files which
examines the `EI_OSABI' field of the ELF header, as well as note
sections known to be used by several operating systems.

   A "handler" is used to fine-tune the `gdbarch' structure for the
selected OS ABI.  There may be only one handler for a given OS ABI for
each BFD architecture.

   The following OS ABI variants are defined in `osabi.h':

`GDB_OSABI_UNKNOWN'
     The ABI of the inferior is unknown.  The default `gdbarch'
     settings for the architecture will be used.

`GDB_OSABI_SVR4'
     UNIX System V Release 4

`GDB_OSABI_HURD'
     GNU using the Hurd kernel

`GDB_OSABI_SOLARIS'
     Sun Solaris

`GDB_OSABI_OSF1'
     OSF/1, including Digital UNIX and Compaq Tru64 UNIX

`GDB_OSABI_LINUX'
     GNU using the Linux kernel

`GDB_OSABI_FREEBSD_AOUT'
     FreeBSD using the a.out executable format

`GDB_OSABI_FREEBSD_ELF'
     FreeBSD using the ELF executable format

`GDB_OSABI_NETBSD_AOUT'
     NetBSD using the a.out executable format

`GDB_OSABI_NETBSD_ELF'
     NetBSD using the ELF executable format

`GDB_OSABI_WINCE'
     Windows CE

`GDB_OSABI_GO32'
     DJGPP

`GDB_OSABI_NETWARE'
     Novell NetWare

`GDB_OSABI_ARM_EABI_V1'
     ARM Embedded ABI version 1

`GDB_OSABI_ARM_EABI_V2'
     ARM Embedded ABI version 2

`GDB_OSABI_ARM_APCS'
     Generic ARM Procedure Call Standard

   Here are the functions that make up the OS ABI framework:

 - Function: const char *gdbarch_osabi_name (enum gdb_osabi OSABI)
     Return the name of the OS ABI corresponding to OSABI.

 - Function: void gdbarch_register_osabi (enum bfd_architecture ARCH,
          enum gdb_osabi OSABI, void (*INIT_OSABI)(struct gdbarch_info
          INFO, struct gdbarch *GDBARCH))
     Register the OS ABI handler specified by INIT_OSABI for the
     architecture/OS ABI pair specified by ARCH and OSABI.

 - Function: void gdbarch_register_osabi_sniffer (enum bfd_architecture
          ARCH, enum bfd_flavour FLAVOUR, enum gdb_osabi (*SNIFFER)(bfd
          *ABFD))
     Register the OS ABI file sniffer specified by SNIFFER for the BFD
     architecture/flavour pair specified by ARCH and FLAVOUR.  If ARCH
     is `bfd_arch_unknown', the sniffer is considered to be generic,
     and is allowed to examine FLAVOUR-flavoured files for any
     architecture.

 - Function: enum gdb_osabi gdbarch_lookup_osabi (bfd *ABFD)
     Examine the file described by ABFD to determine its OS ABI.  The
     value `GDB_OSABI_UNKNOWN' is returned if the OS ABI cannot be
     determined.

 - Function: void gdbarch_init_osabi (struct gdbarch info INFO, struct
          gdbarch *GDBARCH, enum gdb_osabi OSABI)
     Invoke the OS ABI handler corresponding to OSABI to fine-tune the
     `gdbarch' structure specified by GDBARCH.  If a handler
     corresponding to OSABI has not been registered for GDBARCH's
     architecture, a warning will be issued and the debugging session
     will continue with the defaults already established for GDBARCH.

Registers and Memory
====================

   GDB's model of the target machine is rather simple.  GDB assumes the
machine includes a bank of registers and a block of memory.  Each
register may have a different size.

   GDB does not have a magical way to match up with the compiler's idea
of which registers are which; however, it is critical that they do
match up accurately.  The only way to make this work is to get accurate
information about the order that the compiler uses, and to reflect that
in the `REGISTER_NAME' and related macros.

   GDB can handle big-endian, little-endian, and bi-endian
architectures.

Pointers Are Not Always Addresses
=================================

   On almost all 32-bit architectures, the representation of a pointer
is indistinguishable from the representation of some fixed-length number
whose value is the byte address of the object pointed to.  On such
machines, the words "pointer" and "address" can be used interchangeably.
However, architectures with smaller word sizes are often cramped for
address space, so they may choose a pointer representation that breaks
this identity, and allows a larger code address space.

   For example, the Mitsubishi D10V is a 16-bit VLIW processor whose
instructions are 32 bits long(1).  If the D10V used ordinary byte
addresses to refer to code locations, then the processor would only be
able to address 64kb of instructions.  However, since instructions must
be aligned on four-byte boundaries, the low two bits of any valid
instruction's byte address are always zero--byte addresses waste two
bits.  So instead of byte addresses, the D10V uses word addresses--byte
addresses shifted right two bits--to refer to code.  Thus, the D10V can
use 16-bit words to address 256kb of code space.

   However, this means that code pointers and data pointers have
different forms on the D10V.  The 16-bit word `0xC020' refers to byte
address `0xC020' when used as a data address, but refers to byte address
`0x30080' when used as a code address.

   (The D10V also uses separate code and data address spaces, which also
affects the correspondence between pointers and addresses, but we're
going to ignore that here; this example is already too long.)

   To cope with architectures like this--the D10V is not the only
one!--GDB tries to distinguish between "addresses", which are byte
numbers, and "pointers", which are the target's representation of an
address of a particular type of data.  In the example above, `0xC020'
is the pointer, which refers to one of the addresses `0xC020' or
`0x30080', depending on the type imposed upon it.  GDB provides
functions for turning a pointer into an address and vice versa, in the
appropriate way for the current architecture.

   Unfortunately, since addresses and pointers are identical on almost
all processors, this distinction tends to bit-rot pretty quickly.  Thus,
each time you port GDB to an architecture which does distinguish
between pointers and addresses, you'll probably need to clean up some
architecture-independent code.

   Here are functions which convert between pointers and addresses:

 - Function: CORE_ADDR extract_typed_address (void *BUF, struct type
          *TYPE)
     Treat the bytes at BUF as a pointer or reference of type TYPE, and
     return the address it represents, in a manner appropriate for the
     current architecture.  This yields an address GDB can use to read
     target memory, disassemble, etc.  Note that BUF refers to a buffer
     in GDB's memory, not the inferior's.

     For example, if the current architecture is the Intel x86, this
     function extracts a little-endian integer of the appropriate
     length from BUF and returns it.  However, if the current
     architecture is the D10V, this function will return a 16-bit
     integer extracted from BUF, multiplied by four if TYPE is a
     pointer to a function.

     If TYPE is not a pointer or reference type, then this function
     will signal an internal error.

 - Function: CORE_ADDR store_typed_address (void *BUF, struct type
          *TYPE, CORE_ADDR ADDR)
     Store the address ADDR in BUF, in the proper format for a pointer
     of type TYPE in the current architecture.  Note that BUF refers to
     a buffer in GDB's memory, not the inferior's.

     For example, if the current architecture is the Intel x86, this
     function stores ADDR unmodified as a little-endian integer of the
     appropriate length in BUF.  However, if the current architecture
     is the D10V, this function divides ADDR by four if TYPE is a
     pointer to a function, and then stores it in BUF.

     If TYPE is not a pointer or reference type, then this function
     will signal an internal error.

 - Function: CORE_ADDR value_as_address (struct value *VAL)
     Assuming that VAL is a pointer, return the address it represents,
     as appropriate for the current architecture.

     This function actually works on integral values, as well as
     pointers.  For pointers, it performs architecture-specific
     conversions as described above for `extract_typed_address'.

 - Function: CORE_ADDR value_from_pointer (struct type *TYPE, CORE_ADDR
          ADDR)
     Create and return a value representing a pointer of type TYPE to
     the address ADDR, as appropriate for the current architecture.
     This function performs architecture-specific conversions as
     described above for `store_typed_address'.

   GDB also provides functions that do the same tasks, but assume that
pointers are simply byte addresses; they aren't sensitive to the
current architecture, beyond knowing the appropriate endianness.

 - Function: CORE_ADDR extract_address (void *ADDR, int len)
     Extract a LEN-byte number from ADDR in the appropriate endianness
     for the current architecture, and return it.  Note that ADDR
     refers to GDB's memory, not the inferior's.

     This function should only be used in architecture-specific code; it
     doesn't have enough information to turn bits into a true address
     in the appropriate way for the current architecture.  If you can,
     use `extract_typed_address' instead.

 - Function: void store_address (void *ADDR, int LEN, LONGEST VAL)
     Store VAL at ADDR as a LEN-byte integer, in the appropriate
     endianness for the current architecture.  Note that ADDR refers to
     a buffer in GDB's memory, not the inferior's.

     This function should only be used in architecture-specific code; it
     doesn't have enough information to turn a true address into bits
     in the appropriate way for the current architecture.  If you can,
     use `store_typed_address' instead.

   Here are some macros which architectures can define to indicate the
relationship between pointers and addresses.  These have default
definitions, appropriate for architectures on which all pointers are
simple unsigned byte addresses.

 - Target Macro: CORE_ADDR POINTER_TO_ADDRESS (struct type *TYPE, char
          *BUF)
     Assume that BUF holds a pointer of type TYPE, in the appropriate
     format for the current architecture.  Return the byte address the
     pointer refers to.

     This function may safely assume that TYPE is either a pointer or a
     C++ reference type.

 - Target Macro: void ADDRESS_TO_POINTER (struct type *TYPE, char *BUF,
          CORE_ADDR ADDR)
     Store in BUF a pointer of type TYPE representing the address ADDR,
     in the appropriate format for the current architecture.

     This function may safely assume that TYPE is either a pointer or a
     C++ reference type.

Raw and Virtual Register Representations
========================================

   _Maintainer note: This section is pretty much obsolete.  The
functionality described here has largely been replaced by
pseudo-registers and the mechanisms described in *Note Using Different
Register and Memory Data Representations: Target Architecture
Definition.  See also Bug Tracking Database
(http://www.gnu.org/software/gdb/bugs/) and ARI Index
(http://sources.redhat.com/gdb/current/ari/) for more up-to-date
information._

   Some architectures use one representation for a value when it lives
in a register, but use a different representation when it lives in
memory.  In GDB's terminology, the "raw" representation is the one used
in the target registers, and the "virtual" representation is the one
used in memory, and within GDB `struct value' objects.

   _Maintainer note: Notice that the same mechanism is being used to
both convert a register to a `struct value' and alternative register
forms._

   For almost all data types on almost all architectures, the virtual
and raw representations are identical, and no special handling is
needed.  However, they do occasionally differ.  For example:

   * The x86 architecture supports an 80-bit `long double' type.
     However, when we store those values in memory, they occupy twelve
     bytes: the floating-point number occupies the first ten, and the
     final two bytes are unused.  This keeps the values aligned on
     four-byte boundaries, allowing more efficient access.  Thus, the
     x86 80-bit floating-point type is the raw representation, and the
     twelve-byte loosely-packed arrangement is the virtual
     representation.

   * Some 64-bit MIPS targets present 32-bit registers to GDB as 64-bit
     registers, with garbage in their upper bits.  GDB ignores the top
     32 bits.  Thus, the 64-bit form, with garbage in the upper 32
     bits, is the raw representation, and the trimmed 32-bit
     representation is the virtual representation.

   In general, the raw representation is determined by the
architecture, or GDB's interface to the architecture, while the virtual
representation can be chosen for GDB's convenience.  GDB's register
file, `registers', holds the register contents in raw format, and the
GDB remote protocol transmits register values in raw format.

   Your architecture may define the following macros to request
conversions between the raw and virtual format:

 - Target Macro: int REGISTER_CONVERTIBLE (int REG)
     Return non-zero if register number REG's value needs different raw
     and virtual formats.

     You should not use `REGISTER_CONVERT_TO_VIRTUAL' for a register
     unless this macro returns a non-zero value for that register.

 - Target Macro: int REGISTER_RAW_SIZE (int REG)
     The size of register number REG's raw value.  This is the number
     of bytes the register will occupy in `registers', or in a GDB
     remote protocol packet.

 - Target Macro: int REGISTER_VIRTUAL_SIZE (int REG)
     The size of register number REG's value, in its virtual format.
     This is the size a `struct value''s buffer will have, holding that
     register's value.

 - Target Macro: struct type *REGISTER_VIRTUAL_TYPE (int REG)
     This is the type of the virtual representation of register number
     REG.  Note that there is no need for a macro giving a type for the
     register's raw form; once the register's value has been obtained,
     GDB always uses the virtual form.

 - Target Macro: void REGISTER_CONVERT_TO_VIRTUAL (int REG, struct type
          *TYPE, char *FROM, char *TO)
     Convert the value of register number REG to TYPE, which should
     always be `REGISTER_VIRTUAL_TYPE (REG)'.  The buffer at FROM holds
     the register's value in raw format; the macro should convert the
     value to virtual format, and place it at TO.

     Note that `REGISTER_CONVERT_TO_VIRTUAL' and
     `REGISTER_CONVERT_TO_RAW' take their REG and TYPE arguments in
     different orders.

     You should only use `REGISTER_CONVERT_TO_VIRTUAL' with registers
     for which the `REGISTER_CONVERTIBLE' macro returns a non-zero
     value.

 - Target Macro: void REGISTER_CONVERT_TO_RAW (struct type *TYPE, int
          REG, char *FROM, char *TO)
     Convert the value of register number REG to TYPE, which should
     always be `REGISTER_VIRTUAL_TYPE (REG)'.  The buffer at FROM holds
     the register's value in raw format; the macro should convert the
     value to virtual format, and place it at TO.

     Note that REGISTER_CONVERT_TO_VIRTUAL and REGISTER_CONVERT_TO_RAW
     take their REG and TYPE arguments in different orders.

Using Different Register and Memory Data Representations
========================================================

   _Maintainer's note: The way GDB manipulates registers is undergoing
significant change.  Many of the macros and functions refered to in this
section are likely to be subject to further revision.  See A.R. Index
(http://sources.redhat.com/gdb/current/ari/) and Bug Tracking Database
(http://www.gnu.org/software/gdb/bugs) for further information.
cagney/2002-05-06._

   Some architectures can represent a data object in a register using a
form that is different to the objects more normal memory representation.
For example:

   * The Alpha architecture can represent 32 bit integer values in
     floating-point registers.

   * The x86 architecture supports 80-bit floating-point registers.  The
     `long double' data type occupies 96 bits in memory but only 80 bits
     when stored in a register.


   In general, the register representation of a data type is determined
by the architecture, or GDB's interface to the architecture, while the
memory representation is determined by the Application Binary Interface.

   For almost all data types on almost all architectures, the two
representations are identical, and no special handling is needed.
However, they do occasionally differ.  Your architecture may define the
following macros to request conversions between the register and memory
representations of a data type:

 - Target Macro: int CONVERT_REGISTER_P (int REG)
     Return non-zero if the representation of a data value stored in
     this register may be different to the representation of that same
     data value when stored in memory.

     When non-zero, the macros `REGISTER_TO_VALUE' and
     `VALUE_TO_REGISTER' are used to perform any necessary conversion.

 - Target Macro: void REGISTER_TO_VALUE (int REG, struct type *TYPE,
          char *FROM, char *TO)
     Convert the value of register number REG to a data object of type
     TYPE.  The buffer at FROM holds the register's value in raw
     format; the converted value should be placed in the buffer at TO.

     Note that `REGISTER_TO_VALUE' and `VALUE_TO_REGISTER' take their
     REG and TYPE arguments in different orders.

     You should only use `REGISTER_TO_VALUE' with registers for which
     the `CONVERT_REGISTER_P' macro returns a non-zero value.

 - Target Macro: void VALUE_TO_REGISTER (struct type *TYPE, int REG,
          char *FROM, char *TO)
     Convert a data value of type TYPE to register number REG' raw
     format.

     Note that `REGISTER_TO_VALUE' and `VALUE_TO_REGISTER' take their
     REG and TYPE arguments in different orders.

     You should only use `VALUE_TO_REGISTER' with registers for which
     the `CONVERT_REGISTER_P' macro returns a non-zero value.

 - Target Macro: void REGISTER_CONVERT_TO_TYPE (int REGNUM, struct type
          *TYPE, char *BUF)
     See `mips-tdep.c'.  It does not do what you want.

Frame Interpretation
====================

Inferior Call Setup
===================

Compiler Characteristics
========================

Target Conditionals
===================

   This section describes the macros that you can use to define the
target machine.

`ADDITIONAL_OPTIONS'
`ADDITIONAL_OPTION_CASES'
`ADDITIONAL_OPTION_HANDLER'
`ADDITIONAL_OPTION_HELP'
     These are a set of macros that allow the addition of additional
     command line options to GDB.  They are currently used only for the
     unsupported i960 Nindy target, and should not be used in any other
     configuration.

`ADDR_BITS_REMOVE (addr)'
     If a raw machine instruction address includes any bits that are not
     really part of the address, then define this macro to expand into
     an expression that zeroes those bits in ADDR.  This is only used
     for addresses of instructions, and even then not in all contexts.

     For example, the two low-order bits of the PC on the
     Hewlett-Packard PA 2.0 architecture contain the privilege level of
     the corresponding instruction.  Since instructions must always be
     aligned on four-byte boundaries, the processor masks out these
     bits to generate the actual address of the instruction.
     ADDR_BITS_REMOVE should filter out these bits with an expression
     such as `((addr) & ~3)'.

`ADDRESS_TO_POINTER (TYPE, BUF, ADDR)'
     Store in BUF a pointer of type TYPE representing the address ADDR,
     in the appropriate format for the current architecture.  This
     macro may safely assume that TYPE is either a pointer or a C++
     reference type.  *Note Pointers Are Not Always Addresses: Target
     Architecture Definition.

`BEFORE_MAIN_LOOP_HOOK'
     Define this to expand into any code that you want to execute
     before the main loop starts.  Although this is not, strictly
     speaking, a target conditional, that is how it is currently being
     used.  Note that if a configuration were to define it one way for
     a host and a different way for the target, GDB will probably not
     compile, let alone run correctly.  This macro is currently used
     only for the unsupported i960 Nindy target, and should not be used
     in any other configuration.

`BELIEVE_PCC_PROMOTION'
     Define if the compiler promotes a `short' or `char' parameter to
     an `int', but still reports the parameter as its original type,
     rather than the promoted type.

`BELIEVE_PCC_PROMOTION_TYPE'
     Define this if GDB should believe the type of a `short' argument
     when compiled by `pcc', but look within a full int space to get
     its value.  Only defined for Sun-3 at present.

`BITS_BIG_ENDIAN'
     Define this if the numbering of bits in the targets does *not*
     match the endianness of the target byte order.  A value of 1 means
     that the bits are numbered in a big-endian bit order, 0 means
     little-endian.

`BREAKPOINT'
     This is the character array initializer for the bit pattern to put
     into memory where a breakpoint is set.  Although it's common to
     use a trap instruction for a breakpoint, it's not required; for
     instance, the bit pattern could be an invalid instruction.  The
     breakpoint must be no longer than the shortest instruction of the
     architecture.

     `BREAKPOINT' has been deprecated in favor of `BREAKPOINT_FROM_PC'.

`BIG_BREAKPOINT'
`LITTLE_BREAKPOINT'
     Similar to BREAKPOINT, but used for bi-endian targets.

     `BIG_BREAKPOINT' and `LITTLE_BREAKPOINT' have been deprecated in
     favor of `BREAKPOINT_FROM_PC'.

`REMOTE_BREAKPOINT'
`LITTLE_REMOTE_BREAKPOINT'
`BIG_REMOTE_BREAKPOINT'
     Similar to BREAKPOINT, but used for remote targets.

     `BIG_REMOTE_BREAKPOINT' and `LITTLE_REMOTE_BREAKPOINT' have been
     deprecated in favor of `BREAKPOINT_FROM_PC'.

`BREAKPOINT_FROM_PC (PCPTR, LENPTR)'
     Use the program counter to determine the contents and size of a
     breakpoint instruction.  It returns a pointer to a string of bytes
     that encode a breakpoint instruction, stores the length of the
     string to *LENPTR, and adjusts pc (if necessary) to point to the
     actual memory location where the breakpoint should be inserted.

     Although it is common to use a trap instruction for a breakpoint,
     it's not required; for instance, the bit pattern could be an
     invalid instruction.  The breakpoint must be no longer than the
     shortest instruction of the architecture.

     Replaces all the other BREAKPOINT macros.

`MEMORY_INSERT_BREAKPOINT (ADDR, CONTENTS_CACHE)'
`MEMORY_REMOVE_BREAKPOINT (ADDR, CONTENTS_CACHE)'
     Insert or remove memory based breakpoints.  Reasonable defaults
     (`default_memory_insert_breakpoint' and
     `default_memory_remove_breakpoint' respectively) have been
     provided so that it is not necessary to define these for most
     architectures.  Architectures which may want to define
     `MEMORY_INSERT_BREAKPOINT' and `MEMORY_REMOVE_BREAKPOINT' will
     likely have instructions that are oddly sized or are not stored in
     a conventional manner.

     It may also be desirable (from an efficiency standpoint) to define
     custom breakpoint insertion and removal routines if
     `BREAKPOINT_FROM_PC' needs to read the target's memory for some
     reason.

`CALL_DUMMY_P'
     A C expression that is non-zero when the target supports inferior
     function calls.

`CALL_DUMMY_WORDS'
     Pointer to an array of `LONGEST' words of data containing
     host-byte-ordered `REGISTER_BYTES' sized values that partially
     specify the sequence of instructions needed for an inferior
     function call.

     Should be deprecated in favor of a macro that uses
     target-byte-ordered data.

`SIZEOF_CALL_DUMMY_WORDS'
     The size of `CALL_DUMMY_WORDS'.  When `CALL_DUMMY_P' this must
     return a positive value.  See also `CALL_DUMMY_LENGTH'.

`CALL_DUMMY'
     A static initializer for `CALL_DUMMY_WORDS'.  Deprecated.

`CALL_DUMMY_LOCATION'
     See the file `inferior.h'.

`CALL_DUMMY_STACK_ADJUST'
     Stack adjustment needed when performing an inferior function call.

     Should be deprecated in favor of something like `STACK_ALIGN'.

`CALL_DUMMY_STACK_ADJUST_P'
     Predicate for use of `CALL_DUMMY_STACK_ADJUST'.

     Should be deprecated in favor of something like `STACK_ALIGN'.

`CANNOT_FETCH_REGISTER (REGNO)'
     A C expression that should be nonzero if REGNO cannot be fetched
     from an inferior process.  This is only relevant if
     `FETCH_INFERIOR_REGISTERS' is not defined.

`CANNOT_STORE_REGISTER (REGNO)'
     A C expression that should be nonzero if REGNO should not be
     written to the target.  This is often the case for program
     counters, status words, and other special registers.  If this is
     not defined, GDB will assume that all registers may be written.

`DO_DEFERRED_STORES'
`CLEAR_DEFERRED_STORES'
     Define this to execute any deferred stores of registers into the
     inferior, and to cancel any deferred stores.

     Currently only implemented correctly for native Sparc
     configurations?

`COERCE_FLOAT_TO_DOUBLE (FORMAL, ACTUAL)'
     Return non-zero if GDB should promote `float' values to `double'
     when calling a non-prototyped function.  The argument ACTUAL is
     the type of the value we want to pass to the function.  The
     argument FORMAL is the type of this argument, as it appears in the
     function's definition.  Note that FORMAL may be zero if we have no
     debugging information for the function, or if we're passing more
     arguments than are officially declared (for example, varargs).
     This macro is never invoked if the function definitely has a
     prototype.

     How you should pass arguments to a function depends on whether it
     was defined in K&R style or prototype style.  If you define a
     function using the K&R syntax that takes a `float' argument, then
     callers must pass that argument as a `double'.  If you define the
     function using the prototype syntax, then you must pass the
     argument as a `float', with no promotion.

     Unfortunately, on certain older platforms, the debug info doesn't
     indicate reliably how each function was defined.  A function type's
     `TYPE_FLAG_PROTOTYPED' flag may be unset, even if the function was
     defined in prototype style.  When calling a function whose
     `TYPE_FLAG_PROTOTYPED' flag is unset, GDB consults the
     `COERCE_FLOAT_TO_DOUBLE' macro to decide what to do.

     For modern targets, it is proper to assume that, if the prototype
     flag is unset, that can be trusted: `float' arguments should be
     promoted to `double'.  You should use the function
     `standard_coerce_float_to_double' to get this behavior.

     For some older targets, if the prototype flag is unset, that
     doesn't tell us anything.  So we guess that, if we don't have a
     type for the formal parameter (i.e., the first argument to
     `COERCE_FLOAT_TO_DOUBLE' is null), then we should promote it;
     otherwise, we should leave it alone.  The function
     `default_coerce_float_to_double' provides this behavior; it is the
     default value, for compatibility with older configurations.

`int CONVERT_REGISTER_P(REGNUM)'
     Return non-zero if register REGNUM can represent data values in a
     non-standard form.  *Note Using Different Register and Memory Data
     Representations: Target Architecture Definition.

`CPLUS_MARKER'
     Define this to expand into the character that G++ uses to
     distinguish compiler-generated identifiers from
     programmer-specified identifiers.  By default, this expands into
     `'$''.  Most System V targets should define this to `'.''.

`DBX_PARM_SYMBOL_CLASS'
     Hook for the `SYMBOL_CLASS' of a parameter when decoding DBX symbol
     information.  In the i960, parameters can be stored as locals or as
     args, depending on the type of the debug record.

`DECR_PC_AFTER_BREAK'
     Define this to be the amount by which to decrement the PC after the
     program encounters a breakpoint.  This is often the number of
     bytes in `BREAKPOINT', though not always.  For most targets this
     value will be 0.

`DECR_PC_AFTER_HW_BREAK'
     Similarly, for hardware breakpoints.

`DISABLE_UNSETTABLE_BREAK (ADDR)'
     If defined, this should evaluate to 1 if ADDR is in a shared
     library in which breakpoints cannot be set and so should be
     disabled.

`DO_REGISTERS_INFO'
     If defined, use this to print the value of a register or all
     registers.

     This method is deprecated.

`PRINT_FLOAT_INFO()'
     If defined, then the `info float' command will print information
     about the processor's floating point unit.

`print_registers_info (GDBARCH, FRAME, REGNUM, ALL)'
     If defined, pretty print the value of the register REGNUM for the
     specified FRAME.  If the value of REGNUM is -1, pretty print
     either all registers (ALL is non zero) or a select subset of
     registers (ALL is zero).

     The default method prints one register per line, and if ALL is
     zero omits floating-point registers.

`PRINT_VECTOR_INFO()'
     If defined, then the `info vector' command will call this function
     to print information about the processor's vector unit.

     By default, the `info vector' command will print all vector
     registers (the register's type having the vector attribute).

`DWARF_REG_TO_REGNUM'
     Convert DWARF register number into GDB regnum.  If not defined, no
     conversion will be performed.

`DWARF2_REG_TO_REGNUM'
     Convert DWARF2 register number into GDB regnum.  If not defined,
     no conversion will be performed.

`ECOFF_REG_TO_REGNUM'
     Convert ECOFF register number into GDB regnum.  If not defined, no
     conversion will be performed.

`END_OF_TEXT_DEFAULT'
     This is an expression that should designate the end of the text
     section.

`EXTRACT_RETURN_VALUE(TYPE, REGBUF, VALBUF)'
     Define this to extract a function's return value of type TYPE from
     the raw register state REGBUF and copy that, in virtual format,
     into VALBUF.

`EXTRACT_STRUCT_VALUE_ADDRESS(REGBUF)'
     When defined, extract from the array REGBUF (containing the raw
     register state) the `CORE_ADDR' at which a function should return
     its structure value.

     If not defined, `EXTRACT_RETURN_VALUE' is used.

`EXTRACT_STRUCT_VALUE_ADDRESS_P()'
     Predicate for `EXTRACT_STRUCT_VALUE_ADDRESS'.

`FLOAT_INFO'
     Deprecated in favor of `PRINT_FLOAT_INFO'.

`FP_REGNUM'
     If the virtual frame pointer is kept in a register, then define
     this macro to be the number (greater than or equal to zero) of
     that register.

     This should only need to be defined if `TARGET_READ_FP' is not
     defined.

`FRAMELESS_FUNCTION_INVOCATION(FI)'
     Define this to an expression that returns 1 if the function
     invocation represented by FI does not have a stack frame
     associated with it.  Otherwise return 0.

`FRAME_ARGS_ADDRESS_CORRECT'
     See `stack.c'.

`FRAME_CHAIN(FRAME)'
     Given FRAME, return a pointer to the calling frame.

`FRAME_CHAIN_VALID(CHAIN, THISFRAME)'
     Define this to be an expression that returns zero if the given
     frame is an outermost frame, with no caller, and nonzero
     otherwise.  Several common definitions are available:

        * `file_frame_chain_valid' is nonzero if the chain pointer is
          nonzero and given frame's PC is not inside the startup file
          (such as `crt0.o').

        * `func_frame_chain_valid' is nonzero if the chain pointer is
          nonzero and the given frame's PC is not in `main' or a known
          entry point function (such as `_start').

        * `generic_file_frame_chain_valid' and
          `generic_func_frame_chain_valid' are equivalent
          implementations for targets using generic dummy frames.

`FRAME_INIT_SAVED_REGS(FRAME)'
     See `frame.h'.  Determines the address of all registers in the
     current stack frame storing each in `frame->saved_regs'.  Space for
     `frame->saved_regs' shall be allocated by `FRAME_INIT_SAVED_REGS'
     using either `frame_saved_regs_zalloc' or `frame_obstack_alloc'.

     `FRAME_FIND_SAVED_REGS' and `EXTRA_FRAME_INFO' are deprecated.

`FRAME_NUM_ARGS (FI)'
     For the frame described by FI return the number of arguments that
     are being passed.  If the number of arguments is not known, return
     `-1'.

`FRAME_SAVED_PC(FRAME)'
     Given FRAME, return the pc saved there.  This is the return
     address.

`FUNCTION_EPILOGUE_SIZE'
     For some COFF targets, the `x_sym.x_misc.x_fsize' field of the
     function end symbol is 0.  For such targets, you must define
     `FUNCTION_EPILOGUE_SIZE' to expand into the standard size of a
     function's epilogue.

`FUNCTION_START_OFFSET'
     An integer, giving the offset in bytes from a function's address
     (as used in the values of symbols, function pointers, etc.), and
     the function's first genuine instruction.

     This is zero on almost all machines: the function's address is
     usually the address of its first instruction.  However, on the
     VAX, for example, each function starts with two bytes containing a
     bitmask indicating which registers to save upon entry to the
     function.  The VAX `call' instructions check this value, and save
     the appropriate registers automatically.  Thus, since the offset
     from the function's address to its first instruction is two bytes,
     `FUNCTION_START_OFFSET' would be 2 on the VAX.

`GCC_COMPILED_FLAG_SYMBOL'
`GCC2_COMPILED_FLAG_SYMBOL'
     If defined, these are the names of the symbols that GDB will look
     for to detect that GCC compiled the file.  The default symbols are
     `gcc_compiled.' and `gcc2_compiled.', respectively.  (Currently
     only defined for the Delta 68.)

`GDB_MULTI_ARCH'
     If defined and non-zero, enables support for multiple architectures
     within GDB.

     This support can be enabled at two levels.  At level one, only
     definitions for previously undefined macros are provided; at level
     two, a multi-arch definition of all architecture dependent macros
     will be defined.

`GDB_TARGET_IS_HPPA'
     This determines whether horrible kludge code in `dbxread.c' and
     `partial-stab.h' is used to mangle multiple-symbol-table files from
     HPPA's.  This should all be ripped out, and a scheme like
     `elfread.c' used instead.

`GET_LONGJMP_TARGET'
     For most machines, this is a target-dependent parameter.  On the
     DECstation and the Iris, this is a native-dependent parameter,
     since the header file `setjmp.h' is needed to define it.

     This macro determines the target PC address that `longjmp' will
     jump to, assuming that we have just stopped at a `longjmp'
     breakpoint.  It takes a `CORE_ADDR *' as argument, and stores the
     target PC value through this pointer.  It examines the current
     state of the machine as needed.

`GET_SAVED_REGISTER'
     Define this if you need to supply your own definition for the
     function `get_saved_register'.

`IBM6000_TARGET'
     Shows that we are configured for an IBM RS/6000 target.  This
     conditional should be eliminated (FIXME) and replaced by
     feature-specific macros.  It was introduced in a haste and we are
     repenting at leisure.

`I386_USE_GENERIC_WATCHPOINTS'
     An x86-based target can define this to use the generic x86
     watchpoint support; see *Note I386_USE_GENERIC_WATCHPOINTS:
     Algorithms.

`SYMBOLS_CAN_START_WITH_DOLLAR'
     Some systems have routines whose names start with `$'.  Giving this
     macro a non-zero value tells GDB's expression parser to check for
     such routines when parsing tokens that begin with `$'.

     On HP-UX, certain system routines (millicode) have names beginning
     with `$' or `$$'.  For example, `$$dyncall' is a millicode routine
     that handles inter-space procedure calls on PA-RISC.

`INIT_EXTRA_FRAME_INFO (FROMLEAF, FRAME)'
     If additional information about the frame is required this should
     be stored in `frame->extra_info'.  Space for `frame->extra_info'
     is allocated using `frame_obstack_alloc'.

`INIT_FRAME_PC (FROMLEAF, PREV)'
     This is a C statement that sets the pc of the frame pointed to by
     PREV.  [By default...]

`INNER_THAN (LHS, RHS)'
     Returns non-zero if stack address LHS is inner than (nearer to the
     stack top) stack address RHS. Define this as `lhs < rhs' if the
     target's stack grows downward in memory, or `lhs > rsh' if the
     stack grows upward.

`gdbarch_in_function_epilogue_p (GDBARCH, PC)'
     Returns non-zero if the given PC is in the epilogue of a function.
     The epilogue of a function is defined as the part of a function
     where the stack frame of the function already has been destroyed
     up to the final `return from function call' instruction.

`SIGTRAMP_START (PC)'
`SIGTRAMP_END (PC)'
     Define these to be the start and end address of the `sigtramp' for
     the given PC.  On machines where the address is just a compile time
     constant, the macro expansion will typically just ignore the
     supplied PC.

`IN_SOLIB_CALL_TRAMPOLINE (PC, NAME)'
     Define this to evaluate to nonzero if the program is stopped in the
     trampoline that connects to a shared library.

`IN_SOLIB_RETURN_TRAMPOLINE (PC, NAME)'
     Define this to evaluate to nonzero if the program is stopped in the
     trampoline that returns from a shared library.

`IN_SOLIB_DYNSYM_RESOLVE_CODE (PC)'
     Define this to evaluate to nonzero if the program is stopped in the
     dynamic linker.

`SKIP_SOLIB_RESOLVER (PC)'
     Define this to evaluate to the (nonzero) address at which execution
     should continue to get past the dynamic linker's symbol resolution
     function.  A zero value indicates that it is not important or
     necessary to set a breakpoint to get through the dynamic linker
     and that single stepping will suffice.

`INTEGER_TO_ADDRESS (TYPE, BUF)'
     Define this when the architecture needs to handle non-pointer to
     address conversions specially.  Converts that value to an address
     according to the current architectures conventions.

     _Pragmatics: When the user copies a well defined expression from
     their source code and passes it, as a parameter, to GDB's `print'
     command, they should get the same value as would have been
     computed by the target program.  Any deviation from this rule can
     cause major confusion and annoyance, and needs to be justified
     carefully.  In other words, GDB doesn't really have the freedom to
     do these conversions in clever and useful ways.  It has, however,
     been pointed out that users aren't complaining about how GDB casts
     integers to pointers; they are complaining that they can't take an
     address from a disassembly listing and give it to `x/i'.  Adding
     an architecture method like `INTEGER_TO_ADDRESS' certainly makes
     it possible for GDB to "get it right" in all circumstances._

     *Note Pointers Are Not Always Addresses: Target Architecture
     Definition.

`IS_TRAPPED_INTERNALVAR (NAME)'
     This is an ugly hook to allow the specification of special actions
     that should occur as a side-effect of setting the value of a
     variable internal to GDB.  Currently only used by the h8500.  Note
     that this could be either a host or target conditional.

`NEED_TEXT_START_END'
     Define this if GDB should determine the start and end addresses of
     the text section.  (Seems dubious.)

`NO_HIF_SUPPORT'
     (Specific to the a29k.)

`POINTER_TO_ADDRESS (TYPE, BUF)'
     Assume that BUF holds a pointer of type TYPE, in the appropriate
     format for the current architecture.  Return the byte address the
     pointer refers to.  *Note Pointers Are Not Always Addresses:
     Target Architecture Definition.

`REGISTER_CONVERTIBLE (REG)'
     Return non-zero if REG uses different raw and virtual formats.
     *Note Raw and Virtual Register Representations: Target
     Architecture Definition.

`REGISTER_TO_VALUE(REGNUM, TYPE, FROM, TO)'
     Convert the raw contents of register REGNUM into a value of type
     TYPE.  *Note Using Different Register and Memory Data
     Representations: Target Architecture Definition.

`REGISTER_RAW_SIZE (REG)'
     Return the raw size of REG; defaults to the size of the register's
     virtual type.  *Note Raw and Virtual Register Representations:
     Target Architecture Definition.

`REGISTER_VIRTUAL_SIZE (REG)'
     Return the virtual size of REG; defaults to the size of the
     register's virtual type.  Return the virtual size of REG.  *Note
     Raw and Virtual Register Representations: Target Architecture
     Definition.

`REGISTER_VIRTUAL_TYPE (REG)'
     Return the virtual type of REG.  *Note Raw and Virtual Register
     Representations: Target Architecture Definition.

`REGISTER_CONVERT_TO_VIRTUAL(REG, TYPE, FROM, TO)'
     Convert the value of register REG from its raw form to its virtual
     form.  *Note Raw and Virtual Register Representations: Target
     Architecture Definition.

`REGISTER_CONVERT_TO_RAW(TYPE, REG, FROM, TO)'
     Convert the value of register REG from its virtual form to its raw
     form.  *Note Raw and Virtual Register Representations: Target
     Architecture Definition.

`RETURN_VALUE_ON_STACK(TYPE)'
     Return non-zero if values of type TYPE are returned on the stack,
     using the "struct convention" (i.e., the caller provides a pointer
     to a buffer in which the callee should store the return value).
     This controls how the `finish' command finds a function's return
     value, and whether an inferior function call reserves space on the
     stack for the return value.

     The full logic GDB uses here is kind of odd.

        * If the type being returned by value is not a structure,
          union, or array, and `RETURN_VALUE_ON_STACK' returns zero,
          then GDB concludes the value is not returned using the struct
          convention.

        * Otherwise, GDB calls `USE_STRUCT_CONVENTION' (see below).  If
          that returns non-zero, GDB assumes the struct convention is
          in use.

     In other words, to indicate that a given type is returned by value
     using the struct convention, that type must be either a struct,
     union, array, or something `RETURN_VALUE_ON_STACK' likes, _and_
     something that `USE_STRUCT_CONVENTION' likes.

     Note that, in C and C++, arrays are never returned by value.  In
     those languages, these predicates will always see a pointer type,
     never an array type.  All the references above to arrays being
     returned by value apply only to other languages.

`SOFTWARE_SINGLE_STEP_P()'
     Define this as 1 if the target does not have a hardware single-step
     mechanism.  The macro `SOFTWARE_SINGLE_STEP' must also be defined.

`SOFTWARE_SINGLE_STEP(SIGNAL, INSERT_BREAPOINTS_P)'
     A function that inserts or removes (depending on
     INSERT_BREAPOINTS_P) breakpoints at each possible destinations of
     the next instruction. See `sparc-tdep.c' and `rs6000-tdep.c' for
     examples.

`SOFUN_ADDRESS_MAYBE_MISSING'
     Somebody clever observed that, the more actual addresses you have
     in the debug information, the more time the linker has to spend
     relocating them.  So whenever there's some other way the debugger
     could find the address it needs, you should omit it from the debug
     info, to make linking faster.

     `SOFUN_ADDRESS_MAYBE_MISSING' indicates that a particular set of
     hacks of this sort are in use, affecting `N_SO' and `N_FUN'
     entries in stabs-format debugging information.  `N_SO' stabs mark
     the beginning and ending addresses of compilation units in the text
     segment.  `N_FUN' stabs mark the starts and ends of functions.

     `SOFUN_ADDRESS_MAYBE_MISSING' means two things:

        * `N_FUN' stabs have an address of zero.  Instead, you should
          find the addresses where the function starts by taking the
          function name from the stab, and then looking that up in the
          minsyms (the linker/assembler symbol table).  In other words,
          the stab has the name, and the linker/assembler symbol table
          is the only place that carries the address.

        * `N_SO' stabs have an address of zero, too.  You just look at
          the `N_FUN' stabs that appear before and after the `N_SO'
          stab, and guess the starting and ending addresses of the
          compilation unit from them.

`PCC_SOL_BROKEN'
     (Used only in the Convex target.)

`PC_IN_CALL_DUMMY'
     See `inferior.h'.

`PC_IN_SIGTRAMP (PC, NAME)'
     The "sigtramp" is a routine that the kernel calls (which then calls
     the signal handler).  On most machines it is a library routine
     that is linked into the executable.

     This function, given a program counter value in PC and the
     (possibly NULL) name of the function in which that PC resides,
     returns nonzero if the PC and/or NAME show that we are in sigtramp.

`PC_LOAD_SEGMENT'
     If defined, print information about the load segment for the
     program counter.  (Defined only for the RS/6000.)

`PC_REGNUM'
     If the program counter is kept in a register, then define this
     macro to be the number (greater than or equal to zero) of that
     register.

     This should only need to be defined if `TARGET_READ_PC' and
     `TARGET_WRITE_PC' are not defined.

`NPC_REGNUM'
     The number of the "next program counter" register, if defined.

`PARM_BOUNDARY'
     If non-zero, round arguments to a boundary of this many bits before
     pushing them on the stack.

`PRINT_REGISTER_HOOK (REGNO)'
     If defined, this must be a function that prints the contents of the
     given register to standard output.

`PRINT_TYPELESS_INTEGER'
     This is an obscure substitute for `print_longest' that seems to
     have been defined for the Convex target.

`PROCESS_LINENUMBER_HOOK'
     A hook defined for XCOFF reading.

`PROLOGUE_FIRSTLINE_OVERLAP'
     (Only used in unsupported Convex configuration.)

`PS_REGNUM'
     If defined, this is the number of the processor status register.
     (This definition is only used in generic code when parsing "$ps".)

`POP_FRAME'
     Used in `call_function_by_hand' to remove an artificial stack
     frame and in `return_command' to remove a real stack frame.

`PUSH_ARGUMENTS (NARGS, ARGS, SP, STRUCT_RETURN, STRUCT_ADDR)'
     Define this to push arguments onto the stack for inferior function
     call.  Returns the updated stack pointer value.

`PUSH_DUMMY_FRAME'
     Used in `call_function_by_hand' to create an artificial stack
     frame.

`REGISTER_BYTES'
     The total amount of space needed to store GDB's copy of the
     machine's register state.

`REGISTER_NAME(I)'
     Return the name of register I as a string.  May return `NULL' or
     `NUL' to indicate that register I is not valid.

`REGISTER_NAMES'
     Deprecated in favor of `REGISTER_NAME'.

`REG_STRUCT_HAS_ADDR (GCC_P, TYPE)'
     Define this to return 1 if the given type will be passed by pointer
     rather than directly.

`SAVE_DUMMY_FRAME_TOS (SP)'
     Used in `call_function_by_hand' to notify the target dependent code
     of the top-of-stack value that will be passed to the the inferior
     code.  This is the value of the `SP' after both the dummy frame
     and space for parameters/results have been allocated on the stack.

`SDB_REG_TO_REGNUM'
     Define this to convert sdb register numbers into GDB regnums.  If
     not defined, no conversion will be done.

`SKIP_PERMANENT_BREAKPOINT'
     Advance the inferior's PC past a permanent breakpoint.  GDB
     normally steps over a breakpoint by removing it, stepping one
     instruction, and re-inserting the breakpoint.  However, permanent
     breakpoints are hardwired into the inferior, and can't be removed,
     so this strategy doesn't work.  Calling
     `SKIP_PERMANENT_BREAKPOINT' adjusts the processor's state so that
     execution will resume just after the breakpoint.  This macro does
     the right thing even when the breakpoint is in the delay slot of a
     branch or jump.

`SKIP_PROLOGUE (PC)'
     A C expression that returns the address of the "real" code beyond
     the function entry prologue found at PC.

`SKIP_TRAMPOLINE_CODE (PC)'
     If the target machine has trampoline code that sits between
     callers and the functions being called, then define this macro to
     return a new PC that is at the start of the real function.

`SP_REGNUM'
     If the stack-pointer is kept in a register, then define this macro
     to be the number (greater than or equal to zero) of that register.

     This should only need to be defined if `TARGET_WRITE_SP' and
     `TARGET_WRITE_SP' are not defined.

`STAB_REG_TO_REGNUM'
     Define this to convert stab register numbers (as gotten from `r'
     declarations) into GDB regnums.  If not defined, no conversion
     will be done.

`STACK_ALIGN (ADDR)'
     Define this to adjust the address to the alignment required for the
     processor's stack.

`STEP_SKIPS_DELAY (ADDR)'
     Define this to return true if the address is of an instruction
     with a delay slot.  If a breakpoint has been placed in the
     instruction's delay slot, GDB will single-step over that
     instruction before resuming normally.  Currently only defined for
     the Mips.

`STORE_RETURN_VALUE (TYPE, REGCACHE, VALBUF)'
     A C expression that writes the function return value, found in
     VALBUF, into the REGCACHE.  TYPE is the type of the value that is
     to be returned.

`SUN_FIXED_LBRAC_BUG'
     (Used only for Sun-3 and Sun-4 targets.)

`SYMBOL_RELOADING_DEFAULT'
     The default value of the "symbol-reloading" variable.  (Never
     defined in current sources.)

`TARGET_CHAR_BIT'
     Number of bits in a char; defaults to 8.

`TARGET_CHAR_SIGNED'
     Non-zero if `char' is normally signed on this architecture; zero if
     it should be unsigned.

     The ISO C standard requires the compiler to treat `char' as
     equivalent to either `signed char' or `unsigned char'; any
     character in the standard execution set is supposed to be positive.
     Most compilers treat `char' as signed, but `char' is unsigned on
     the IBM S/390, RS6000, and PowerPC targets.

`TARGET_COMPLEX_BIT'
     Number of bits in a complex number; defaults to `2 *
     TARGET_FLOAT_BIT'.

     At present this macro is not used.

`TARGET_DOUBLE_BIT'
     Number of bits in a double float; defaults to `8 *
     TARGET_CHAR_BIT'.

`TARGET_DOUBLE_COMPLEX_BIT'
     Number of bits in a double complex; defaults to `2 *
     TARGET_DOUBLE_BIT'.

     At present this macro is not used.

`TARGET_FLOAT_BIT'
     Number of bits in a float; defaults to `4 * TARGET_CHAR_BIT'.

`TARGET_INT_BIT'
     Number of bits in an integer; defaults to `4 * TARGET_CHAR_BIT'.

`TARGET_LONG_BIT'
     Number of bits in a long integer; defaults to `4 *
     TARGET_CHAR_BIT'.

`TARGET_LONG_DOUBLE_BIT'
     Number of bits in a long double float; defaults to `2 *
     TARGET_DOUBLE_BIT'.

`TARGET_LONG_LONG_BIT'
     Number of bits in a long long integer; defaults to `2 *
     TARGET_LONG_BIT'.

`TARGET_PTR_BIT'
     Number of bits in a pointer; defaults to `TARGET_INT_BIT'.

`TARGET_SHORT_BIT'
     Number of bits in a short integer; defaults to `2 *
     TARGET_CHAR_BIT'.

`TARGET_READ_PC'
`TARGET_WRITE_PC (VAL, PID)'
`TARGET_READ_SP'
`TARGET_WRITE_SP'
`TARGET_READ_FP'
     These change the behavior of `read_pc', `write_pc', `read_sp',
     `write_sp' and `read_fp'.  For most targets, these may be left
     undefined.  GDB will call the read and write register functions
     with the relevant `_REGNUM' argument.

     These macros are useful when a target keeps one of these registers
     in a hard to get at place; for example, part in a segment register
     and part in an ordinary register.

`TARGET_VIRTUAL_FRAME_POINTER(PC, REGP, OFFSETP)'
     Returns a `(register, offset)' pair representing the virtual frame
     pointer in use at the code address PC.  If virtual frame pointers
     are not used, a default definition simply returns `FP_REGNUM',
     with an offset of zero.

`TARGET_HAS_HARDWARE_WATCHPOINTS'
     If non-zero, the target has support for hardware-assisted
     watchpoints.  *Note watchpoints: Algorithms, for more details and
     other related macros.

`TARGET_PRINT_INSN (ADDR, INFO)'
     This is the function used by GDB to print an assembly instruction.
     It prints the instruction at address ADDR in debugged memory and
     returns the length of the instruction, in bytes.  If a target
     doesn't define its own printing routine, it defaults to an
     accessor function for the global pointer `tm_print_insn'. This
     usually points to a function in the `opcodes' library (*note
     Opcodes: Support Libraries.).  INFO is a structure (of type
     `disassemble_info') defined in `include/dis-asm.h' used to pass
     information to the instruction decoding routine.

`USE_STRUCT_CONVENTION (GCC_P, TYPE)'
     If defined, this must be an expression that is nonzero if a value
     of the given TYPE being returned from a function must have space
     allocated for it on the stack.  GCC_P is true if the function
     being considered is known to have been compiled by GCC; this is
     helpful for systems where GCC is known to use different calling
     convention than other compilers.

`VALUE_TO_REGISTER(TYPE, REGNUM, FROM, TO)'
     Convert a value of type TYPE into the raw contents of register
     REGNUM's.  *Note Using Different Register and Memory Data
     Representations: Target Architecture Definition.

`VARIABLES_INSIDE_BLOCK (DESC, GCC_P)'
     For dbx-style debugging information, if the compiler puts variable
     declarations inside LBRAC/RBRAC blocks, this should be defined to
     be nonzero.  DESC is the value of `n_desc' from the `N_RBRAC'
     symbol, and GCC_P is true if GDB has noticed the presence of
     either the `GCC_COMPILED_SYMBOL' or the `GCC2_COMPILED_SYMBOL'.
     By default, this is 0.

`OS9K_VARIABLES_INSIDE_BLOCK (DESC, GCC_P)'
     Similarly, for OS/9000.  Defaults to 1.

   Motorola M68K target conditionals.

`BPT_VECTOR'
     Define this to be the 4-bit location of the breakpoint trap
     vector.  If not defined, it will default to `0xf'.

`REMOTE_BPT_VECTOR'
     Defaults to `1'.

Adding a New Target
===================

   The following files add a target to GDB:

`gdb/config/ARCH/TTT.mt'
     Contains a Makefile fragment specific to this target.  Specifies
     what object files are needed for target TTT, by defining
     `TDEPFILES=...' and `TDEPLIBS=...'.  Also specifies the header
     file which describes TTT, by defining `TM_FILE= tm-TTT.h'.

     You can also define `TM_CFLAGS', `TM_CLIBS', `TM_CDEPS', but these
     are now deprecated, replaced by autoconf, and may go away in
     future versions of GDB.

`gdb/TTT-tdep.c'
     Contains any miscellaneous code required for this target machine.
     On some machines it doesn't exist at all.  Sometimes the macros in
     `tm-TTT.h' become very complicated, so they are implemented as
     functions here instead, and the macro is simply defined to call the
     function.  This is vastly preferable, since it is easier to
     understand and debug.

`gdb/ARCH-tdep.c'
`gdb/ARCH-tdep.h'
     This often exists to describe the basic layout of the target
     machine's processor chip (registers, stack, etc.).  If used, it is
     included by `TTT-tdep.h'.  It can be shared among many targets
     that use the same processor.

`gdb/config/ARCH/tm-TTT.h'
     (`tm.h' is a link to this file, created by `configure').  Contains
     macro definitions about the target machine's registers, stack frame
     format and instructions.

     New targets do not need this file and should not create it.

`gdb/config/ARCH/tm-ARCH.h'
     This often exists to describe the basic layout of the target
     machine's processor chip (registers, stack, etc.).  If used, it is
     included by `tm-TTT.h'.  It can be shared among many targets that
     use the same processor.

     New targets do not need this file and should not create it.

   If you are adding a new operating system for an existing CPU chip,
add a `config/tm-OS.h' file that describes the operating system
facilities that are unusual (extra symbol table info; the breakpoint
instruction needed; etc.).  Then write a `ARCH/tm-OS.h' that just
`#include's `tm-ARCH.h' and `config/tm-OS.h'.

Converting an existing Target Architecture to Multi-arch
========================================================

   This section describes the current accepted best practice for
converting an existing target architecture to the multi-arch framework.

   The process consists of generating, testing, posting and committing a
sequence of patches.  Each patch must contain a single change, for
instance:

   * Directly convert a group of functions into macros (the conversion
     does not change the behavior of any of the functions).

   * Replace a non-multi-arch with a multi-arch mechanism (e.g.,
     `FRAME_INFO').

   * Enable multi-arch level one.

   * Delete one or more files.


There isn't a size limit on a patch, however, a developer is strongly
encouraged to keep the patch size down.

   Since each patch is well defined, and since each change has been
tested and shows no regressions, the patches are considered _fairly_
obvious.  Such patches, when submitted by developers listed in the
`MAINTAINERS' file, do not need approval.  Occasional steps in the
process may be more complicated and less clear.  The developer is
expected to use their judgment and is encouraged to seek advice as
needed.

Preparation
-----------

   The first step is to establish control.  Build (with `-Werror'
enabled) and test the target so that there is a baseline against which
the debugger can be compared.

   At no stage can the test results regress or GDB stop compiling with
`-Werror'.

Add the multi-arch initialization code
--------------------------------------

   The objective of this step is to establish the basic multi-arch
framework.  It involves

   * The addition of a `ARCH_gdbarch_init' function(2) that creates the
     architecture:
          static struct gdbarch *
          d10v_gdbarch_init (info, arches)
               struct gdbarch_info info;
               struct gdbarch_list *arches;
          {
            struct gdbarch *gdbarch;
            /* there is only one d10v architecture */
            if (arches != NULL)
              return arches->gdbarch;
            gdbarch = gdbarch_alloc (&info, NULL);
            return gdbarch;
          }

     __

   * A per-architecture dump function to print any architecture specific
     information:
          static void
          mips_dump_tdep (struct gdbarch *current_gdbarch,
                          struct ui_file *file)
          {
             ... code to print architecture specific info ...
          }

   * A change to `_initialize_ARCH_tdep' to register this new
     architecture:
          void
          _initialize_mips_tdep (void)
          {
            gdbarch_register (bfd_arch_mips, mips_gdbarch_init,
                              mips_dump_tdep);

   * Add the macro `GDB_MULTI_ARCH', defined as 0 (zero), to the file
     `config/ARCH/tm-ARCH.h'.


Update multi-arch incompatible mechanisms
-----------------------------------------

   Some mechanisms do not work with multi-arch.  They include:

`EXTRA_FRAME_INFO'
     Delete.

`FRAME_FIND_SAVED_REGS'
     Replaced with `FRAME_INIT_SAVED_REGS'

At this stage you could also consider converting the macros into
functions.

Prepare for multi-arch level to one
-----------------------------------

   Temporally set `GDB_MULTI_ARCH' to `GDB_MULTI_ARCH_PARTIAL' and then
build and start GDB (the change should not be committed).  GDB may not
build, and once built, it may die with an internal error listing the
architecture methods that must be provided.

   Fix any build problems (patch(es)).

   Convert all the architecture methods listed, which are only macros,
into functions (patch(es)).

   Update `ARCH_gdbarch_init' to set all the missing architecture
methods and wrap the corresponding macros in `#if !GDB_MULTI_ARCH'
(patch(es)).

Set multi-arch level one
------------------------

   Change the value of `GDB_MULTI_ARCH' to GDB_MULTI_ARCH_PARTIAL (a
single patch).

   Any problems with throwing "the switch" should have been fixed
already.

Convert remaining macros
------------------------

   Suggest converting macros into functions (and setting the
corresponding architecture method) in small batches.

Set multi-arch level to two
---------------------------

   This should go smoothly.

Delete the TM file
------------------

   The `tm-ARCH.h' can be deleted.  `ARCH.mt' and `configure.in'
updated.

   ---------- Footnotes ----------

   (1) Some D10V instructions are actually pairs of 16-bit
sub-instructions.  However, since you can't jump into the middle of
such a pair, code addresses can only refer to full 32 bit instructions,
which is what matters in this explanation.

   (2) The above is from the original example and uses K&R C.  GDB has
since converted to ISO C but lets ignore that.


File: gdbint.info,  Node: Target Vector Definition,  Next: Native Debugging,  Prev: Target Architecture Definition,  Up: Top

Target Vector Definition
************************

   The target vector defines the interface between GDB's abstract
handling of target systems, and the nitty-gritty code that actually
exercises control over a process or a serial port.  GDB includes some
30-40 different target vectors; however, each configuration of GDB
includes only a few of them.

File Targets
============

   Both executables and core files have target vectors.

Standard Protocol and Remote Stubs
==================================

   GDB's file `remote.c' talks a serial protocol to code that runs in
the target system.  GDB provides several sample "stubs" that can be
integrated into target programs or operating systems for this purpose;
they are named `*-stub.c'.

   The GDB user's manual describes how to put such a stub into your
target code.  What follows is a discussion of integrating the SPARC
stub into a complicated operating system (rather than a simple
program), by Stu Grossman, the author of this stub.

   The trap handling code in the stub assumes the following upon entry
to `trap_low':

  1. %l1 and %l2 contain pc and npc respectively at the time of the
     trap;

  2. traps are disabled;

  3. you are in the correct trap window.

   As long as your trap handler can guarantee those conditions, then
there is no reason why you shouldn't be able to "share" traps with the
stub.  The stub has no requirement that it be jumped to directly from
the hardware trap vector.  That is why it calls `exceptionHandler()',
which is provided by the external environment.  For instance, this could
set up the hardware traps to actually execute code which calls the stub
first, and then transfers to its own trap handler.

   For the most point, there probably won't be much of an issue with
"sharing" traps, as the traps we use are usually not used by the kernel,
and often indicate unrecoverable error conditions.  Anyway, this is all
controlled by a table, and is trivial to modify.  The most important
trap for us is for `ta 1'.  Without that, we can't single step or do
breakpoints.  Everything else is unnecessary for the proper operation
of the debugger/stub.

   From reading the stub, it's probably not obvious how breakpoints
work.  They are simply done by deposit/examine operations from GDB.

ROM Monitor Interface
=====================

Custom Protocols
================

Transport Layer
===============

Builtin Simulator
=================


File: gdbint.info,  Node: Native Debugging,  Next: Support Libraries,  Prev: Target Vector Definition,  Up: Top

Native Debugging
****************

   Several files control GDB's configuration for native support:

`gdb/config/ARCH/XYZ.mh'
     Specifies Makefile fragments needed by a _native_ configuration on
     machine XYZ.  In particular, this lists the required
     native-dependent object files, by defining `NATDEPFILES=...'.
     Also specifies the header file which describes native support on
     XYZ, by defining `NAT_FILE= nm-XYZ.h'.  You can also define
     `NAT_CFLAGS', `NAT_ADD_FILES', `NAT_CLIBS', `NAT_CDEPS', etc.; see
     `Makefile.in'.

     _Maintainer's note: The `.mh' suffix is because this file
     originally contained `Makefile' fragments for hosting GDB on
     machine XYZ.  While the file is no longer used for this purpose,
     the `.mh' suffix remains.  Perhaps someone will eventually rename
     these fragments so that they have a `.mn' suffix._

`gdb/config/ARCH/nm-XYZ.h'
     (`nm.h' is a link to this file, created by `configure').  Contains
     C macro definitions describing the native system environment, such
     as child process control and core file support.

`gdb/XYZ-nat.c'
     Contains any miscellaneous C code required for this native support
     of this machine.  On some machines it doesn't exist at all.

   There are some "generic" versions of routines that can be used by
various systems.  These can be customized in various ways by macros
defined in your `nm-XYZ.h' file.  If these routines work for the XYZ
host, you can just include the generic file's name (with `.o', not
`.c') in `NATDEPFILES'.

   Otherwise, if your machine needs custom support routines, you will
need to write routines that perform the same functions as the generic
file.  Put them into `XYZ-nat.c', and put `XYZ-nat.o' into
`NATDEPFILES'.

`inftarg.c'
     This contains the _target_ops vector_ that supports Unix child
     processes on systems which use ptrace and wait to control the
     child.

`procfs.c'
     This contains the _target_ops vector_ that supports Unix child
     processes on systems which use /proc to control the child.

`fork-child.c'
     This does the low-level grunge that uses Unix system calls to do a
     "fork and exec" to start up a child process.

`infptrace.c'
     This is the low level interface to inferior processes for systems
     using the Unix `ptrace' call in a vanilla way.

Native core file Support
========================

`core-aout.c::fetch_core_registers()'
     Support for reading registers out of a core file.  This routine
     calls `register_addr()', see below.  Now that BFD is used to read
     core files, virtually all machines should use `core-aout.c', and
     should just provide `fetch_core_registers' in `XYZ-nat.c' (or
     `REGISTER_U_ADDR' in `nm-XYZ.h').

`core-aout.c::register_addr()'
     If your `nm-XYZ.h' file defines the macro `REGISTER_U_ADDR(addr,
     blockend, regno)', it should be defined to set `addr' to the
     offset within the `user' struct of GDB register number `regno'.
     `blockend' is the offset within the "upage" of `u.u_ar0'.  If
     `REGISTER_U_ADDR' is defined, `core-aout.c' will define the
     `register_addr()' function and use the macro in it.  If you do not
     define `REGISTER_U_ADDR', but you are using the standard
     `fetch_core_registers()', you will need to define your own version
     of `register_addr()', put it into your `XYZ-nat.c' file, and be
     sure `XYZ-nat.o' is in the `NATDEPFILES' list.  If you have your
     own `fetch_core_registers()', you may not need a separate
     `register_addr()'.  Many custom `fetch_core_registers()'
     implementations simply locate the registers themselves.

   When making GDB run native on a new operating system, to make it
possible to debug core files, you will need to either write specific
code for parsing your OS's core files, or customize `bfd/trad-core.c'.
First, use whatever `#include' files your machine uses to define the
struct of registers that is accessible (possibly in the u-area) in a
core file (rather than `machine/reg.h'), and an include file that
defines whatever header exists on a core file (e.g. the u-area or a
`struct core').  Then modify `trad_unix_core_file_p' to use these
values to set up the section information for the data segment, stack
segment, any other segments in the core file (perhaps shared library
contents or control information), "registers" segment, and if there are
two discontiguous sets of registers (e.g.  integer and float), the
"reg2" segment.  This section information basically delimits areas in
the core file in a standard way, which the section-reading routines in
BFD know how to seek around in.

   Then back in GDB, you need a matching routine called
`fetch_core_registers'.  If you can use the generic one, it's in
`core-aout.c'; if not, it's in your `XYZ-nat.c' file.  It will be
passed a char pointer to the entire "registers" segment, its length,
and a zero; or a char pointer to the entire "regs2" segment, its
length, and a 2.  The routine should suck out the supplied register
values and install them into GDB's "registers" array.

   If your system uses `/proc' to control processes, and uses ELF
format core files, then you may be able to use the same routines for
reading the registers out of processes and out of core files.

ptrace
======

/proc
=====

win32
=====

shared libraries
================

Native Conditionals
===================

   When GDB is configured and compiled, various macros are defined or
left undefined, to control compilation when the host and target systems
are the same.  These macros should be defined (or left undefined) in
`nm-SYSTEM.h'.

`ATTACH_DETACH'
     If defined, then GDB will include support for the `attach' and
     `detach' commands.

`CHILD_PREPARE_TO_STORE'
     If the machine stores all registers at once in the child process,
     then define this to ensure that all values are correct.  This
     usually entails a read from the child.

     [Note that this is incorrectly defined in `xm-SYSTEM.h' files
     currently.]

`FETCH_INFERIOR_REGISTERS'
     Define this if the native-dependent code will provide its own
     routines `fetch_inferior_registers' and `store_inferior_registers'
     in `HOST-nat.c'.  If this symbol is _not_ defined, and
     `infptrace.c' is included in this configuration, the default
     routines in `infptrace.c' are used for these functions.

`FILES_INFO_HOOK'
     (Only defined for Convex.)

`FP0_REGNUM'
     This macro is normally defined to be the number of the first
     floating point register, if the machine has such registers.  As
     such, it would appear only in target-specific code.  However,
     `/proc' support uses this to decide whether floats are in use on
     this target.

`GET_LONGJMP_TARGET'
     For most machines, this is a target-dependent parameter.  On the
     DECstation and the Iris, this is a native-dependent parameter,
     since `setjmp.h' is needed to define it.

     This macro determines the target PC address that `longjmp' will
     jump to, assuming that we have just stopped at a longjmp
     breakpoint.  It takes a `CORE_ADDR *' as argument, and stores the
     target PC value through this pointer.  It examines the current
     state of the machine as needed.

`I386_USE_GENERIC_WATCHPOINTS'
     An x86-based machine can define this to use the generic x86
     watchpoint support; see *Note I386_USE_GENERIC_WATCHPOINTS:
     Algorithms.

`KERNEL_U_ADDR'
     Define this to the address of the `u' structure (the "user
     struct", also known as the "u-page") in kernel virtual memory.
     GDB needs to know this so that it can subtract this address from
     absolute addresses in the upage, that are obtained via ptrace or
     from core files.  On systems that don't need this value, set it to
     zero.

`KERNEL_U_ADDR_BSD'
     Define this to cause GDB to determine the address of `u' at
     runtime, by using Berkeley-style `nlist' on the kernel's image in
     the root directory.

`KERNEL_U_ADDR_HPUX'
     Define this to cause GDB to determine the address of `u' at
     runtime, by using HP-style `nlist' on the kernel's image in the
     root directory.

`ONE_PROCESS_WRITETEXT'
     Define this to be able to, when a breakpoint insertion fails, warn
     the user that another process may be running with the same
     executable.

`PREPARE_TO_PROCEED (SELECT_IT)'
     This (ugly) macro allows a native configuration to customize the
     way the `proceed' function in `infrun.c' deals with switching
     between threads.

     In a multi-threaded task we may select another thread and then
     continue or step.  But if the old thread was stopped at a
     breakpoint, it will immediately cause another breakpoint stop
     without any execution (i.e. it will report a breakpoint hit
     incorrectly).  So GDB must step over it first.

     If defined, `PREPARE_TO_PROCEED' should check the current thread
     against the thread that reported the most recent event.  If a
     step-over is required, it returns TRUE.  If SELECT_IT is non-zero,
     it should reselect the old thread.

`PROC_NAME_FMT'
     Defines the format for the name of a `/proc' device.  Should be
     defined in `nm.h' _only_ in order to override the default
     definition in `procfs.c'.

`PTRACE_FP_BUG'
     See `mach386-xdep.c'.

`PTRACE_ARG3_TYPE'
     The type of the third argument to the `ptrace' system call, if it
     exists and is different from `int'.

`REGISTER_U_ADDR'
     Defines the offset of the registers in the "u area".

`SHELL_COMMAND_CONCAT'
     If defined, is a string to prefix on the shell command used to
     start the inferior.

`SHELL_FILE'
     If defined, this is the name of the shell to use to run the
     inferior.  Defaults to `"/bin/sh"'.

`SOLIB_ADD (FILENAME, FROM_TTY, TARG, READSYMS)'
     Define this to expand into an expression that will cause the
     symbols in FILENAME to be added to GDB's symbol table. If READSYMS
     is zero symbols are not read but any necessary low level
     processing for FILENAME is still done.

`SOLIB_CREATE_INFERIOR_HOOK'
     Define this to expand into any shared-library-relocation code that
     you want to be run just after the child process has been forked.

`START_INFERIOR_TRAPS_EXPECTED'
     When starting an inferior, GDB normally expects to trap twice;
     once when the shell execs, and once when the program itself execs.
     If the actual number of traps is something other than 2, then
     define this macro to expand into the number expected.

`SVR4_SHARED_LIBS'
     Define this to indicate that SVR4-style shared libraries are in
     use.

`USE_PROC_FS'
     This determines whether small routines in `*-tdep.c', which
     translate register values between GDB's internal representation
     and the `/proc' representation, are compiled.

`U_REGS_OFFSET'
     This is the offset of the registers in the upage.  It need only be
     defined if the generic ptrace register access routines in
     `infptrace.c' are being used (that is, `infptrace.c' is configured
     in, and `FETCH_INFERIOR_REGISTERS' is not defined).  If the
     default value from `infptrace.c' is good enough, leave it
     undefined.

     The default value means that u.u_ar0 _points to_ the location of
     the registers.  I'm guessing that `#define U_REGS_OFFSET 0' means
     that `u.u_ar0' _is_ the location of the registers.

`CLEAR_SOLIB'
     See `objfiles.c'.

`DEBUG_PTRACE'
     Define this to debug `ptrace' calls.


File: gdbint.info,  Node: Support Libraries,  Next: Coding,  Prev: Native Debugging,  Up: Top

Support Libraries
*****************

BFD
===

   BFD provides support for GDB in several ways:

_identifying executable and core files_
     BFD will identify a variety of file types, including a.out, coff,
     and several variants thereof, as well as several kinds of core
     files.

_access to sections of files_
     BFD parses the file headers to determine the names, virtual
     addresses, sizes, and file locations of all the various named
     sections in files (such as the text section or the data section).
     GDB simply calls BFD to read or write section X at byte offset Y
     for length Z.

_specialized core file support_
     BFD provides routines to determine the failing command name stored
     in a core file, the signal with which the program failed, and
     whether a core file matches (i.e. could be a core dump of) a
     particular executable file.

_locating the symbol information_
     GDB uses an internal interface of BFD to determine where to find
     the symbol information in an executable file or symbol-file.  GDB
     itself handles the reading of symbols, since BFD does not
     "understand" debug symbols, but GDB uses BFD's cached information
     to find the symbols, string table, etc.

opcodes
=======

   The opcodes library provides GDB's disassembler.  (It's a separate
library because it's also used in binutils, for `objdump').

readline
========

mmalloc
=======

libiberty
=========

gnu-regex
=========

   Regex conditionals.

`C_ALLOCA'

`NFAILURES'

`RE_NREGS'

`SIGN_EXTEND_CHAR'

`SWITCH_ENUM_BUG'

`SYNTAX_TABLE'

`Sword'

`sparc'
include
=======


File: gdbint.info,  Node: Coding,  Next: Porting GDB,  Prev: Support Libraries,  Up: Top

Coding
******

   This chapter covers topics that are lower-level than the major
algorithms of GDB.

Cleanups
========

   Cleanups are a structured way to deal with things that need to be
done later.

   When your code does something (e.g., `xmalloc' some memory, or
`open' a file) that needs to be undone later (e.g., `xfree' the memory
or `close' the file), it can make a cleanup.  The cleanup will be done
at some future point: when the command is finished and control returns
to the top level; when an error occurs and the stack is unwound; or
when your code decides it's time to explicitly perform cleanups.
Alternatively you can elect to discard the cleanups you created.

   Syntax:

`struct cleanup *OLD_CHAIN;'
     Declare a variable which will hold a cleanup chain handle.

`OLD_CHAIN = make_cleanup (FUNCTION, ARG);'
     Make a cleanup which will cause FUNCTION to be called with ARG (a
     `char *') later.  The result, OLD_CHAIN, is a handle that can
     later be passed to `do_cleanups' or `discard_cleanups'.  Unless
     you are going to call `do_cleanups' or `discard_cleanups', you can
     ignore the result from `make_cleanup'.

`do_cleanups (OLD_CHAIN);'
     Do all cleanups added to the chain since the corresponding
     `make_cleanup' call was made.

`discard_cleanups (OLD_CHAIN);'
     Same as `do_cleanups' except that it just removes the cleanups from
     the chain and does not call the specified functions.

   Cleanups are implemented as a chain.  The handle returned by
`make_cleanups' includes the cleanup passed to the call and any later
cleanups appended to the chain (but not yet discarded or performed).
E.g.:

     make_cleanup (a, 0);
     {
       struct cleanup *old = make_cleanup (b, 0);
       make_cleanup (c, 0)
       ...
       do_cleanups (old);
     }

will call `c()' and `b()' but will not call `a()'.  The cleanup that
calls `a()' will remain in the cleanup chain, and will be done later
unless otherwise discarded.

   Your function should explicitly do or discard the cleanups it
creates.  Failing to do this leads to non-deterministic behavior since
the caller will arbitrarily do or discard your functions cleanups.
This need leads to two common cleanup styles.

   The first style is try/finally.  Before it exits, your code-block
calls `do_cleanups' with the old cleanup chain and thus ensures that
your code-block's cleanups are always performed.  For instance, the
following code-segment avoids a memory leak problem (even when `error'
is called and a forced stack unwind occurs) by ensuring that the
`xfree' will always be called:

     struct cleanup *old = make_cleanup (null_cleanup, 0);
     data = xmalloc (sizeof blah);
     make_cleanup (xfree, data);
     ... blah blah ...
     do_cleanups (old);

   The second style is try/except.  Before it exits, your code-block
calls `discard_cleanups' with the old cleanup chain and thus ensures
that any created cleanups are not performed.  For instance, the
following code segment, ensures that the file will be closed but only
if there is an error:

     FILE *file = fopen ("afile", "r");
     struct cleanup *old = make_cleanup (close_file, file);
     ... blah blah ...
     discard_cleanups (old);
     return file;

   Some functions, e.g. `fputs_filtered()' or `error()', specify that
they "should not be called when cleanups are not in place".  This means
that any actions you need to reverse in the case of an error or
interruption must be on the cleanup chain before you call these
functions, since they might never return to your code (they `longjmp'
instead).

Per-architecture module data
============================

   The multi-arch framework includes a mechanism for adding module
specific per-architecture data-pointers to the `struct gdbarch'
architecture object.

   A module registers one or more per-architecture data-pointers using
the function `register_gdbarch_data':

 - Function: struct gdbarch_data *register_gdbarch_data
          (gdbarch_data_init_ftype *INIT, gdbarch_data_free_ftype *FREE)
     The INIT function is used to obtain an initial value for a
     per-architecture data-pointer.  The function is called, after the
     architecture has been created, when the data-pointer is still
     uninitialized (`NULL') and its value has been requested via a call
     to `gdbarch_data'.  A data-pointer can also be initialize
     explicitly using `set_gdbarch_data'.

     The FREE function is called when a data-pointer needs to be
     destroyed.  This occurs when either the corresponding `struct
     gdbarch' object is being destroyed or when `set_gdbarch_data' is
     overriding a non-`NULL' data-pointer value.

     The function `register_gdbarch_data' returns a `struct
     gdbarch_data' that is used to identify the data-pointer that was
     added to the module.


   A typical module has `init' and `free' functions of the form:

     static struct gdbarch_data *nozel_handle;
     static void *
     nozel_init (struct gdbarch *gdbarch)
     {
       struct nozel *data = XMALLOC (struct nozel);
       ...
       return data;
     }
     ...
     static void
     nozel_free (struct gdbarch *gdbarch, void *data)
     {
       xfree (data);
     }

   Since uninitialized (`NULL') data-pointers are initialized
on-demand, an `init' function is free to call other modules that use
data-pointers.  Those modules data-pointers will be initialized as
needed.  Care should be taken to ensure that the `init' call graph does
not contain cycles.

   The data-pointer is registered with the call:

     void
     _initialize_nozel (void)
     {
       nozel_handle = register_gdbarch_data (nozel_init, nozel_free);
     ...

   The per-architecture data-pointer is accessed using the function:

 - Function: void *gdbarch_data (struct gdbarch *GDBARCH, struct
          gdbarch_data *DATA_HANDLE)
     Given the architecture ARCH and module data handle DATA_HANDLE
     (returned by `register_gdbarch_data', this function returns the
     current value of the per-architecture data-pointer.

   The non-`NULL' data-pointer returned by `gdbarch_data' should be
saved in a local variable and then used directly:

     int
     nozel_total (struct gdbarch *gdbarch)
     {
       int total;
       struct nozel *data = gdbarch_data (gdbarch, nozel_handle);
       ...
       return total;
     }

   It is also possible to directly initialize the data-pointer using:

 - Function: void set_gdbarch_data (struct gdbarch *GDBARCH, struct
          gdbarch_data *handle, void *POINTER)
     Update the data-pointer corresponding to HANDLE with the value of
     POINTER.  If the previous data-pointer value is non-NULL, then it
     is freed using data-pointers FREE function.

   This function is used by modules that require a mechanism for
explicitly setting the per-architecture data-pointer during
architecture creation:

     /* Called during architecture creation.  */
     extern void
     set_gdbarch_nozel (struct gdbarch *gdbarch,
                        int total)
     {
       struct nozel *data = XMALLOC (struct nozel);
       ...
       set_gdbarch_data (gdbarch, nozel_handle, nozel);
     }

     /* Default, called when nozel not set by set_gdbarch_nozel().  */
     static void *
     nozel_init (struct gdbarch *gdbarch)
     {
       struct nozel *default_nozel = XMALLOC (struc nozel);
       ...
       return default_nozel;
     }

     void
     _initialize_nozel (void)
     {
       nozel_handle = register_gdbarch_data (nozel_init, NULL);
       ...

Note that an `init' function still needs to be registered.  It is used
to initialize the data-pointer when the architecture creation phase
fail to set an initial value.

Wrapping Output Lines
=====================

   Output that goes through `printf_filtered' or `fputs_filtered' or
`fputs_demangled' needs only to have calls to `wrap_here' added in
places that would be good breaking points.  The utility routines will
take care of actually wrapping if the line width is exceeded.

   The argument to `wrap_here' is an indentation string which is
printed _only_ if the line breaks there.  This argument is saved away
and used later.  It must remain valid until the next call to
`wrap_here' or until a newline has been printed through the
`*_filtered' functions.  Don't pass in a local variable and then return!

   It is usually best to call `wrap_here' after printing a comma or
space.  If you call it before printing a space, make sure that your
indentation properly accounts for the leading space that will print if
the line wraps there.

   Any function or set of functions that produce filtered output must
finish by printing a newline, to flush the wrap buffer, before switching
to unfiltered (`printf') output.  Symbol reading routines that print
warnings are a good example.

GDB Coding Standards
====================

   GDB follows the GNU coding standards, as described in
`etc/standards.texi'.  This file is also available for anonymous FTP
from GNU archive sites.  GDB takes a strict interpretation of the
standard; in general, when the GNU standard recommends a practice but
does not require it, GDB requires it.

   GDB follows an additional set of coding standards specific to GDB,
as described in the following sections.

ISO C
-----

   GDB assumes an ISO/IEC 9899:1990 (a.k.a. ISO C90) compliant compiler.

   GDB does not assume an ISO C or POSIX compliant C library.

Memory Management
-----------------

   GDB does not use the functions `malloc', `realloc', `calloc', `free'
and `asprintf'.

   GDB uses the functions `xmalloc', `xrealloc' and `xcalloc' when
allocating memory.  Unlike `malloc' et.al.  these functions do not
return when the memory pool is empty.  Instead, they unwind the stack
using cleanups.  These functions return `NULL' when requested to
allocate a chunk of memory of size zero.

   _Pragmatics: By using these functions, the need to check every
memory allocation is removed.  These functions provide portable
behavior._

   GDB does not use the function `free'.

   GDB uses the function `xfree' to return memory to the memory pool.
Consistent with ISO-C, this function ignores a request to free a `NULL'
pointer.

   _Pragmatics: On some systems `free' fails when passed a `NULL'
pointer._

   GDB can use the non-portable function `alloca' for the allocation of
small temporary values (such as strings).

   _Pragmatics: This function is very non-portable.  Some systems
restrict the memory being allocated to no more than a few kilobytes._

   GDB uses the string function `xstrdup' and the print function
`xasprintf'.

   _Pragmatics: `asprintf' and `strdup' can fail.  Print functions such
as `sprintf' are very prone to buffer overflow errors._

Compiler Warnings
-----------------

   With few exceptions, developers should include the configuration
option `--enable-gdb-build-warnings=,-Werror' when building GDB.  The
exceptions are listed in the file `gdb/MAINTAINERS'.

   This option causes GDB (when built using GCC) to be compiled with a
carefully selected list of compiler warning flags.  Any warnings from
those flags being treated as errors.

   The current list of warning flags includes:

`-Wimplicit'
     Since GDB coding standard requires all functions to be declared
     using a prototype, the flag has the side effect of ensuring that
     prototyped functions are always visible with out resorting to
     `-Wstrict-prototypes'.

`-Wreturn-type'
     Such code often appears to work except on instruction set
     architectures that use register windows.

`-Wcomment'

`-Wtrigraphs'

`-Wformat'
     Since GDB uses the `format printf' attribute on all `printf' like
     functions this checks not just `printf' calls but also calls to
     functions such as `fprintf_unfiltered'.

`-Wparentheses'
     This warning includes uses of the assignment operator within an
     `if' statement.

`-Wpointer-arith'

`-Wuninitialized'
   _Pragmatics: Due to the way that GDB is implemented most functions
have unused parameters.  Consequently the warning `-Wunused-parameter'
is precluded from the list.  The macro `ATTRIBUTE_UNUSED' is not used
as it leads to false negatives -- it is not an error to have
`ATTRIBUTE_UNUSED' on a parameter that is being used.  The options
`-Wall' and `-Wunused' are also precluded because they both include
`-Wunused-parameter'._

   _Pragmatics: GDB has not simply accepted the warnings enabled by
`-Wall -Werror -W...'.  Instead it is selecting warnings when and where
their benefits can be demonstrated._

Formatting
----------

   The standard GNU recommendations for formatting must be followed
strictly.

   A function declaration should not have its name in column zero.  A
function definition should have its name in column zero.

     /* Declaration */
     static void foo (void);
     /* Definition */
     void
     foo (void)
     {
     }

   _Pragmatics: This simplifies scripting.  Function definitions can be
found using `^function-name'._

   There must be a space between a function or macro name and the
opening parenthesis of its argument list (except for macro definitions,
as required by C).  There must not be a space after an open
paren/bracket or before a close paren/bracket.

   While additional whitespace is generally helpful for reading, do not
use more than one blank line to separate blocks, and avoid adding
whitespace after the end of a program line (as of 1/99, some 600 lines
had whitespace after the semicolon).  Excess whitespace causes
difficulties for `diff' and `patch' utilities.

   Pointers are declared using the traditional K&R C style:

     void *foo;

and not:

     void * foo;
     void* foo;

Comments
--------

   The standard GNU requirements on comments must be followed strictly.

   Block comments must appear in the following form, with no `/*'- or
`*/'-only lines, and no leading `*':

     /* Wait for control to return from inferior to debugger.  If inferior
        gets a signal, we may decide to start it up again instead of
        returning.  That is why there is a loop in this function.  When
        this function actually returns it means the inferior should be left
        stopped and GDB should read more commands.  */

   (Note that this format is encouraged by Emacs; tabbing for a
multi-line comment works correctly, and `M-q' fills the block
consistently.)

   Put a blank line between the block comments preceding function or
variable definitions, and the definition itself.

   In general, put function-body comments on lines by themselves, rather
than trying to fit them into the 20 characters left at the end of a
line, since either the comment or the code will inevitably get longer
than will fit, and then somebody will have to move it anyhow.

C Usage
-------

   Code must not depend on the sizes of C data types, the format of the
host's floating point numbers, the alignment of anything, or the order
of evaluation of expressions.

   Use functions freely.  There are only a handful of compute-bound
areas in GDB that might be affected by the overhead of a function call,
mainly in symbol reading.  Most of GDB's performance is limited by the
target interface (whether serial line or system call).

   However, use functions with moderation.  A thousand one-line
functions are just as hard to understand as a single thousand-line
function.

   _Macros are bad, M'kay._ (But if you have to use a macro, make sure
that the macro arguments are protected with parentheses.)

   Declarations like `struct foo *' should be used in preference to
declarations like `typedef struct foo { ... } *foo_ptr'.

Function Prototypes
-------------------

   Prototypes must be used when both _declaring_ and _defining_ a
function.  Prototypes for GDB functions must include both the argument
type and name, with the name matching that used in the actual function
definition.

   All external functions should have a declaration in a header file
that callers include, except for `_initialize_*' functions, which must
be external so that `init.c' construction works, but shouldn't be
visible to random source files.

   Where a source file needs a forward declaration of a static function,
that declaration must appear in a block near the top of the source file.

Internal Error Recovery
-----------------------

   During its execution, GDB can encounter two types of errors.  User
errors and internal errors.  User errors include not only a user
entering an incorrect command but also problems arising from corrupt
object files and system errors when interacting with the target.
Internal errors include situations where GDB has detected, at run time,
a corrupt or erroneous situation.

   When reporting an internal error, GDB uses `internal_error' and
`gdb_assert'.

   GDB must not call `abort' or `assert'.

   _Pragmatics: There is no `internal_warning' function.  Either the
code detected a user error, recovered from it and issued a `warning' or
the code failed to correctly recover from the user error and issued an
`internal_error'._

File Names
----------

   Any file used when building the core of GDB must be in lower case.
Any file used when building the core of GDB must be 8.3 unique.  These
requirements apply to both source and generated files.

   _Pragmatics: The core of GDB must be buildable on many platforms
including DJGPP and MacOS/HFS.  Every time an unfriendly file is
introduced to the build process both `Makefile.in' and `configure.in'
need to be modified accordingly.  Compare the convoluted conversion
process needed to transform `COPYING' into `copying.c' with the
conversion needed to transform `version.in' into `version.c'._

   Any file non 8.3 compliant file (that is not used when building the
core of GDB) must be added to `gdb/config/djgpp/fnchange.lst'.

   _Pragmatics: This is clearly a compromise._

   When GDB has a local version of a system header file (ex `string.h')
the file name based on the POSIX header prefixed with `gdb_'
(`gdb_string.h').

   For other files `-' is used as the separator.

Include Files
-------------

   A `.c' file should include `defs.h' first.

   A `.c' file should directly include the `.h' file of every
declaration and/or definition it directly refers to.  It cannot rely on
indirect inclusion.

   A `.h' file should directly include the `.h' file of every
declaration and/or definition it directly refers to.  It cannot rely on
indirect inclusion.  Exception: The file `defs.h' does not need to be
directly included.

   An external declaration should only appear in one include file.

   An external declaration should never appear in a `.c' file.
Exception: a declaration for the `_initialize' function that pacifies
`-Wmissing-declaration'.

   A `typedef' definition should only appear in one include file.

   An opaque `struct' declaration can appear in multiple `.h' files.
Where possible, a `.h' file should use an opaque `struct' declaration
instead of an include.

   All `.h' files should be wrapped in:

     #ifndef INCLUDE_FILE_NAME_H
     #define INCLUDE_FILE_NAME_H
     header body
     #endif

Clean Design and Portable Implementation
----------------------------------------

   In addition to getting the syntax right, there's the little question
of semantics.  Some things are done in certain ways in GDB because long
experience has shown that the more obvious ways caused various kinds of
trouble.

   You can't assume the byte order of anything that comes from a target
(including VALUEs, object files, and instructions).  Such things must
be byte-swapped using `SWAP_TARGET_AND_HOST' in GDB, or one of the swap
routines defined in `bfd.h', such as `bfd_get_32'.

   You can't assume that you know what interface is being used to talk
to the target system.  All references to the target must go through the
current `target_ops' vector.

   You can't assume that the host and target machines are the same
machine (except in the "native" support modules).  In particular, you
can't assume that the target machine's header files will be available
on the host machine.  Target code must bring along its own header files
- written from scratch or explicitly donated by their owner, to avoid
copyright problems.

   Insertion of new `#ifdef''s will be frowned upon.  It's much better
to write the code portably than to conditionalize it for various
systems.

   New `#ifdef''s which test for specific compilers or manufacturers or
operating systems are unacceptable.  All `#ifdef''s should test for
features.  The information about which configurations contain which
features should be segregated into the configuration files.  Experience
has proven far too often that a feature unique to one particular system
often creeps into other systems; and that a conditional based on some
predefined macro for your current system will become worthless over
time, as new versions of your system come out that behave differently
with regard to this feature.

   Adding code that handles specific architectures, operating systems,
target interfaces, or hosts, is not acceptable in generic code.

   One particularly notorious area where system dependencies tend to
creep in is handling of file names.  The mainline GDB code assumes
Posix semantics of file names: absolute file names begin with a forward
slash `/', slashes are used to separate leading directories,
case-sensitive file names.  These assumptions are not necessarily true
on non-Posix systems such as MS-Windows.  To avoid system-dependent
code where you need to take apart or construct a file name, use the
following portable macros:

`HAVE_DOS_BASED_FILE_SYSTEM'
     This preprocessing symbol is defined to a non-zero value on hosts
     whose filesystems belong to the MS-DOS/MS-Windows family.  Use this
     symbol to write conditional code which should only be compiled for
     such hosts.

`IS_DIR_SEPARATOR (C)'
     Evaluates to a non-zero value if C is a directory separator
     character.  On Unix and GNU/Linux systems, only a slash `/' is
     such a character, but on Windows, both `/' and `\' will pass.

`IS_ABSOLUTE_PATH (FILE)'
     Evaluates to a non-zero value if FILE is an absolute file name.
     For Unix and GNU/Linux hosts, a name which begins with a slash `/'
     is absolute.  On DOS and Windows, `d:/foo' and `x:\bar' are also
     absolute file names.

`FILENAME_CMP (F1, F2)'
     Calls a function which compares file names F1 and F2 as
     appropriate for the underlying host filesystem.  For Posix systems,
     this simply calls `strcmp'; on case-insensitive filesystems it
     will call `strcasecmp' instead.

`DIRNAME_SEPARATOR'
     Evaluates to a character which separates directories in
     `PATH'-style lists, typically held in environment variables.  This
     character is `:' on Unix, `;' on DOS and Windows.

`SLASH_STRING'
     This evaluates to a constant string you should use to produce an
     absolute filename from leading directories and the file's basename.
     `SLASH_STRING' is `"/"' on most systems, but might be `"\\"' for
     some Windows-based ports.

   In addition to using these macros, be sure to use portable library
functions whenever possible.  For example, to extract a directory or a
basename part from a file name, use the `dirname' and `basename'
library functions (available in `libiberty' for platforms which don't
provide them), instead of searching for a slash with `strrchr'.

   Another way to generalize GDB along a particular interface is with an
attribute struct.  For example, GDB has been generalized to handle
multiple kinds of remote interfaces--not by `#ifdef's everywhere, but
by defining the `target_ops' structure and having a current target (as
well as a stack of targets below it, for memory references).  Whenever
something needs to be done that depends on which remote interface we are
using, a flag in the current target_ops structure is tested (e.g.,
`target_has_stack'), or a function is called through a pointer in the
current target_ops structure.  In this way, when a new remote interface
is added, only one module needs to be touched--the one that actually
implements the new remote interface.  Other examples of
attribute-structs are BFD access to multiple kinds of object file
formats, or GDB's access to multiple source languages.

   Please avoid duplicating code.  For example, in GDB 3.x all the code
interfacing between `ptrace' and the rest of GDB was duplicated in
`*-dep.c', and so changing something was very painful.  In GDB 4.x,
these have all been consolidated into `infptrace.c'.  `infptrace.c' can
deal with variations between systems the same way any system-independent
file would (hooks, `#if defined', etc.), and machines which are
radically different don't need to use `infptrace.c' at all.

   All debugging code must be controllable using the `set debug MODULE'
command.  Do not use `printf' to print trace messages.  Use
`fprintf_unfiltered(gdb_stdlog, ...'.  Do not use `#ifdef DEBUG'.


File: gdbint.info,  Node: Porting GDB,  Next: Releasing GDB,  Prev: Coding,  Up: Top

Porting GDB
***********

   Most of the work in making GDB compile on a new machine is in
specifying the configuration of the machine.  This is done in a
dizzying variety of header files and configuration scripts, which we
hope to make more sensible soon.  Let's say your new host is called an
XYZ (e.g.,  `sun4'), and its full three-part configuration name is
`ARCH-XVEND-XOS' (e.g., `sparc-sun-sunos4').  In particular:

   * In the top level directory, edit `config.sub' and add ARCH, XVEND,
     and XOS to the lists of supported architectures, vendors, and
     operating systems near the bottom of the file.  Also, add XYZ as
     an alias that maps to `ARCH-XVEND-XOS'.  You can test your changes
     by running

          ./config.sub XYZ

     and

          ./config.sub `ARCH-XVEND-XOS'

     which should both respond with `ARCH-XVEND-XOS' and no error
     messages.

     You need to port BFD, if that hasn't been done already.  Porting
     BFD is beyond the scope of this manual.

   * To configure GDB itself, edit `gdb/configure.host' to recognize
     your system and set `gdb_host' to XYZ, and (unless your desired
     target is already available) also edit `gdb/configure.tgt',
     setting `gdb_target' to something appropriate (for instance, XYZ).

     _Maintainer's note: Work in progress.  The file
     `gdb/configure.host' originally needed to be modified when either a
     new native target or a new host machine was being added to GDB.
     Recent changes have removed this requirement.  The file now only
     needs to be modified when adding a new native configuration.  This
     will likely changed again in the future._

   * Finally, you'll need to specify and define GDB's host-, native-,
     and target-dependent `.h' and `.c' files used for your
     configuration.

Configuring GDB for Release
===========================

   From the top level directory (containing `gdb', `bfd', `libiberty',
and so on):

     make -f Makefile.in gdb.tar.gz

This will properly configure, clean, rebuild any files that are
distributed pre-built (e.g. `c-exp.tab.c' or `refcard.ps'), and will
then make a tarfile.  (If the top level directory has already been
configured, you can just do `make gdb.tar.gz' instead.)

   This procedure requires:

   * symbolic links;

   * `makeinfo' (texinfo2 level);

   * TeX;

   * `dvips';

   * `yacc' or `bison'.

... and the usual slew of utilities (`sed', `tar', etc.).

TEMPORARY RELEASE PROCEDURE FOR DOCUMENTATION
---------------------------------------------

   `gdb.texinfo' is currently marked up using the texinfo-2 macros,
which are not yet a default for anything (but we have to start using
them sometime).

   For making paper, the only thing this implies is the right
generation of `texinfo.tex' needs to be included in the distribution.

   For making info files, however, rather than duplicating the texinfo2
distribution, generate `gdb-all.texinfo' locally, and include the files
`gdb.info*' in the distribution.  Note the plural; `makeinfo' will
split the document into one overall file and five or so included files.


File: gdbint.info,  Node: Releasing GDB,  Next: Testsuite,  Prev: Porting GDB,  Up: Top

Releasing GDB
*************

Versions and Branches
=====================

Version Identifiers
-------------------

   GDB's version is determined by the file `gdb/version.in'.

   GDB's mainline uses ISO dates to differentiate between versions.
The CVS repository uses YYYY-MM-DD-cvs while the corresponding snapshot
uses YYYYMMDD.

   GDB's release branch uses a slightly more complicated scheme.  When
the branch is first cut, the mainline version identifier is prefixed
with the MAJOR.MINOR from of the previous release series but with .90
appended.  As draft releases are drawn from the branch, the minor minor
number (.90) is incremented.  Once the first release (M.N) has been
made, the version prefix is updated to M.N.0.90 (dot zero, dot ninety).
Follow on releases have an incremented minor minor version number (.0).

   Using 5.1 (previous) and 5.2 (current), the example below
illustrates a typical sequence of version identifiers:

5.1.1
     final release from previous branch

2002-03-03-cvs
     main-line the day the branch is cut

5.1.90-2002-03-03-cvs
     corresponding branch version

5.1.91
     first draft release candidate

5.1.91-2002-03-17-cvs
     updated branch version

5.1.92
     second draft release candidate

5.1.92-2002-03-31-cvs
     updated branch version

5.1.93
     final release candidate (see below)

5.2
     official release

5.2.0.90-2002-04-07-cvs
     updated CVS branch version

5.2.1
     second official release

   Notes:

   * Minor minor minor draft release candidates such as 5.2.0.91 have
     been omitted from the example.  Such release candidates are,
     typically, never made.

   * For 5.1.93 the bziped tar ball `gdb-5.1.93.tar.bz2' is just the
     official `gdb-5.2.tar' renamed and compressed.

   To avoid version conflicts, vendors are expected to modify the file
`gdb/version.in' to include a vendor unique alphabetic identifier (an
official GDB release never uses alphabetic characters in its version
identifer).

   Since GDB does not make minor minor minor releases (e.g., 5.1.0.1)
the conflict between that and a minor minor draft release identifier
(e.g., 5.1.0.90) is avoided.

Branches
--------

   GDB draws a release series (5.2, 5.2.1, ...) from a single release
branch (gdb_5_2-branch).  Since minor minor minor releases (5.1.0.1)
are not made, the need to branch the release branch is avoided (it also
turns out that the effort required for such a a branch and release is
significantly greater than the effort needed to create a new release
from the head of the release branch).

   Releases 5.0 and 5.1 used branch and release tags of the form:

     gdb_N_M-YYYY-MM-DD-branchpoint
     gdb_N_M-YYYY-MM-DD-branch
     gdb_M_N-YYYY-MM-DD-release

   Release 5.2 is trialing the branch and release tags:

     gdb_N_M-YYYY-MM-DD-branchpoint
     gdb_N_M-branch
     gdb_M_N-YYYY-MM-DD-release

   _Pragmatics: The branchpoint and release tags need to identify when
a branch and release are made.  The branch tag, denoting the head of the
branch, does not have this criteria._

Branch Commit Policy
====================

   The branch commit policy is pretty slack.  GDB releases 5.0, 5.1 and
5.2 all used the below:

   * The `gdb/MAINTAINERS' file still holds.

   * Don't fix something on the branch unless/until it is also fixed in
     the trunk.  If this isn't possible, mentioning it in the
     `gdb/PROBLEMS' file is better than committing a hack.

   * When considering a patch for the branch, suggested criteria
     include: Does it fix a build?  Does it fix the sequence `break
     main; run' when debugging a static binary?

   * The further a change is from the core of GDB, the less likely the
     change will worry anyone (e.g., target specific code).

   * Only post a proposal to change the core of GDB after you've sent
     individual bribes to all the people listed in the `MAINTAINERS'
     file ;-)

   _Pragmatics: Provided updates are restricted to non-core
functionality there is little chance that a broken change will be fatal.
This means that changes such as adding a new architectures or (within
reason) support for a new host are considered acceptable._

Obsoleting code
===============

   Before anything else, poke the other developers (and around the
source code) to see if there is anything that can be removed from GDB
(an old target, an unused file).

   Obsolete code is identified by adding an `OBSOLETE' prefix to every
line.  Doing this means that it is easy to identify something that has
been obsoleted when greping through the sources.

   The process is done in stages -- this is mainly to ensure that the
wider GDB community has a reasonable opportunity to respond.  Remember,
everything on the Internet takes a week.

  1. Post the proposal on the GDB mailing list <gdb@sources.redhat.com>
     Creating a bug report to track the task's state, is also highly
     recommended.

  2. Wait a week or so.

  3. Post the proposal on the GDB Announcement mailing list
     <gdb-announce@sources.redhat.com>.

  4. Wait a week or so.

  5. Go through and edit all relevant files and lines so that they are
     prefixed with the word `OBSOLETE'.

  6. Wait until the next GDB version, containing this obsolete code,
     has been released.

  7. Remove the obsolete code.

_Maintainer note: While removing old code is regrettable it is
hopefully better for GDB's long term development.  Firstly it helps the
developers by removing code that is either no longer relevant or simply
wrong.  Secondly since it removes any history associated with the file
(effectively clearing the slate) the developer has a much freer hand
when it comes to fixing broken files._

Before the Branch
=================

   The most important objective at this stage is to find and fix simple
changes that become a pain to track once the branch is created.  For
instance, configuration problems that stop GDB from even building.  If
you can't get the problem fixed, document it in the `gdb/PROBLEMS' file.

Prompt for `gdb/NEWS'
---------------------

   People always forget.  Send a post reminding them but also if you
know something interesting happened add it yourself.  The `schedule'
script will mention this in its e-mail.

Review `gdb/README'
-------------------

   Grab one of the nightly snapshots and then walk through the
`gdb/README' looking for anything that can be improved.  The `schedule'
script will mention this in its e-mail.

Refresh any imported files.
---------------------------

   A number of files are taken from external repositories.  They
include:

   * `texinfo/texinfo.tex'

   * `config.guess' et. al. (see the top-level `MAINTAINERS' file)

   * `etc/standards.texi', `etc/make-stds.texi'

Check the ARI
-------------

   A.R.I. is an `awk' script (Awk Regression Index ;-) that checks for
a number of errors and coding conventions.  The checks include things
like using `malloc' instead of `xmalloc' and file naming problems.
There shouldn't be any regressions.

Review the bug data base
------------------------

   Close anything obviously fixed.

Check all cross targets build
-----------------------------

   The targets are listed in `gdb/MAINTAINERS'.

Cut the Branch
==============

Create the branch
-----------------

     $  u=5.1
     $  v=5.2
     $  V=`echo $v | sed 's/\./_/g'`
     $  D=`date -u +%Y-%m-%d`
     $  echo $u $V $D
     5.1 5_2 2002-03-03
     $  echo cvs -f -d :ext:sources.redhat.com:/cvs/src rtag \
     -D $D-gmt gdb_$V-$D-branchpoint insight+dejagnu
     cvs -f -d :ext:sources.redhat.com:/cvs/src rtag
     -D 2002-03-03-gmt gdb_5_2-2002-03-03-branchpoint insight+dejagnu
     $  ^echo ^^
     ...
     $  echo cvs -f -d :ext:sources.redhat.com:/cvs/src rtag \
     -b -r gdb_$V-$D-branchpoint gdb_$V-branch insight+dejagnu
     cvs -f -d :ext:sources.redhat.com:/cvs/src rtag \
     -b -r gdb_5_2-2002-03-03-branchpoint gdb_5_2-branch insight+dejagnu
     $  ^echo ^^
     ...
     $

   * by using `-D YYYY-MM-DD-gmt' the branch is forced to an exact
     date/time.

   * the trunk is first taged so that the branch point can easily be
     found

   * Insight (which includes GDB) and dejagnu are all tagged at the
     same time

   * `version.in' gets bumped to avoid version number conflicts

   * the reading of `.cvsrc' is disabled using `-f'

Update `version.in'
-------------------

     $  u=5.1
     $  v=5.2
     $  V=`echo $v | sed 's/\./_/g'`
     $  echo $u $v$V
     5.1 5_2
     $  cd /tmp
     $  echo cvs -f -d :ext:sources.redhat.com:/cvs/src co \
     -r gdb_$V-branch src/gdb/version.in
     cvs -f -d :ext:sources.redhat.com:/cvs/src co
      -r gdb_5_2-branch src/gdb/version.in
     $  ^echo ^^
     U src/gdb/version.in
     $  cd src/gdb
     $  echo $u.90-0000-00-00-cvs > version.in
     $  cat version.in
     5.1.90-0000-00-00-cvs
     $  cvs -f commit version.in

   * `0000-00-00' is used as a date to pump prime the version.in update
     mechanism

   * `.90' and the previous branch version are used as fairly arbitrary
     initial branch version number

Update the web and news pages
-----------------------------

   Something?

Tweak cron to track the new branch
----------------------------------

   The file `gdbadmin/cron/crontab' contains gdbadmin's cron table.
This file needs to be updated so that:

   * a daily timestamp is added to the file `version.in'

   * the new branch is included in the snapshot process

See the file `gdbadmin/cron/README' for how to install the updated cron
table.

   The file `gdbadmin/ss/README' should also be reviewed to reflect any
changes.  That file is copied to both the branch/ and current/ snapshot
directories.

Update the NEWS and README files
--------------------------------

   The `NEWS' file needs to be updated so that on the branch it refers
to _changes in the current release_ while on the trunk it also refers
to _changes since the current release_.

   The `README' file needs to be updated so that it refers to the
current release.

Post the branch info
--------------------

   Send an announcement to the mailing lists:

   * GDB Announcement mailing list <gdb-announce@sources.redhat.com>

   * GDB Discsussion mailing list <gdb@sources.redhat.com> and GDB
     Discsussion mailing list <gdb-testers@sources.redhat.com>

   _Pragmatics: The branch creation is sent to the announce list to
ensure that people people not subscribed to the higher volume discussion
list are alerted._

   The announcement should include:

   * the branch tag

   * how to check out the branch using CVS

   * the date/number of weeks until the release

   * the branch commit policy still holds.

Stabilize the branch
====================

   Something goes here.

Create a Release
================

   The process of creating and then making available a release is broken
down into a number of stages.  The first part addresses the technical
process of creating a releasable tar ball.  The later stages address the
process of releasing that tar ball.

   When making a release candidate just the first section is needed.

Create a release candidate
--------------------------

   The objective at this stage is to create a set of tar balls that can
be made available as a formal release (or as a less formal release
candidate).

Freeze the branch
.................

   Send out an e-mail notifying everyone that the branch is frozen to
<gdb-patches@sources.redhat.com>.

Establish a few defaults.
.........................

     $  b=gdb_5_2-branch
     $  v=5.2
     $  t=/sourceware/snapshot-tmp/gdbadmin-tmp
     $  echo $t/$b/$v
     /sourceware/snapshot-tmp/gdbadmin-tmp/gdb_5_2-branch/5.2
     $  mkdir -p $t/$b/$v
     $  cd $t/$b/$v
     $  pwd
     /sourceware/snapshot-tmp/gdbadmin-tmp/gdb_5_2-branch/5.2
     $  which autoconf
     /home/gdbadmin/bin/autoconf
     $

Notes:

   * Check the `autoconf' version carefully.  You want to be using the
     version taken from the `binutils' snapshot directory, which can be
     found at `ftp://sources.redhat.com/pub/binutils/'. It is very
     unlikely that a system installed version of `autoconf' (e.g.,
     `/usr/bin/autoconf') is correct.

Check out the relevant modules:
...............................

     $  for m in gdb insight dejagnu
     do
     ( mkdir -p $m && cd $m && cvs -q -f -d /cvs/src co -P -r $b $m )
     done
     $

Note:

   * The reading of `.cvsrc' is disabled (`-f') so that there isn't any
     confusion between what is written here and what your local `cvs'
     really does.

Update relevant files.
......................

`gdb/NEWS'
     Major releases get their comments added as part of the mainline.
     Minor releases should probably mention any significant bugs that
     were fixed.

     Don't forget to include the `ChangeLog' entry.

          $  emacs gdb/src/gdb/NEWS
          ...
          c-x 4 a
          ...
          c-x c-s c-x c-c
          $  cp gdb/src/gdb/NEWS insight/src/gdb/NEWS
          $  cp gdb/src/gdb/ChangeLog insight/src/gdb/ChangeLog

`gdb/README'
     You'll need to update:

        * the version

        * the update date

        * who did it

          $  emacs gdb/src/gdb/README
          ...
          c-x 4 a
          ...
          c-x c-s c-x c-c
          $  cp gdb/src/gdb/README insight/src/gdb/README
          $  cp gdb/src/gdb/ChangeLog insight/src/gdb/ChangeLog

     _Maintainer note: Hopefully the `README' file was reviewed before
     the initial branch was cut so just a simple substitute is needed
     to get it updated._

     _Maintainer note: Other projects generate `README' and `INSTALL'
     from the core documentation.  This might be worth pursuing._

`gdb/version.in'
          $  echo $v > gdb/src/gdb/version.in
          $  cat gdb/src/gdb/version.in
          5.2
          $  emacs gdb/src/gdb/version.in
          ...
          c-x 4 a
          ... Bump to version ...
          c-x c-s c-x c-c
          $  cp gdb/src/gdb/version.in insight/src/gdb/version.in
          $  cp gdb/src/gdb/ChangeLog insight/src/gdb/ChangeLog

`dejagnu/src/dejagnu/configure.in'
     Dejagnu is more complicated.  The version number is a parameter to
     `AM_INIT_AUTOMAKE'.  Tweak it to read something like gdb-5.1.91.

     Don't forget to re-generate `configure'.

     Don't forget to include a `ChangeLog' entry.

          $  emacs dejagnu/src/dejagnu/configure.in
          ...
          c-x 4 a
          ...
          c-x c-s c-x c-c
          $  ( cd  dejagnu/src/dejagnu && autoconf )

Do the dirty work
.................

   This is identical to the process used to create the daily snapshot.

     $  for m in gdb insight
     do
     ( cd $m/src && gmake -f Makefile.in $m.tar )
     done
     $  ( m=dejagnu; cd $m/src && gmake -f Makefile.in $m.tar.bz2 )

Check the source files
......................

   You're looking for files that have mysteriously disappeared.
`distclean' has the habit of deleting files it shouldn't.  Watch out
for the `version.in' update `cronjob'.

     $  ( cd gdb/src && cvs -f -q -n update )
     M djunpack.bat
     ? gdb-5.1.91.tar
     ? proto-toplev
     ... lots of generated files ...
     M gdb/ChangeLog
     M gdb/NEWS
     M gdb/README
     M gdb/version.in
     ... lots of generated files ...
     $

_Don't worry about the `gdb.info-??' or `gdb/p-exp.tab.c'.  They were
generated (and yes `gdb.info-1' was also generated only something
strange with CVS means that they didn't get supressed).  Fixing it
would be nice though._

Create compressed versions of the release
.........................................

     $  cp */src/*.tar .
     $  cp */src/*.bz2 .
     $  ls -F
     dejagnu/ dejagnu-gdb-5.2.tar.bz2 gdb/ gdb-5.2.tar insight/ insight-5.2.tar
     $  for m in gdb insight
     do
     bzip2 -v -9 -c $m-$v.tar > $m-$v.tar.bz2
     gzip -v -9 -c $m-$v.tar > $m-$v.tar.gz
     done
     $

Note:

   * A pipe such as `bunzip2 < xxx.bz2 | gzip -9 > xxx.gz' is not since,
     in that mode, `gzip' does not know the name of the file and, hence,
     can not include it in the compressed file.  This is also why the
     release process runs `tar' and `bzip2' as separate passes.

Sanity check the tar ball
-------------------------

   Pick a popular machine (Solaris/PPC?) and try the build on that.

     $  bunzip2 < gdb-5.2.tar.bz2 | tar xpf -
     $  cd gdb-5.2
     $  ./configure
     $  make
     ...
     $  ./gdb/gdb ./gdb/gdb
     GNU gdb 5.2
     ...
     (gdb)  b main
     Breakpoint 1 at 0x80732bc: file main.c, line 734.
     (gdb)  run
     Starting program: /tmp/gdb-5.2/gdb/gdb
     
     Breakpoint 1, main (argc=1, argv=0xbffff8b4) at main.c:734
     734       catch_errors (captured_main, &args, "", RETURN_MASK_ALL);
     (gdb)  print args
     $1 = {argc = 136426532, argv = 0x821b7f0}
     (gdb)

Make a release candidate available
----------------------------------

   If this is a release candidate then the only remaining steps are:

  1. Commit `version.in' and `ChangeLog'

  2. Tweak `version.in' (and `ChangeLog' to read L.M.N-0000-00-00-cvs
     so that the version update process can restart.

  3. Make the release candidate available in
     `ftp://sources.redhat.com/pub/gdb/snapshots/branch'

  4. Notify the relevant mailing lists ( <gdb@sources.redhat.com> and
     <gdb-testers@sources.redhat.com> that the candidate is available.

Make a formal release available
-------------------------------

   (And you thought all that was required was to post an e-mail.)

Install on sware
................

   Copy the new files to both the release and the old release directory:

     $  cp *.bz2 *.gz ~ftp/pub/gdb/old-releases/
     $  cp *.bz2 *.gz ~ftp/pub/gdb/releases

Clean up the releases directory so that only the most recent releases
are available (e.g. keep 5.2 and 5.2.1 but remove 5.1):

     $  cd ~ftp/pub/gdb/releases
     $  rm ...

Update the file `README' and `.message' in the releases directory:

     $  vi README
     ...
     $  rm -f .message
     $  ln README .message

Update the web pages.
.....................

`htdocs/download/ANNOUNCEMENT'
     This file, which is posted as the official announcement, includes:
        * General announcement

        * News.  If making an M.N.1 release, retain the news from
          earlier M.N release.

        * Errata

`htdocs/index.html'
`htdocs/news/index.html'
`htdocs/download/index.html'
     These files include:
        * announcement of the most recent release

        * news entry (remember to update both the top level and the
          news directory).
     These pages also need to be regenerate using `index.sh'.

`download/onlinedocs/'
     You need to find the magic command that is used to generate the
     online docs from the `.tar.bz2'.  The best way is to look in the
     output from one of the nightly `cron' jobs and then just edit
     accordingly.  Something like:

          $  ~/ss/update-web-docs \
           ~ftp/pub/gdb/releases/gdb-5.2.tar.bz2 \
           $PWD/www \
           /www/sourceware/htdocs/gdb/download/onlinedocs \
           gdb

`download/ari/'
     Just like the online documentation.  Something like:

          $  /bin/sh ~/ss/update-web-ari \
           ~ftp/pub/gdb/releases/gdb-5.2.tar.bz2 \
           $PWD/www \
           /www/sourceware/htdocs/gdb/download/ari \
           gdb

Shadow the pages onto gnu
.........................

   Something goes here.

Install the GDB tar ball on GNU
...............................

   At the time of writing, the GNU machine was `gnudist.gnu.org' in
`~ftp/gnu/gdb'.

Make the `ANNOUNCEMENT'
.......................

   Post the `ANNOUNCEMENT' file you created above to:

   * GDB Announcement mailing list <gdb-announce@sources.redhat.com>

   * General GNU Announcement list <info-gnu@gnu.org> (but delay it a
     day or so to let things get out)

   * GDB Bug Report mailing list <bug-gdb@gnu.org>

Cleanup
-------

   The release is out but you're still not finished.

Commit outstanding changes
..........................

   In particular you'll need to commit any changes to:

   * `gdb/ChangeLog'

   * `gdb/version.in'

   * `gdb/NEWS'

   * `gdb/README'

Tag the release
...............

   Something like:

     $  d=`date -u +%Y-%m-%d`
     $  echo $d
     2002-01-24
     $  ( cd insight/src/gdb && cvs -f -q update )
     $  ( cd insight/src && cvs -f -q tag gdb_5_2-$d-release )

   Insight is used since that contains more of the release than GDB
(`dejagnu' doesn't get tagged but I think we can live with that).

Mention the release on the trunk
................................

   Just put something in the `ChangeLog' so that the trunk also
indicates when the release was made.

Restart `gdb/version.in'
........................

   If `gdb/version.in' does not contain an ISO date such as
`2002-01-24' then the daily `cronjob' won't update it.  Having
committed all the release changes it can be set to
`5.2.0_0000-00-00-cvs' which will restart things (yes the `_' is
important - it affects the snapshot process).

   Don't forget the `ChangeLog'.

Merge into trunk
................

   The files committed to the branch may also need changes merged into
the trunk.

Revise the release schedule
...........................

   Post a revised release schedule to GDB Discussion List
<gdb@sources.redhat.com> with an updated announcement.  The schedule
can be generated by running:

     $  ~/ss/schedule `date +%s` schedule

The first parameter is approximate date/time in seconds (from the epoch)
of the most recent release.

   Also update the schedule `cronjob'.

Post release
============

   Remove any `OBSOLETE' code.


File: gdbint.info,  Node: Testsuite,  Next: Hints,  Prev: Releasing GDB,  Up: Top

Testsuite
*********

   The testsuite is an important component of the GDB package.  While
it is always worthwhile to encourage user testing, in practice this is
rarely sufficient; users typically use only a small subset of the
available commands, and it has proven all too common for a change to
cause a significant regression that went unnoticed for some time.

   The GDB testsuite uses the DejaGNU testing framework.  DejaGNU is
built using `Tcl' and `expect'.  The tests themselves are calls to
various `Tcl' procs; the framework runs all the procs and summarizes
the passes and fails.

Using the Testsuite
===================

   To run the testsuite, simply go to the GDB object directory (or to
the testsuite's objdir) and type `make check'.  This just sets up some
environment variables and invokes DejaGNU's `runtest' script.  While
the testsuite is running, you'll get mentions of which test file is in
use, and a mention of any unexpected passes or fails.  When the
testsuite is finished, you'll get a summary that looks like this:

                     === gdb Summary ===
     
     # of expected passes            6016
     # of unexpected failures        58
     # of unexpected successes       5
     # of expected failures          183
     # of unresolved testcases       3
     # of untested testcases         5

   The ideal test run consists of expected passes only; however, reality
conspires to keep us from this ideal.  Unexpected failures indicate
real problems, whether in GDB or in the testsuite.  Expected failures
are still failures, but ones which have been decided are too hard to
deal with at the time; for instance, a test case might work everywhere
except on AIX, and there is no prospect of the AIX case being fixed in
the near future.  Expected failures should not be added lightly, since
you may be masking serious bugs in GDB.  Unexpected successes are
expected fails that are passing for some reason, while unresolved and
untested cases often indicate some minor catastrophe, such as the
compiler being unable to deal with a test program.

   When making any significant change to GDB, you should run the
testsuite before and after the change, to confirm that there are no
regressions.  Note that truly complete testing would require that you
run the testsuite with all supported configurations and a variety of
compilers; however this is more than really necessary.  In many cases
testing with a single configuration is sufficient.  Other useful
options are to test one big-endian (Sparc) and one little-endian (x86)
host, a cross config with a builtin simulator (powerpc-eabi, mips-elf),
or a 64-bit host (Alpha).

   If you add new functionality to GDB, please consider adding tests
for it as well; this way future GDB hackers can detect and fix their
changes that break the functionality you added.  Similarly, if you fix
a bug that was not previously reported as a test failure, please add a
test case for it.  Some cases are extremely difficult to test, such as
code that handles host OS failures or bugs in particular versions of
compilers, and it's OK not to try to write tests for all of those.

Testsuite Organization
======================

   The testsuite is entirely contained in `gdb/testsuite'.  While the
testsuite includes some makefiles and configury, these are very minimal,
and used for little besides cleaning up, since the tests themselves
handle the compilation of the programs that GDB will run.  The file
`testsuite/lib/gdb.exp' contains common utility procs useful for all
GDB tests, while the directory `testsuite/config' contains
configuration-specific files, typically used for special-purpose
definitions of procs like `gdb_load' and `gdb_start'.

   The tests themselves are to be found in `testsuite/gdb.*' and
subdirectories of those.  The names of the test files must always end
with `.exp'.  DejaGNU collects the test files by wildcarding in the
test directories, so both subdirectories and individual files get
chosen and run in alphabetical order.

   The following table lists the main types of subdirectories and what
they are for.  Since DejaGNU finds test files no matter where they are
located, and since each test file sets up its own compilation and
execution environment, this organization is simply for convenience and
intelligibility.

`gdb.base'
     This is the base testsuite.  The tests in it should apply to all
     configurations of GDB (but generic native-only tests may live
     here).  The test programs should be in the subset of C that is
     valid K&R, ANSI/ISO, and C++ (`#ifdef's are allowed if necessary,
     for instance for prototypes).

`gdb.LANG'
     Language-specific tests for any language LANG besides C.  Examples
     are `gdb.c++' and `gdb.java'.

`gdb.PLATFORM'
     Non-portable tests.  The tests are specific to a specific
     configuration (host or target), such as HP-UX or eCos.  Example is
     `gdb.hp', for HP-UX.

`gdb.COMPILER'
     Tests specific to a particular compiler.  As of this writing (June
     1999), there aren't currently any groups of tests in this category
     that couldn't just as sensibly be made platform-specific, but one
     could imagine a `gdb.gcc', for tests of GDB's handling of GCC
     extensions.

`gdb.SUBSYSTEM'
     Tests that exercise a specific GDB subsystem in more depth.  For
     instance, `gdb.disasm' exercises various disassemblers, while
     `gdb.stabs' tests pathways through the stabs symbol reader.

Writing Tests
=============

   In many areas, the GDB tests are already quite comprehensive; you
should be able to copy existing tests to handle new cases.

   You should try to use `gdb_test' whenever possible, since it
includes cases to handle all the unexpected errors that might happen.
However, it doesn't cost anything to add new test procedures; for
instance, `gdb.base/exprs.exp' defines a `test_expr' that calls
`gdb_test' multiple times.

   Only use `send_gdb' and `gdb_expect' when absolutely necessary, such
as when GDB has several valid responses to a command.

   The source language programs do _not_ need to be in a consistent
style.  Since GDB is used to debug programs written in many different
styles, it's worth having a mix of styles in the testsuite; for
instance, some GDB bugs involving the display of source lines would
never manifest themselves if the programs used GNU coding style
uniformly.


File: gdbint.info,  Node: Hints,  Next: GNU Free Documentation License,  Prev: Testsuite,  Up: Top

Hints
*****

   Check the `README' file, it often has useful information that does
not appear anywhere else in the directory.

* Menu:

* Getting Started::		Getting started working on GDB
* Debugging GDB::		Debugging GDB with itself


File: gdbint.info,  Node: Getting Started,  Up: Hints

Getting Started
===============

   GDB is a large and complicated program, and if you first starting to
work on it, it can be hard to know where to start.  Fortunately, if you
know how to go about it, there are ways to figure out what is going on.

   This manual, the GDB Internals manual, has information which applies
generally to many parts of GDB.

   Information about particular functions or data structures are
located in comments with those functions or data structures.  If you
run across a function or a global variable which does not have a
comment correctly explaining what is does, this can be thought of as a
bug in GDB; feel free to submit a bug report, with a suggested comment
if you can figure out what the comment should say.  If you find a
comment which is actually wrong, be especially sure to report that.

   Comments explaining the function of macros defined in host, target,
or native dependent files can be in several places.  Sometimes they are
repeated every place the macro is defined.  Sometimes they are where the
macro is used.  Sometimes there is a header file which supplies a
default definition of the macro, and the comment is there.  This manual
also documents all the available macros.

   Start with the header files.  Once you have some idea of how GDB's
internal symbol tables are stored (see `symtab.h', `gdbtypes.h'), you
will find it much easier to understand the code which uses and creates
those symbol tables.

   You may wish to process the information you are getting somehow, to
enhance your understanding of it.  Summarize it, translate it to another
language, add some (perhaps trivial or non-useful) feature to GDB, use
the code to predict what a test case would do and write the test case
and verify your prediction, etc.  If you are reading code and your eyes
are starting to glaze over, this is a sign you need to use a more active
approach.

   Once you have a part of GDB to start with, you can find more
specifically the part you are looking for by stepping through each
function with the `next' command.  Do not use `step' or you will
quickly get distracted; when the function you are stepping through
calls another function try only to get a big-picture understanding
(perhaps using the comment at the beginning of the function being
called) of what it does.  This way you can identify which of the
functions being called by the function you are stepping through is the
one which you are interested in.  You may need to examine the data
structures generated at each stage, with reference to the comments in
the header files explaining what the data structures are supposed to
look like.

   Of course, this same technique can be used if you are just reading
the code, rather than actually stepping through it.  The same general
principle applies--when the code you are looking at calls something
else, just try to understand generally what the code being called does,
rather than worrying about all its details.

   A good place to start when tracking down some particular area is with
a command which invokes that feature.  Suppose you want to know how
single-stepping works.  As a GDB user, you know that the `step' command
invokes single-stepping.  The command is invoked via command tables
(see `command.h'); by convention the function which actually performs
the command is formed by taking the name of the command and adding
`_command', or in the case of an `info' subcommand, `_info'.  For
example, the `step' command invokes the `step_command' function and the
`info display' command invokes `display_info'.  When this convention is
not followed, you might have to use `grep' or `M-x tags-search' in
emacs, or run GDB on itself and set a breakpoint in `execute_command'.

   If all of the above fail, it may be appropriate to ask for
information on `bug-gdb'.  But _never_ post a generic question like "I
was wondering if anyone could give me some tips about understanding
GDB"--if we had some magic secret we would put it in this manual.
Suggestions for improving the manual are always welcome, of course.


File: gdbint.info,  Node: Debugging GDB,  Up: Hints

Debugging GDB with itself
=========================

   If GDB is limping on your machine, this is the preferred way to get
it fully functional.  Be warned that in some ancient Unix systems, like
Ultrix 4.2, a program can't be running in one process while it is being
debugged in another.  Rather than typing the command `./gdb ./gdb',
which works on Suns and such, you can copy `gdb' to `gdb2' and then
type `./gdb ./gdb2'.

   When you run GDB in the GDB source directory, it will read a
`.gdbinit' file that sets up some simple things to make debugging gdb
easier.  The `info' command, when executed without a subcommand in a
GDB being debugged by gdb, will pop you back up to the top level gdb.
See `.gdbinit' for details.

   If you use emacs, you will probably want to do a `make TAGS' after
you configure your distribution; this will put the machine dependent
routines for your local machine where they will be accessed first by
`M-.'

   Also, make sure that you've either compiled GDB with your local cc,
or have run `fixincludes' if you are compiling with gcc.

Submitting Patches
==================

   Thanks for thinking of offering your changes back to the community of
GDB users.  In general we like to get well designed enhancements.
Thanks also for checking in advance about the best way to transfer the
changes.

   The GDB maintainers will only install "cleanly designed" patches.
This manual summarizes what we believe to be clean design for GDB.

   If the maintainers don't have time to put the patch in when it
arrives, or if there is any question about a patch, it goes into a
large queue with everyone else's patches and bug reports.

   The legal issue is that to incorporate substantial changes requires a
copyright assignment from you and/or your employer, granting ownership
of the changes to the Free Software Foundation.  You can get the
standard documents for doing this by sending mail to `gnu@gnu.org' and
asking for it.  We recommend that people write in "All programs owned
by the Free Software Foundation" as "NAME OF PROGRAM", so that changes
in many programs (not just GDB, but GAS, Emacs, GCC, etc) can be
contributed with only one piece of legalese pushed through the
bureaucracy and filed with the FSF.  We can't start merging changes
until this paperwork is received by the FSF (their rules, which we
follow since we maintain it for them).

   Technically, the easiest way to receive changes is to receive each
feature as a small context diff or unidiff, suitable for `patch'.  Each
message sent to me should include the changes to C code and header
files for a single feature, plus `ChangeLog' entries for each directory
where files were modified, and diffs for any changes needed to the
manuals (`gdb/doc/gdb.texinfo' or `gdb/doc/gdbint.texinfo').  If there
are a lot of changes for a single feature, they can be split down into
multiple messages.

   In this way, if we read and like the feature, we can add it to the
sources with a single patch command, do some testing, and check it in.
If you leave out the `ChangeLog', we have to write one.  If you leave
out the doc, we have to puzzle out what needs documenting.  Etc., etc.

   The reason to send each change in a separate message is that we will
not install some of the changes.  They'll be returned to you with
questions or comments.  If we're doing our job correctly, the message
back to you will say what you have to fix in order to make the change
acceptable.  The reason to have separate messages for separate features
is so that the acceptable changes can be installed while one or more
changes are being reworked.  If multiple features are sent in a single
message, we tend to not put in the effort to sort out the acceptable
changes from the unacceptable, so none of the features get installed
until all are acceptable.

   If this sounds painful or authoritarian, well, it is.  But we get a
lot of bug reports and a lot of patches, and many of them don't get
installed because we don't have the time to finish the job that the bug
reporter or the contributor could have done.  Patches that arrive
complete, working, and well designed, tend to get installed on the day
they arrive.  The others go into a queue and get installed as time
permits, which, since the maintainers have many demands to meet, may not
be for quite some time.

   Please send patches directly to the GDB maintainers
<gdb-patches@sources.redhat.com>.

Obsolete Conditionals
=====================

   Fragments of old code in GDB sometimes reference or set the following
configuration macros.  They should not be used by new code, and old uses
should be removed as those parts of the debugger are otherwise touched.

`STACK_END_ADDR'
     This macro used to define where the end of the stack appeared, for
     use in interpreting core file formats that don't record this
     address in the core file itself.  This information is now
     configured in BFD, and GDB gets the info portably from there.  The
     values in GDB's configuration files should be moved into BFD
     configuration files (if needed there), and deleted from all of
     GDB's config files.

     Any `FOO-xdep.c' file that references STACK_END_ADDR is so old
     that it has never been converted to use BFD.  Now that's old!


File: gdbint.info,  Node: GNU Free Documentation License,  Next: Index,  Prev: Hints,  Up: Top

GNU Free Documentation License
******************************

                        Version 1.1, March 2000
     Copyright (C) 2000  Free Software Foundation, Inc.
     59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
     
     Everyone is permitted to copy and distribute verbatim copies
     of this license document, but changing it is not allowed.


  0. PREAMBLE

     The purpose of this License is to make a manual, textbook, or other
     written document "free" in the sense of freedom: to assure everyone
     the effective freedom to copy and redistribute it, with or without
     modifying it, either commercially or noncommercially.  Secondarily,
     this License preserves for the author and publisher a way to get
     credit for their work, while not being considered responsible for
     modifications made by others.

     This License is a kind of "copyleft", which means that derivative
     works of the document must themselves be free in the same sense.
     It complements the GNU General Public License, which is a copyleft
     license designed for free software.

     We have designed this License in order to use it for manuals for
     free software, because free software needs free documentation: a
     free program should come with manuals providing the same freedoms
     that the software does.  But this License is not limited to
     software manuals; it can be used for any textual work, regardless
     of subject matter or whether it is published as a printed book.
     We recommend this License principally for works whose purpose is
     instruction or reference.


  1. APPLICABILITY AND DEFINITIONS

     This License applies to any manual or other work that contains a
     notice placed by the copyright holder saying it can be distributed
     under the terms of this License.  The "Document", below, refers to
     any such manual or work.  Any member of the public is a licensee,
     and is addressed as "you."

     A "Modified Version" of the Document means any work containing the
     Document or a portion of it, either copied verbatim, or with
     modifications and/or translated into another language.

     A "Secondary Section" is a named appendix or a front-matter
     section of the Document that deals exclusively with the
     relationship of the publishers or authors of the Document to the
     Document's overall subject (or to related matters) and contains
     nothing that could fall directly within that overall subject.
     (For example, if the Document is in part a textbook of
     mathematics, a Secondary Section may not explain any mathematics.)
     The relationship could be a matter of historical connection with
     the subject or with related matters, or of legal, commercial,
     philosophical, ethical or political position regarding them.

     The "Invariant Sections" are certain Secondary Sections whose
     titles are designated, as being those of Invariant Sections, in
     the notice that says that the Document is released under this
     License.

     The "Cover Texts" are certain short passages of text that are
     listed, as Front-Cover Texts or Back-Cover Texts, in the notice
     that says that the Document is released under this License.

     A "Transparent" copy of the Document means a machine-readable copy,
     represented in a format whose specification is available to the
     general public, whose contents can be viewed and edited directly
     and straightforwardly with generic text editors or (for images
     composed of pixels) generic paint programs or (for drawings) some
     widely available drawing editor, and that is suitable for input to
     text formatters or for automatic translation to a variety of
     formats suitable for input to text formatters.  A copy made in an
     otherwise Transparent file format whose markup has been designed
     to thwart or discourage subsequent modification by readers is not
     Transparent.  A copy that is not "Transparent" is called "Opaque."

     Examples of suitable formats for Transparent copies include plain
     ASCII without markup, Texinfo input format, LaTeX input format,
     SGML or XML using a publicly available DTD, and
     standard-conforming simple HTML designed for human modification.
     Opaque formats include PostScript, PDF, proprietary formats that
     can be read and edited only by proprietary word processors, SGML
     or XML for which the DTD and/or processing tools are not generally
     available, and the machine-generated HTML produced by some word
     processors for output purposes only.

     The "Title Page" means, for a printed book, the title page itself,
     plus such following pages as are needed to hold, legibly, the
     material this License requires to appear in the title page.  For
     works in formats which do not have any title page as such, "Title
     Page" means the text near the most prominent appearance of the
     work's title, preceding the beginning of the body of the text.

  2. VERBATIM COPYING

     You may copy and distribute the Document in any medium, either
     commercially or noncommercially, provided that this License, the
     copyright notices, and the license notice saying this License
     applies to the Document are reproduced in all copies, and that you
     add no other conditions whatsoever to those of this License.  You
     may not use technical measures to obstruct or control the reading
     or further copying of the copies you make or distribute.  However,
     you may accept compensation in exchange for copies.  If you
     distribute a large enough number of copies you must also follow
     the conditions in section 3.

     You may also lend copies, under the same conditions stated above,
     and you may publicly display copies.

  3. COPYING IN QUANTITY

     If you publish printed copies of the Document numbering more than
     100, and the Document's license notice requires Cover Texts, you
     must enclose the copies in covers that carry, clearly and legibly,
     all these Cover Texts: Front-Cover Texts on the front cover, and
     Back-Cover Texts on the back cover.  Both covers must also clearly
     and legibly identify you as the publisher of these copies.  The
     front cover must present the full title with all words of the
     title equally prominent and visible.  You may add other material
     on the covers in addition.  Copying with changes limited to the
     covers, as long as they preserve the title of the Document and
     satisfy these conditions, can be treated as verbatim copying in
     other respects.

     If the required texts for either cover are too voluminous to fit
     legibly, you should put the first ones listed (as many as fit
     reasonably) on the actual cover, and continue the rest onto
     adjacent pages.

     If you publish or distribute Opaque copies of the Document
     numbering more than 100, you must either include a
     machine-readable Transparent copy along with each Opaque copy, or
     state in or with each Opaque copy a publicly-accessible
     computer-network location containing a complete Transparent copy
     of the Document, free of added material, which the general
     network-using public has access to download anonymously at no
     charge using public-standard network protocols.  If you use the
     latter option, you must take reasonably prudent steps, when you
     begin distribution of Opaque copies in quantity, to ensure that
     this Transparent copy will remain thus accessible at the stated
     location until at least one year after the last time you
     distribute an Opaque copy (directly or through your agents or
     retailers) of that edition to the public.

     It is requested, but not required, that you contact the authors of
     the Document well before redistributing any large number of
     copies, to give them a chance to provide you with an updated
     version of the Document.

  4. MODIFICATIONS

     You may copy and distribute a Modified Version of the Document
     under the conditions of sections 2 and 3 above, provided that you
     release the Modified Version under precisely this License, with
     the Modified Version filling the role of the Document, thus
     licensing distribution and modification of the Modified Version to
     whoever possesses a copy of it.  In addition, you must do these
     things in the Modified Version:

     A. Use in the Title Page (and on the covers, if any) a title
     distinct    from that of the Document, and from those of previous
     versions    (which should, if there were any, be listed in the
     History section    of the Document).  You may use the same title
     as a previous version    if the original publisher of that version
     gives permission.
     B. List on the Title Page, as authors, one or more persons or
     entities    responsible for authorship of the modifications in the
     Modified    Version, together with at least five of the principal
     authors of the    Document (all of its principal authors, if it
     has less than five).
     C. State on the Title page the name of the publisher of the
     Modified Version, as the publisher.
     D. Preserve all the copyright notices of the Document.
     E. Add an appropriate copyright notice for your modifications
     adjacent to the other copyright notices.
     F. Include, immediately after the copyright notices, a license
     notice    giving the public permission to use the Modified Version
     under the    terms of this License, in the form shown in the
     Addendum below.
     G. Preserve in that license notice the full lists of Invariant
     Sections    and required Cover Texts given in the Document's
     license notice.
     H. Include an unaltered copy of this License.
     I. Preserve the section entitled "History", and its title, and add
     to    it an item stating at least the title, year, new authors, and
       publisher of the Modified Version as given on the Title Page.
     If    there is no section entitled "History" in the Document,
     create one    stating the title, year, authors, and publisher of
     the Document as    given on its Title Page, then add an item
     describing the Modified    Version as stated in the previous
     sentence.
     J. Preserve the network location, if any, given in the Document for
       public access to a Transparent copy of the Document, and
     likewise    the network locations given in the Document for
     previous versions    it was based on.  These may be placed in the
     "History" section.     You may omit a network location for a work
     that was published at    least four years before the Document
     itself, or if the original    publisher of the version it refers
     to gives permission.
     K. In any section entitled "Acknowledgements" or "Dedications",
     preserve the section's title, and preserve in the section all the
      substance and tone of each of the contributor acknowledgements
     and/or dedications given therein.
     L. Preserve all the Invariant Sections of the Document,
     unaltered in their text and in their titles.  Section numbers
     or the equivalent are not considered part of the section titles.
     M. Delete any section entitled "Endorsements."  Such a section
     may not be included in the Modified Version.
     N. Do not retitle any existing section as "Endorsements"    or to
     conflict in title with any Invariant Section.

     If the Modified Version includes new front-matter sections or
     appendices that qualify as Secondary Sections and contain no
     material copied from the Document, you may at your option
     designate some or all of these sections as invariant.  To do this,
     add their titles to the list of Invariant Sections in the Modified
     Version's license notice.  These titles must be distinct from any
     other section titles.

     You may add a section entitled "Endorsements", provided it contains
     nothing but endorsements of your Modified Version by various
     parties-for example, statements of peer review or that the text has
     been approved by an organization as the authoritative definition
     of a standard.

     You may add a passage of up to five words as a Front-Cover Text,
     and a passage of up to 25 words as a Back-Cover Text, to the end
     of the list of Cover Texts in the Modified Version.  Only one
     passage of Front-Cover Text and one of Back-Cover Text may be
     added by (or through arrangements made by) any one entity.  If the
     Document already includes a cover text for the same cover,
     previously added by you or by arrangement made by the same entity
     you are acting on behalf of, you may not add another; but you may
     replace the old one, on explicit permission from the previous
     publisher that added the old one.

     The author(s) and publisher(s) of the Document do not by this
     License give permission to use their names for publicity for or to
     assert or imply endorsement of any Modified Version.

  5. COMBINING DOCUMENTS

     You may combine the Document with other documents released under
     this License, under the terms defined in section 4 above for
     modified versions, provided that you include in the combination
     all of the Invariant Sections of all of the original documents,
     unmodified, and list them all as Invariant Sections of your
     combined work in its license notice.

     The combined work need only contain one copy of this License, and
     multiple identical Invariant Sections may be replaced with a single
     copy.  If there are multiple Invariant Sections with the same name
     but different contents, make the title of each such section unique
     by adding at the end of it, in parentheses, the name of the
     original author or publisher of that section if known, or else a
     unique number.  Make the same adjustment to the section titles in
     the list of Invariant Sections in the license notice of the
     combined work.

     In the combination, you must combine any sections entitled
     "History" in the various original documents, forming one section
     entitled "History"; likewise combine any sections entitled
     "Acknowledgements", and any sections entitled "Dedications."  You
     must delete all sections entitled "Endorsements."

  6. COLLECTIONS OF DOCUMENTS

     You may make a collection consisting of the Document and other
     documents released under this License, and replace the individual
     copies of this License in the various documents with a single copy
     that is included in the collection, provided that you follow the
     rules of this License for verbatim copying of each of the
     documents in all other respects.

     You may extract a single document from such a collection, and
     distribute it individually under this License, provided you insert
     a copy of this License into the extracted document, and follow
     this License in all other respects regarding verbatim copying of
     that document.

  7. AGGREGATION WITH INDEPENDENT WORKS

     A compilation of the Document or its derivatives with other
     separate and independent documents or works, in or on a volume of
     a storage or distribution medium, does not as a whole count as a
     Modified Version of the Document, provided no compilation
     copyright is claimed for the compilation.  Such a compilation is
     called an "aggregate", and this License does not apply to the
     other self-contained works thus compiled with the Document, on
     account of their being thus compiled, if they are not themselves
     derivative works of the Document.

     If the Cover Text requirement of section 3 is applicable to these
     copies of the Document, then if the Document is less than one
     quarter of the entire aggregate, the Document's Cover Texts may be
     placed on covers that surround only the Document within the
     aggregate.  Otherwise they must appear on covers around the whole
     aggregate.

  8. TRANSLATION

     Translation is considered a kind of modification, so you may
     distribute translations of the Document under the terms of section
     4.  Replacing Invariant Sections with translations requires special
     permission from their copyright holders, but you may include
     translations of some or all Invariant Sections in addition to the
     original versions of these Invariant Sections.  You may include a
     translation of this License provided that you also include the
     original English version of this License.  In case of a
     disagreement between the translation and the original English
     version of this License, the original English version will prevail.

  9. TERMINATION

     You may not copy, modify, sublicense, or distribute the Document
     except as expressly provided for under this License.  Any other
     attempt to copy, modify, sublicense or distribute the Document is
     void, and will automatically terminate your rights under this
     License.  However, parties who have received copies, or rights,
     from you under this License will not have their licenses
     terminated so long as such parties remain in full compliance.

 10. FUTURE REVISIONS OF THIS LICENSE

     The Free Software Foundation may publish new, revised versions of
     the GNU Free Documentation License from time to time.  Such new
     versions will be similar in spirit to the present version, but may
     differ in detail to address new problems or concerns.  See
     http://www.gnu.org/copyleft/.

     Each version of the License is given a distinguishing version
     number.  If the Document specifies that a particular numbered
     version of this License "or any later version" applies to it, you
     have the option of following the terms and conditions either of
     that specified version or of any later version that has been
     published (not as a draft) by the Free Software Foundation.  If
     the Document does not specify a version number of this License,
     you may choose any version ever published (not as a draft) by the
     Free Software Foundation.


ADDENDUM: How to use this License for your documents
====================================================

   To use this License in a document you have written, include a copy of
the License in the document and put the following copyright and license
notices just after the title page:

     Copyright (C)  YEAR  YOUR NAME.
     Permission is granted to copy, distribute and/or modify this document
     under the terms of the GNU Free Documentation License, Version 1.1
     or any later version published by the Free Software Foundation;
     with the Invariant Sections being LIST THEIR TITLES, with the
     Front-Cover Texts being LIST, and with the Back-Cover Texts being LIST.
     A copy of the license is included in the section entitled "GNU
     Free Documentation License."

   If you have no Invariant Sections, write "with no Invariant Sections"
instead of saying which ones are invariant.  If you have no Front-Cover
Texts, write "no Front-Cover Texts" instead of "Front-Cover Texts being
LIST"; likewise for Back-Cover Texts.

   If your document contains nontrivial examples of program code, we
recommend releasing these examples in parallel under your choice of
free software license, such as the GNU General Public License, to
permit their use in free software.


File: gdbint.info,  Node: Index,  Prev: GNU Free Documentation License,  Up: Top

Index
*****

* Menu:

* *gdbarch_data:                         Coding.
* _initialize_language:                  Language Support.
* a.out format:                          Symbol Handling.
* add_cmd:                               User Interface.
* add_com:                               User Interface.
* add_setshow_cmd:                       User Interface.
* add_setshow_cmd_full:                  User Interface.
* add_symtab_fns:                        Symbol Handling.
* adding a new host:                     Host Definition.
* adding a symbol-reading module:        Symbol Handling.
* adding a target:                       Target Architecture Definition.
* adding debugging info reader:          Symbol Handling.
* adding source language:                Language Support.
* ADDITIONAL_OPTION_CASES:               Target Architecture Definition.
* ADDITIONAL_OPTION_HANDLER:             Target Architecture Definition.
* ADDITIONAL_OPTION_HELP:                Target Architecture Definition.
* ADDITIONAL_OPTIONS:                    Target Architecture Definition.
* ADDR_BITS_REMOVE:                      Target Architecture Definition.
* address representation:                Target Architecture Definition.
* address spaces, separate data and code: Target Architecture Definition.
* ADDRESS_TO_POINTER:                    Target Architecture Definition.
* algorithms:                            Algorithms.
* ALIGN_STACK_ON_STARTUP:                Host Definition.
* allocate_symtab:                       Language Support.
* assumptions about targets:             Coding.
* ATTACH_DETACH:                         Native Debugging.
* ATTR_NORETURN:                         Host Definition.
* BEFORE_MAIN_LOOP_HOOK:                 Target Architecture Definition.
* BELIEVE_PCC_PROMOTION:                 Target Architecture Definition.
* BELIEVE_PCC_PROMOTION_TYPE:            Target Architecture Definition.
* BFD library:                           Support Libraries.
* BIG_BREAKPOINT:                        Target Architecture Definition.
* BIG_REMOTE_BREAKPOINT:                 Target Architecture Definition.
* BITS_BIG_ENDIAN:                       Target Architecture Definition.
* BPT_VECTOR:                            Target Architecture Definition.
* BREAKPOINT <1>:                        Algorithms.
* BREAKPOINT:                            Target Architecture Definition.
* BREAKPOINT_FROM_PC:                    Target Architecture Definition.
* breakpoints:                           Algorithms.
* bug-gdb mailing list:                  Getting Started.
* C data types:                          Coding.
* call stack frame:                      Algorithms.
* CALL_DUMMY:                            Target Architecture Definition.
* CALL_DUMMY_LOCATION:                   Target Architecture Definition.
* CALL_DUMMY_P:                          Target Architecture Definition.
* CALL_DUMMY_STACK_ADJUST:               Target Architecture Definition.
* CALL_DUMMY_STACK_ADJUST_P:             Target Architecture Definition.
* CALL_DUMMY_WORDS:                      Target Architecture Definition.
* call_function_by_hand:                 Target Architecture Definition.
* CANNOT_FETCH_REGISTER:                 Target Architecture Definition.
* CANNOT_STEP_HW_WATCHPOINTS:            Algorithms.
* CANNOT_STORE_REGISTER:                 Target Architecture Definition.
* CC_HAS_LONG_LONG:                      Host Definition.
* char:                                  Target Architecture Definition.
* CHILD_PREPARE_TO_STORE:                Native Debugging.
* cleanup:                               User Interface.
* cleanups:                              Coding.
* CLEAR_DEFERRED_STORES:                 Target Architecture Definition.
* CLEAR_SOLIB:                           Native Debugging.
* CLI:                                   User Interface.
* code pointers, word-addressed:         Target Architecture Definition.
* coding standards:                      Coding.
* COERCE_FLOAT_TO_DOUBLE:                Target Architecture Definition.
* COFF debugging info:                   Symbol Handling.
* COFF format:                           Symbol Handling.
* command implementation:                Getting Started.
* command interpreter:                   User Interface.
* comment formatting:                    Coding.
* compiler warnings:                     Coding.
* CONVERT_REGISTER_P:                    Target Architecture Definition.
* converting between pointers and addresses: Target Architecture Definition.
* converting integers to addresses:      Target Architecture Definition.
* converting targets to multi-arch:      Target Architecture Definition.
* CPLUS_MARKERz:                         Target Architecture Definition.
* create_new_frame:                      Algorithms.
* CRLF_SOURCE_FILES:                     Host Definition.
* current_language:                      Language Support.
* D10V addresses:                        Target Architecture Definition.
* data output:                           User Interface.
* data-pointer, per-architecture/per-module: Coding.
* DBX_PARM_SYMBOL_CLASS:                 Target Architecture Definition.
* DEBUG_PTRACE:                          Native Debugging.
* debugging GDB:                         Debugging GDB.
* DECR_PC_AFTER_BREAK:                   Target Architecture Definition.
* DECR_PC_AFTER_HW_BREAK <1>:            Target Architecture Definition.
* DECR_PC_AFTER_HW_BREAK:                Algorithms.
* default_coerce_float_to_double:        Target Architecture Definition.
* DEFAULT_PROMPT:                        Host Definition.
* deprecate_cmd:                         User Interface.
* deprecating commands:                  User Interface.
* design:                                Coding.
* DEV_TTY:                               Host Definition.
* DIRNAME_SEPARATOR:                     Coding.
* DISABLE_UNSETTABLE_BREAK:              Target Architecture Definition.
* discard_cleanups:                      Coding.
* do_cleanups:                           Coding.
* DO_DEFERRED_STORES:                    Target Architecture Definition.
* DO_REGISTERS_INFO:                     Target Architecture Definition.
* DOS text files:                        Host Definition.
* DWARF 1 debugging info:                Symbol Handling.
* DWARF 2 debugging info:                Symbol Handling.
* DWARF2_REG_TO_REGNUM:                  Target Architecture Definition.
* DWARF_REG_TO_REGNUM:                   Target Architecture Definition.
* ECOFF debugging info:                  Symbol Handling.
* ECOFF format:                          Symbol Handling.
* ECOFF_REG_TO_REGNUM:                   Target Architecture Definition.
* ELF format:                            Symbol Handling.
* END_OF_TEXT_DEFAULT:                   Target Architecture Definition.
* evaluate_subexp:                       Language Support.
* expression evaluation routines:        Language Support.
* expression parser:                     Language Support.
* extract_address:                       Target Architecture Definition.
* EXTRACT_RETURN_VALUE:                  Target Architecture Definition.
* EXTRACT_STRUCT_VALUE_ADDRESS:          Target Architecture Definition.
* EXTRACT_STRUCT_VALUE_ADDRESS_P:        Target Architecture Definition.
* extract_typed_address:                 Target Architecture Definition.
* FCLOSE_PROVIDED:                       Host Definition.
* fetch_core_registers:                  Native Debugging.
* FETCH_INFERIOR_REGISTERS:              Native Debugging.
* field output functions:                User Interface.
* file names, portability:               Coding.
* FILENAME_CMP:                          Coding.
* FILES_INFO_HOOK:                       Native Debugging.
* find_pc_function:                      Symbol Handling.
* find_pc_line:                          Symbol Handling.
* find_sym_fns:                          Symbol Handling.
* finding a symbol:                      Symbol Handling.
* fine-tuning gdbarch structure:         Target Architecture Definition.
* float arguments:                       Target Architecture Definition.
* FLOAT_INFO:                            Target Architecture Definition.
* FOPEN_RB:                              Host Definition.
* FP0_REGNUM:                            Native Debugging.
* FP_REGNUM:                             Target Architecture Definition.
* frame:                                 Algorithms.
* frame chain:                           Algorithms.
* frame pointer register:                Algorithms.
* FRAME_ARGS_ADDRESS_CORRECT:            Target Architecture Definition.
* FRAME_CHAIN:                           Target Architecture Definition.
* FRAME_CHAIN_VALID:                     Target Architecture Definition.
* FRAME_FP:                              Algorithms.
* FRAME_INIT_SAVED_REGS:                 Target Architecture Definition.
* FRAME_NUM_ARGS:                        Target Architecture Definition.
* FRAME_SAVED_PC:                        Target Architecture Definition.
* FRAMELESS_FUNCTION_INVOCATION:         Target Architecture Definition.
* full symbol table:                     Symbol Handling.
* function prototypes:                   Coding.
* function usage:                        Coding.
* FUNCTION_EPILOGUE_SIZE:                Target Architecture Definition.
* FUNCTION_START_OFFSET:                 Target Architecture Definition.
* fundamental types:                     Symbol Handling.
* GCC2_COMPILED_FLAG_SYMBOL:             Target Architecture Definition.
* GCC_COMPILED_FLAG_SYMBOL:              Target Architecture Definition.
* GDB_MULTI_ARCH:                        Target Architecture Definition.
* gdb_osabi:                             Target Architecture Definition.
* GDB_OSABI_ARM_APCS:                    Target Architecture Definition.
* GDB_OSABI_ARM_EABI_V1:                 Target Architecture Definition.
* GDB_OSABI_ARM_EABI_V2:                 Target Architecture Definition.
* GDB_OSABI_FREEBSD_AOUT:                Target Architecture Definition.
* GDB_OSABI_FREEBSD_ELF:                 Target Architecture Definition.
* GDB_OSABI_GO32:                        Target Architecture Definition.
* GDB_OSABI_HURD:                        Target Architecture Definition.
* GDB_OSABI_LINUX:                       Target Architecture Definition.
* GDB_OSABI_NETBSD_AOUT:                 Target Architecture Definition.
* GDB_OSABI_NETBSD_ELF:                  Target Architecture Definition.
* GDB_OSABI_NETWARE:                     Target Architecture Definition.
* GDB_OSABI_OSF1:                        Target Architecture Definition.
* GDB_OSABI_SOLARIS:                     Target Architecture Definition.
* GDB_OSABI_SVR4:                        Target Architecture Definition.
* GDB_OSABI_UNKNOWN:                     Target Architecture Definition.
* GDB_OSABI_WINCE:                       Target Architecture Definition.
* GDB_TARGET_IS_HPPA:                    Target Architecture Definition.
* gdbarch_data:                          Coding.
* gdbarch_in_function_epilogue_p:        Target Architecture Definition.
* gdbarch_init_osabi:                    Target Architecture Definition.
* gdbarch_register_osabi:                Target Architecture Definition.
* gdbarch_register_osabi_sniffer:        Target Architecture Definition.
* GDBINIT_FILENAME:                      Host Definition.
* generic dummy frames:                  Host Definition.
* generic host support:                  Host Definition.
* GET_LONGJMP_TARGET <1>:                Target Architecture Definition.
* GET_LONGJMP_TARGET <2>:                Algorithms.
* GET_LONGJMP_TARGET:                    Native Debugging.
* GET_SAVED_REGISTER:                    Target Architecture Definition.
* get_saved_register:                    Target Architecture Definition.
* GETENV_PROVIDED:                       Host Definition.
* hardware breakpoints:                  Algorithms.
* hardware watchpoints:                  Algorithms.
* HAVE_CONTINUABLE_WATCHPOINT:           Algorithms.
* HAVE_DOS_BASED_FILE_SYSTEM:            Coding.
* HAVE_LONG_DOUBLE:                      Host Definition.
* HAVE_MMAP:                             Host Definition.
* HAVE_NONSTEPPABLE_WATCHPOINT:          Algorithms.
* HAVE_STEPPABLE_WATCHPOINT:             Algorithms.
* HAVE_TERMIO:                           Host Definition.
* host:                                  Overall Structure.
* host, adding:                          Host Definition.
* i386_cleanup_dregs:                    Algorithms.
* I386_DR_LOW_GET_STATUS:                Algorithms.
* I386_DR_LOW_RESET_ADDR:                Algorithms.
* I386_DR_LOW_SET_ADDR:                  Algorithms.
* I386_DR_LOW_SET_CONTROL:               Algorithms.
* i386_insert_hw_breakpoint:             Algorithms.
* i386_insert_watchpoint:                Algorithms.
* i386_region_ok_for_watchpoint:         Algorithms.
* i386_remove_hw_breakpoint:             Algorithms.
* i386_remove_watchpoint:                Algorithms.
* i386_stopped_by_hwbp:                  Algorithms.
* i386_stopped_data_address:             Algorithms.
* I386_USE_GENERIC_WATCHPOINTS:          Algorithms.
* IBM6000_TARGET:                        Target Architecture Definition.
* IN_SOLIB_CALL_TRAMPOLINE:              Target Architecture Definition.
* IN_SOLIB_DYNSYM_RESOLVE_CODE:          Target Architecture Definition.
* IN_SOLIB_RETURN_TRAMPOLINE:            Target Architecture Definition.
* INIT_EXTRA_FRAME_INFO:                 Target Architecture Definition.
* INIT_FRAME_PC:                         Target Architecture Definition.
* INNER_THAN:                            Target Architecture Definition.
* insert or remove hardware breakpoint:  Algorithms.
* INT_MAX:                               Host Definition.
* INT_MIN:                               Host Definition.
* INTEGER_TO_ADDRESS:                    Target Architecture Definition.
* IS_ABSOLUTE_PATH:                      Coding.
* IS_DIR_SEPARATOR:                      Coding.
* IS_TRAPPED_INTERNALVAR:                Target Architecture Definition.
* ISATTY:                                Host Definition.
* item output functions:                 User Interface.
* KERNEL_U_ADDR:                         Native Debugging.
* KERNEL_U_ADDR_BSD:                     Native Debugging.
* KERNEL_U_ADDR_HPUX:                    Native Debugging.
* L_SET:                                 Host Definition.
* language parser:                       Language Support.
* language support:                      Language Support.
* legal papers for code contributions:   Debugging GDB.
* length_of_subexp:                      Language Support.
* libgdb:                                libgdb.
* line wrap in output:                   Coding.
* lint:                                  Host Definition.
* list output functions:                 User Interface.
* LITTLE_BREAKPOINT:                     Target Architecture Definition.
* LITTLE_REMOTE_BREAKPOINT:              Target Architecture Definition.
* long long data type:                   Host Definition.
* LONG_MAX:                              Host Definition.
* LONGEST:                               Host Definition.
* longjmp debugging:                     Algorithms.
* lookup_symbol:                         Symbol Handling.
* LSEEK_NOT_LINEAR:                      Host Definition.
* make_cleanup:                          Coding.
* making a distribution tarball:         Porting GDB.
* making a new release of gdb:           Releasing GDB.
* memory representation:                 Target Architecture Definition.
* MEMORY_INSERT_BREAKPOINT:              Target Architecture Definition.
* MEMORY_REMOVE_BREAKPOINT:              Target Architecture Definition.
* minimal symbol table:                  Symbol Handling.
* minsymtabs:                            Symbol Handling.
* mmalloc:                               Host Definition.
* mmap:                                  Host Definition.
* MMAP_BASE_ADDRESS:                     Host Definition.
* MMAP_INCREMENT:                        Host Definition.
* mmcheck:                               Host Definition.
* MMCHECK_FORCE:                         Host Definition.
* multi-arch data:                       Coding.
* NATDEPFILES:                           Native Debugging.
* native conditionals:                   Native Debugging.
* native core files:                     Native Debugging.
* native debugging:                      Native Debugging.
* NEED_TEXT_START_END:                   Target Architecture Definition.
* nesting level in ui_out functions:     User Interface.
* Netware Loadable Module format:        Symbol Handling.
* NO_HIF_SUPPORT:                        Target Architecture Definition.
* NO_MMCHECK:                            Host Definition.
* NO_SIGINTERRUPT:                       Host Definition.
* NO_STD_REGS:                           Host Definition.
* NO_SYS_FILE:                           Host Definition.
* NORETURN:                              Host Definition.
* NPC_REGNUM:                            Target Architecture Definition.
* object file formats:                   Symbol Handling.
* obsolete code:                         Debugging GDB.
* ONE_PROCESS_WRITETEXT:                 Native Debugging.
* op_print_tab:                          Language Support.
* opcodes library:                       Support Libraries.
* OS ABI variants:                       Target Architecture Definition.
* OS9K_VARIABLES_INSIDE_BLOCK:           Target Architecture Definition.
* PARM_BOUNDARY:                         Target Architecture Definition.
* parse_exp_1:                           Language Support.
* partial symbol table:                  Symbol Handling.
* passing arguments to prototyped functions: Target Architecture Definition.
* PC_IN_CALL_DUMMY:                      Target Architecture Definition.
* PC_IN_SIGTRAMP:                        Target Architecture Definition.
* PC_LOAD_SEGMENT:                       Target Architecture Definition.
* PC_REGNUM:                             Target Architecture Definition.
* PCC_SOL_BROKEN:                        Target Architecture Definition.
* PE-COFF format:                        Symbol Handling.
* per-architecture module data:          Coding.
* pointer representation:                Target Architecture Definition.
* POINTER_TO_ADDRESS:                    Target Architecture Definition.
* POP_FRAME:                             Target Architecture Definition.
* portability:                           Coding.
* portable file name handling:           Coding.
* porting to new machines:               Porting GDB.
* prefixify_subexp:                      Language Support.
* PREPARE_TO_PROCEED:                    Native Debugging.
* preparing a release:                   Porting GDB.
* PRINT_FLOAT_INFO:                      Target Architecture Definition.
* PRINT_REGISTER_HOOK:                   Target Architecture Definition.
* print_registers_info:                  Target Architecture Definition.
* print_subexp:                          Language Support.
* PRINT_TYPELESS_INTEGER:                Target Architecture Definition.
* PRINT_VECTOR_INFO:                     Target Architecture Definition.
* PRINTF_HAS_LONG_DOUBLE:                Host Definition.
* PRINTF_HAS_LONG_LONG:                  Host Definition.
* PROC_NAME_FMT:                         Native Debugging.
* PROCESS_LINENUMBER_HOOK:               Target Architecture Definition.
* program counter:                       Algorithms.
* PROLOGUE_FIRSTLINE_OVERLAP:            Target Architecture Definition.
* promotion to double:                   Target Architecture Definition.
* prompt:                                Host Definition.
* prototyped functions, passing arguments to: Target Architecture Definition.
* PS_REGNUM:                             Target Architecture Definition.
* psymtabs:                              Symbol Handling.
* PTRACE_ARG3_TYPE:                      Native Debugging.
* PTRACE_FP_BUG:                         Native Debugging.
* PUSH_ARGUMENTS:                        Target Architecture Definition.
* PUSH_DUMMY_FRAME:                      Target Architecture Definition.
* raw register representation:           Target Architecture Definition.
* read_fp:                               Target Architecture Definition.
* read_pc:                               Target Architecture Definition.
* read_sp:                               Target Architecture Definition.
* reading of symbols:                    Symbol Handling.
* REG_STRUCT_HAS_ADDR:                   Target Architecture Definition.
* register data formats, converting:     Target Architecture Definition.
* register representation:               Target Architecture Definition.
* REGISTER_BYTES:                        Target Architecture Definition.
* REGISTER_CONVERT_TO_RAW:               Target Architecture Definition.
* REGISTER_CONVERT_TO_TYPE:              Target Architecture Definition.
* REGISTER_CONVERT_TO_VIRTUAL:           Target Architecture Definition.
* REGISTER_CONVERTIBLE:                  Target Architecture Definition.
* REGISTER_NAME:                         Target Architecture Definition.
* REGISTER_NAMES:                        Target Architecture Definition.
* REGISTER_RAW_SIZE:                     Target Architecture Definition.
* REGISTER_TO_VALUE:                     Target Architecture Definition.
* REGISTER_U_ADDR:                       Native Debugging.
* REGISTER_VIRTUAL_SIZE:                 Target Architecture Definition.
* REGISTER_VIRTUAL_TYPE:                 Target Architecture Definition.
* regular expressions library:           Support Libraries.
* remote debugging support:              Host Definition.
* REMOTE_BPT_VECTOR:                     Target Architecture Definition.
* REMOTE_BREAKPOINT:                     Target Architecture Definition.
* representations, raw and virtual registers: Target Architecture Definition.
* representations, register and memory:  Target Architecture Definition.
* requirements for GDB:                  Requirements.
* return_command:                        Target Architecture Definition.
* RETURN_VALUE_ON_STACK:                 Target Architecture Definition.
* returning structures by value:         Target Architecture Definition.
* running the test suite:                Testsuite.
* SAVE_DUMMY_FRAME_TOS:                  Target Architecture Definition.
* SCANF_HAS_LONG_DOUBLE:                 Host Definition.
* SDB_REG_TO_REGNUM:                     Target Architecture Definition.
* secondary symbol file:                 Symbol Handling.
* SEEK_CUR:                              Host Definition.
* SEEK_SET:                              Host Definition.
* separate data and code address spaces: Target Architecture Definition.
* serial line support:                   Host Definition.
* set_gdbarch_data:                      Coding.
* SHELL_COMMAND_CONCAT:                  Native Debugging.
* SHELL_FILE:                            Native Debugging.
* siginterrupt:                          Host Definition.
* sigtramp:                              Target Architecture Definition.
* SIGTRAMP_END:                          Target Architecture Definition.
* SIGTRAMP_START:                        Target Architecture Definition.
* SIGWINCH_HANDLER:                      Host Definition.
* SIGWINCH_HANDLER_BODY:                 Host Definition.
* SIZEOF_CALL_DUMMY_WORDS:               Target Architecture Definition.
* SKIP_PERMANENT_BREAKPOINT:             Target Architecture Definition.
* SKIP_PROLOGUE:                         Target Architecture Definition.
* SKIP_SOLIB_RESOLVER:                   Target Architecture Definition.
* SKIP_TRAMPOLINE_CODE:                  Target Architecture Definition.
* SLASH_STRING:                          Coding.
* software breakpoints:                  Algorithms.
* software watchpoints:                  Algorithms.
* SOFTWARE_SINGLE_STEP:                  Target Architecture Definition.
* SOFTWARE_SINGLE_STEP_P:                Target Architecture Definition.
* SOFUN_ADDRESS_MAYBE_MISSING:           Target Architecture Definition.
* SOLIB_ADD:                             Native Debugging.
* SOLIB_CREATE_INFERIOR_HOOK:            Native Debugging.
* SOM debugging info:                    Symbol Handling.
* SOM format:                            Symbol Handling.
* source code formatting:                Coding.
* SP_REGNUM:                             Target Architecture Definition.
* spaces, separate data and code address: Target Architecture Definition.
* STAB_REG_TO_REGNUM:                    Target Architecture Definition.
* stabs debugging info:                  Symbol Handling.
* stack alignment:                       Host Definition.
* STACK_ALIGN:                           Target Architecture Definition.
* standard_coerce_float_to_double:       Target Architecture Definition.
* START_INFERIOR_TRAPS_EXPECTED:         Native Debugging.
* STEP_SKIPS_DELAY:                      Target Architecture Definition.
* STOP_SIGNAL:                           Host Definition.
* STOPPED_BY_WATCHPOINT:                 Algorithms.
* store_address:                         Target Architecture Definition.
* STORE_RETURN_VALUE:                    Target Architecture Definition.
* store_typed_address:                   Target Architecture Definition.
* struct value, converting register contents to: Target Architecture Definition.
* structures, returning by value:        Target Architecture Definition.
* submitting patches:                    Debugging GDB.
* SUN_FIXED_LBRAC_BUG:                   Target Architecture Definition.
* SVR4_SHARED_LIBS:                      Native Debugging.
* sym_fns structure:                     Symbol Handling.
* symbol files:                          Symbol Handling.
* symbol lookup:                         Symbol Handling.
* symbol reading:                        Symbol Handling.
* SYMBOL_RELOADING_DEFAULT:              Target Architecture Definition.
* SYMBOLS_CAN_START_WITH_DOLLAR:         Target Architecture Definition.
* symtabs:                               Symbol Handling.
* system dependencies:                   Coding.
* table output functions:                User Interface.
* target:                                Overall Structure.
* target architecture definition:        Target Architecture Definition.
* target vector:                         Target Vector Definition.
* TARGET_CAN_USE_HARDWARE_WATCHPOINT:    Algorithms.
* TARGET_CHAR_BIT:                       Target Architecture Definition.
* TARGET_CHAR_SIGNED:                    Target Architecture Definition.
* TARGET_COMPLEX_BIT:                    Target Architecture Definition.
* TARGET_DISABLE_HW_WATCHPOINTS:         Algorithms.
* TARGET_DOUBLE_BIT:                     Target Architecture Definition.
* TARGET_DOUBLE_COMPLEX_BIT:             Target Architecture Definition.
* TARGET_ENABLE_HW_WATCHPOINTS:          Algorithms.
* TARGET_FLOAT_BIT:                      Target Architecture Definition.
* TARGET_HAS_HARDWARE_WATCHPOINTS:       Algorithms.
* target_insert_hw_breakpoint:           Algorithms.
* target_insert_watchpoint:              Algorithms.
* TARGET_INT_BIT:                        Target Architecture Definition.
* TARGET_LONG_BIT:                       Target Architecture Definition.
* TARGET_LONG_DOUBLE_BIT:                Target Architecture Definition.
* TARGET_LONG_LONG_BIT:                  Target Architecture Definition.
* TARGET_PRINT_INSN:                     Target Architecture Definition.
* TARGET_PTR_BIT:                        Target Architecture Definition.
* TARGET_READ_FP:                        Target Architecture Definition.
* TARGET_READ_PC:                        Target Architecture Definition.
* TARGET_READ_SP:                        Target Architecture Definition.
* TARGET_REGION_OK_FOR_HW_WATCHPOINT:    Algorithms.
* TARGET_REGION_SIZE_OK_FOR_HW_WATCHPOINT: Algorithms.
* target_remove_hw_breakpoint:           Algorithms.
* target_remove_watchpoint:              Algorithms.
* TARGET_SHORT_BIT:                      Target Architecture Definition.
* target_stopped_data_address:           Algorithms.
* TARGET_VIRTUAL_FRAME_POINTER:          Target Architecture Definition.
* TARGET_WRITE_PC:                       Target Architecture Definition.
* TARGET_WRITE_SP:                       Target Architecture Definition.
* TCP remote support:                    Host Definition.
* TDEPFILES:                             Target Architecture Definition.
* terminal device:                       Host Definition.
* test suite:                            Testsuite.
* test suite organization:               Testsuite.
* trimming language-dependent code:      Language Support.
* tuple output functions:                User Interface.
* type:                                  Target Architecture Definition.
* type codes:                            Symbol Handling.
* types:                                 Coding.
* U_REGS_OFFSET:                         Native Debugging.
* ui_out functions:                      User Interface.
* ui_out functions, usage examples:      User Interface.
* ui_out_field_core_addr:                User Interface.
* ui_out_field_fmt:                      User Interface.
* ui_out_field_int:                      User Interface.
* ui_out_field_skip:                     User Interface.
* ui_out_field_stream:                   User Interface.
* ui_out_field_string:                   User Interface.
* ui_out_flush:                          User Interface.
* ui_out_list_begin:                     User Interface.
* ui_out_list_end:                       User Interface.
* ui_out_message:                        User Interface.
* ui_out_spaces:                         User Interface.
* ui_out_stream_delete:                  User Interface.
* ui_out_table_begin:                    User Interface.
* ui_out_table_body:                     User Interface.
* ui_out_table_end:                      User Interface.
* ui_out_table_header:                   User Interface.
* ui_out_text:                           User Interface.
* ui_out_tuple_begin:                    User Interface.
* ui_out_tuple_end:                      User Interface.
* ui_out_wrap_hint:                      User Interface.
* ui_stream:                             User Interface.
* UINT_MAX:                              Host Definition.
* ULONG_MAX:                             Host Definition.
* USE_GENERIC_DUMMY_FRAMES:              Host Definition.
* USE_MMALLOC:                           Host Definition.
* USE_O_NOCTTY:                          Host Definition.
* USE_PROC_FS:                           Native Debugging.
* USE_STRUCT_CONVENTION:                 Target Architecture Definition.
* USG:                                   Host Definition.
* using ui_out functions:                User Interface.
* value_as_address:                      Target Architecture Definition.
* value_from_pointer:                    Target Architecture Definition.
* VALUE_TO_REGISTER:                     Target Architecture Definition.
* VARIABLES_INSIDE_BLOCK:                Target Architecture Definition.
* virtual register representation:       Target Architecture Definition.
* volatile:                              Host Definition.
* watchpoints:                           Algorithms.
* watchpoints, on x86:                   Algorithms.
* word-addressed machines:               Target Architecture Definition.
* wrap_here:                             Coding.
* write_pc:                              Target Architecture Definition.
* write_sp:                              Target Architecture Definition.
* writing tests:                         Testsuite.
* x86 debug registers:                   Algorithms.
* XCOFF format:                          Symbol Handling.



Tag Table:
Node: Top997
Node: Requirements1728
Node: Overall Structure3215
Node: Algorithms6485
Node: User Interface24868
Ref: User Interface-Footnote-148183
Ref: User Interface-Footnote-248232
Node: libgdb48467
Node: Symbol Handling52425
Node: Language Support66571
Node: Host Definition71966
Node: Target Architecture Definition81910
Ref: Target Architecture Definition-Footnote-1144519
Ref: Target Architecture Definition-Footnote-2144762
Node: Target Vector Definition144881
Node: Native Debugging147449
Node: Support Libraries159071
Node: Coding160781
Node: Porting GDB185856
Node: Releasing GDB189049
Node: Testsuite210775
Node: Hints217260
Node: Getting Started217596
Node: Debugging GDB221732
Node: GNU Free Documentation License227072
Node: Index246767

End Tag Table
