This is doc/gcc.info, produced by makeinfo version 4.2 from
doc/gcc.texi.

INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* gcc: (gcc).                  The GNU Compiler Collection.
END-INFO-DIR-ENTRY
   This file documents the use of the GNU compilers.

   Published by the Free Software Foundation
59 Temple Place - Suite 330
Boston, MA 02111-1307 USA

   Copyright (C) 1988, 1989, 1992, 1993, 1994, 1995, 1996, 1997, 1998,
1999, 2000, 2001, 2002 Free Software Foundation, Inc.

   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.1 or
any later version published by the Free Software Foundation; with the
Invariant Sections being "GNU General Public License" and "Funding Free
Software", the Front-Cover texts being (a) (see below), and with the
Back-Cover Texts being (b) (see below).  A copy of the license is
included in the section entitled "GNU Free Documentation License".

   (a) The FSF's Front-Cover Text is:

   A GNU Manual

   (b) The FSF's Back-Cover Text is:

   You have freedom to copy and modify this GNU Manual, like GNU
software.  Copies published by the Free Software Foundation raise
funds for GNU development.


File: gcc.info,  Node: MIPS Options,  Next: i386 and x86-64 Options,  Prev: RT Options,  Up: Submodel Options

MIPS Options
------------

   These `-m' options are defined for the MIPS family of computers:

`-march=CPU-TYPE'
     Assume the defaults for the machine type CPU-TYPE when generating
     instructions.  The choices for CPU-TYPE are  `r2000', `r3000',
     `r3900', `r4000', `r4100', `r4300', `r4400', `r4600', `r4650',
     `r5000', `r6000', `r8000', and `orion'.  Additionally, the
     `r2000', `r3000', `r4000', `r5000', and `r6000' can be abbreviated
     as `r2k' (or `r2K'), `r3k', etc.

`-mtune=CPU-TYPE'
     Assume the defaults for the machine type CPU-TYPE when scheduling
     instructions.  The choices for CPU-TYPE are `r2000', `r3000',
     `r3900', `r4000', `r4100', `r4300', `r4400', `r4600', `r4650',
     `r5000', `r6000', `r8000', and `orion'.  Additionally, the
     `r2000', `r3000', `r4000', `r5000', and `r6000' can be abbreviated
     as `r2k' (or `r2K'), `r3k', etc.  While picking a specific
     CPU-TYPE will schedule things appropriately for that particular
     chip, the compiler will not generate any code that does not meet
     level 1 of the MIPS ISA (instruction set architecture) without a
     `-mipsX' or `-mabi' switch being used.

`-mcpu=CPU-TYPE'
     This is identical to specifying both `-march' and `-mtune'.

`-mips1'
     Issue instructions from level 1 of the MIPS ISA.  This is the
     default.  `r3000' is the default CPU-TYPE at this ISA level.

`-mips2'
     Issue instructions from level 2 of the MIPS ISA (branch likely,
     square root instructions).  `r6000' is the default CPU-TYPE at this
     ISA level.

`-mips3'
     Issue instructions from level 3 of the MIPS ISA (64-bit
     instructions).  `r4000' is the default CPU-TYPE at this ISA level.

`-mips4'
     Issue instructions from level 4 of the MIPS ISA (conditional move,
     prefetch, enhanced FPU instructions).  `r8000' is the default
     CPU-TYPE at this ISA level.

`-mfp32'
     Assume that 32 32-bit floating point registers are available.
     This is the default.

`-mfp64'
     Assume that 32 64-bit floating point registers are available.
     This is the default when the `-mips3' option is used.

`-mfused-madd'
`-mno-fused-madd'
     Generate code that uses (does not use) the floating point multiply
     and accumulate instructions, when they are available.  These
     instructions are generated by default if they are available, but
     this may be undesirable if the extra precision causes problems or
     on certain chips in the mode where denormals are rounded to zero
     where denormals generated by multiply and accumulate instructions
     cause exceptions anyway.

`-mgp32'
     Assume that 32 32-bit general purpose registers are available.
     This is the default.

`-mgp64'
     Assume that 32 64-bit general purpose registers are available.
     This is the default when the `-mips3' option is used.

`-mint64'
     Force int and long types to be 64 bits wide.  See `-mlong32' for an
     explanation of the default, and the width of pointers.

`-mlong64'
     Force long types to be 64 bits wide.  See `-mlong32' for an
     explanation of the default, and the width of pointers.

`-mlong32'
     Force long, int, and pointer types to be 32 bits wide.

     If none of `-mlong32', `-mlong64', or `-mint64' are set, the size
     of ints, longs, and pointers depends on the ABI and ISA chosen.
     For `-mabi=32', and `-mabi=n32', ints and longs are 32 bits wide.
     For `-mabi=64', ints are 32 bits, and longs are 64 bits wide.  For
     `-mabi=eabi' and either `-mips1' or `-mips2', ints and longs are
     32 bits wide.  For `-mabi=eabi' and higher ISAs, ints are 32 bits,
     and longs are 64 bits wide.  The width of pointer types is the
     smaller of the width of longs or the width of general purpose
     registers (which in turn depends on the ISA).

`-mabi=32'
`-mabi=o64'
`-mabi=n32'
`-mabi=64'
`-mabi=eabi'
     Generate code for the indicated ABI.  The default instruction
     level is `-mips1' for `32', `-mips3' for `n32', and `-mips4'
     otherwise.  Conversely, with `-mips1' or `-mips2', the default ABI
     is `32'; otherwise, the default ABI is `64'.

`-mmips-as'
     Generate code for the MIPS assembler, and invoke `mips-tfile' to
     add normal debug information.  This is the default for all
     platforms except for the OSF/1 reference platform, using the
     OSF/rose object format.  If the either of the `-gstabs' or
     `-gstabs+' switches are used, the `mips-tfile' program will
     encapsulate the stabs within MIPS ECOFF.

`-mgas'
     Generate code for the GNU assembler.  This is the default on the
     OSF/1 reference platform, using the OSF/rose object format.  Also,
     this is the default if the configure option `--with-gnu-as' is
     used.

`-msplit-addresses'
`-mno-split-addresses'
     Generate code to load the high and low parts of address constants
     separately.  This allows GCC to optimize away redundant loads of
     the high order bits of addresses.  This optimization requires GNU
     as and GNU ld.  This optimization is enabled by default for some
     embedded targets where GNU as and GNU ld are standard.

`-mrnames'
`-mno-rnames'
     The `-mrnames' switch says to output code using the MIPS software
     names for the registers, instead of the hardware names (ie, A0
     instead of $4).  The only known assembler that supports this option
     is the Algorithmics assembler.

`-mgpopt'
`-mno-gpopt'
     The `-mgpopt' switch says to write all of the data declarations
     before the instructions in the text section, this allows the MIPS
     assembler to generate one word memory references instead of using
     two words for short global or static data items.  This is on by
     default if optimization is selected.

`-mstats'
`-mno-stats'
     For each non-inline function processed, the `-mstats' switch
     causes the compiler to emit one line to the standard error file to
     print statistics about the program (number of registers saved,
     stack size, etc.).

`-mmemcpy'
`-mno-memcpy'
     The `-mmemcpy' switch makes all block moves call the appropriate
     string function (`memcpy' or `bcopy') instead of possibly
     generating inline code.

`-mmips-tfile'
`-mno-mips-tfile'
     The `-mno-mips-tfile' switch causes the compiler not postprocess
     the object file with the `mips-tfile' program, after the MIPS
     assembler has generated it to add debug support.  If `mips-tfile'
     is not run, then no local variables will be available to the
     debugger.  In addition, `stage2' and `stage3' objects will have
     the temporary file names passed to the assembler embedded in the
     object file, which means the objects will not compare the same.
     The `-mno-mips-tfile' switch should only be used when there are
     bugs in the `mips-tfile' program that prevents compilation.

`-msoft-float'
     Generate output containing library calls for floating point.
     *Warning:* the requisite libraries are not part of GCC.  Normally
     the facilities of the machine's usual C compiler are used, but
     this can't be done directly in cross-compilation.  You must make
     your own arrangements to provide suitable library functions for
     cross-compilation.

`-mhard-float'
     Generate output containing floating point instructions.  This is
     the default if you use the unmodified sources.

`-mabicalls'
`-mno-abicalls'
     Emit (or do not emit) the pseudo operations `.abicalls',
     `.cpload', and `.cprestore' that some System V.4 ports use for
     position independent code.

`-mlong-calls'
`-mno-long-calls'
     Do all calls with the `JALR' instruction, which requires loading
     up a function's address into a register before the call.  You need
     to use this switch, if you call outside of the current 512
     megabyte segment to functions that are not through pointers.

`-mhalf-pic'
`-mno-half-pic'
     Put pointers to extern references into the data section and load
     them up, rather than put the references in the text section.

`-membedded-pic'
`-mno-embedded-pic'
     Generate PIC code suitable for some embedded systems.  All calls
     are made using PC relative address, and all data is addressed
     using the $gp register.  No more than 65536 bytes of global data
     may be used.  This requires GNU as and GNU ld which do most of the
     work.  This currently only works on targets which use ECOFF; it
     does not work with ELF.

`-membedded-data'
`-mno-embedded-data'
     Allocate variables to the read-only data section first if
     possible, then next in the small data section if possible,
     otherwise in data.  This gives slightly slower code than the
     default, but reduces the amount of RAM required when executing,
     and thus may be preferred for some embedded systems.

`-muninit-const-in-rodata'
`-mno-uninit-const-in-rodata'
     When used together with `-membedded-data', it will always store
     uninitialized const variables in the read-only data section.

`-msingle-float'
`-mdouble-float'
     The `-msingle-float' switch tells gcc to assume that the floating
     point coprocessor only supports single precision operations, as on
     the `r4650' chip.  The `-mdouble-float' switch permits gcc to use
     double precision operations.  This is the default.

`-mmad'
`-mno-mad'
     Permit use of the `mad', `madu' and `mul' instructions, as on the
     `r4650' chip.

`-m4650'
     Turns on `-msingle-float', `-mmad', and, at least for now,
     `-mcpu=r4650'.

`-mips16'
`-mno-mips16'
     Enable 16-bit instructions.

`-mentry'
     Use the entry and exit pseudo ops.  This option can only be used
     with `-mips16'.

`-EL'
     Compile code for the processor in little endian mode.  The
     requisite libraries are assumed to exist.

`-EB'
     Compile code for the processor in big endian mode.  The requisite
     libraries are assumed to exist.

`-G NUM'
     Put global and static items less than or equal to NUM bytes into
     the small data or bss sections instead of the normal data or bss
     section.  This allows the assembler to emit one word memory
     reference instructions based on the global pointer (GP or $28),
     instead of the normal two words used.  By default, NUM is 8 when
     the MIPS assembler is used, and 0 when the GNU assembler is used.
     The `-G NUM' switch is also passed to the assembler and linker.
     All modules should be compiled with the same `-G NUM' value.

`-nocpp'
     Tell the MIPS assembler to not run its preprocessor over user
     assembler files (with a `.s' suffix) when assembling them.

`-mfix7000'
     Pass an option to gas which will cause nops to be inserted if the
     read of the destination register of an mfhi or mflo instruction
     occurs in the following two instructions.

`-no-crt0'
     Do not include the default crt0.

`-mflush-func=FUNC'
`-mno-flush-func'
     Specifies the function to call to flush the I and D caches, or to
     not call any such function.  If called, the function must take the
     same arguments as the common `_flush_func()', that is, the address
     of the memory range for which the cache is being flushed, the size
     of the memory range, and the number 3 (to flush both caches).  The
     default depends on the target gcc was configured for, but commonly
     is either `_flush_func' or `__cpu_flush'.

   These options are defined by the macro `TARGET_SWITCHES' in the
machine description.  The default for the options is also defined by
that macro, which enables you to change the defaults.


File: gcc.info,  Node: i386 and x86-64 Options,  Next: HPPA Options,  Prev: MIPS Options,  Up: Submodel Options

Intel 386 and AMD x86-64 Options
--------------------------------

   These `-m' options are defined for the i386 and x86-64 family of
computers:

`-mcpu=CPU-TYPE'
     Tune to CPU-TYPE everything applicable about the generated code,
     except for the ABI and the set of available instructions.  The
     choices for CPU-TYPE are `i386', `i486', `i586', `i686',
     `pentium', `pentium-mmx', `pentiumpro', `pentium2', `pentium3',
     `pentium4', `k6', `k6-2', `k6-3', `athlon', `athlon-tbird',
     `athlon-4', `athlon-xp' and `athlon-mp'.

     While picking a specific CPU-TYPE will schedule things
     appropriately for that particular chip, the compiler will not
     generate any code that does not run on the i386 without the
     `-march=CPU-TYPE' option being used.  `i586' is equivalent to
     `pentium' and `i686' is equivalent to `pentiumpro'.  `k6' and
     `athlon' are the AMD chips as opposed to the Intel ones.

`-march=CPU-TYPE'
     Generate instructions for the machine type CPU-TYPE.  The choices
     for CPU-TYPE are the same as for `-mcpu'.  Moreover, specifying
     `-march=CPU-TYPE' implies `-mcpu=CPU-TYPE'.

`-m386'
`-m486'
`-mpentium'
`-mpentiumpro'
     These options are synonyms for `-mcpu=i386', `-mcpu=i486',
     `-mcpu=pentium', and `-mcpu=pentiumpro' respectively.  These
     synonyms are deprecated.

`-mfpmath=UNIT'
     generate floating point arithmetics for selected unit UNIT.  the
     choices for UNIT are:

    `387'
          Use the standard 387 floating point coprocessor present
          majority of chips and emulated otherwise.  Code compiled with
          this option will run almost everywhere.  The temporary
          results are computed in 80bit precesion instead of precision
          specified by the type resulting in slightly different results
          compared to most of other chips. See `-ffloat-store' for more
          detailed description.

          This is the default choice for i386 compiler.

    `sse'
          Use scalar floating point instructions present in the SSE
          instruction set.  This instruction set is supported by
          Pentium3 and newer chips, in the AMD line by Athlon-4,
          Athlon-xp and Athlon-mp chips.  The earlier version of SSE
          instruction set supports only single precision arithmetics,
          thus the double and extended precision arithmetics is still
          done using 387.  Later version, present only in Pentium4 and
          the future AMD x86-64 chips supports double precision
          arithmetics too.

          For i387 you need to use `-march=CPU-TYPE', `-msse' or
          `-msse2' switches to enable SSE extensions and make this
          option effective.  For x86-64 compiler, these extensions are
          enabled by default.

          The resulting code should be considerably faster in majority
          of cases and avoid the numerical instability problems of 387
          code, but may break some existing code that expects
          temporaries to be 80bit.

          This is the default choice for x86-64 compiler.

    `sse,387'
          Attempt to utilize both instruction sets at once.  This
          effectivly double the amount of available registers and on
          chips with separate execution units for 387 and SSE the
          execution resources too.  Use this option with care, as it is
          still experimental, because gcc register allocator does not
          model separate functional units well resulting in instable
          performance.

`-masm=DIALECT'
     Output asm instructions using selected DIALECT. Supported choices
     are `intel' or `att' (the default one).

`-mieee-fp'
`-mno-ieee-fp'
     Control whether or not the compiler uses IEEE floating point
     comparisons.  These handle correctly the case where the result of a
     comparison is unordered.

`-msoft-float'
     Generate output containing library calls for floating point.
     *Warning:* the requisite libraries are not part of GCC.  Normally
     the facilities of the machine's usual C compiler are used, but
     this can't be done directly in cross-compilation.  You must make
     your own arrangements to provide suitable library functions for
     cross-compilation.

     On machines where a function returns floating point results in the
     80387 register stack, some floating point opcodes may be emitted
     even if `-msoft-float' is used.

`-mno-fp-ret-in-387'
     Do not use the FPU registers for return values of functions.

     The usual calling convention has functions return values of types
     `float' and `double' in an FPU register, even if there is no FPU.
     The idea is that the operating system should emulate an FPU.

     The option `-mno-fp-ret-in-387' causes such values to be returned
     in ordinary CPU registers instead.

`-mno-fancy-math-387'
     Some 387 emulators do not support the `sin', `cos' and `sqrt'
     instructions for the 387.  Specify this option to avoid generating
     those instructions.  This option is the default on FreeBSD,
     OpenBSD and NetBSD.  This option is overridden when `-march'
     indicates that the target cpu will always have an FPU and so the
     instruction will not need emulation.  As of revision 2.6.1, these
     instructions are not generated unless you also use the
     `-funsafe-math-optimizations' switch.

`-malign-double'
`-mno-align-double'
     Control whether GCC aligns `double', `long double', and `long
     long' variables on a two word boundary or a one word boundary.
     Aligning `double' variables on a two word boundary will produce
     code that runs somewhat faster on a `Pentium' at the expense of
     more memory.

     *Warning:* if you use the `-malign-double' switch, structures
     containing the above types will be aligned differently than the
     published application binary interface specifications for the 386
     and will not be binary compatible with structures in code compiled
     without that switch.

`-m128bit-long-double'
     Control the size of `long double' type. i386 application binary
     interface specify the size to be 12 bytes, while modern
     architectures (Pentium and newer) prefer `long double' aligned to
     8 or 16 byte boundary.  This is impossible to reach with 12 byte
     long doubles in the array accesses.

     *Warning:* if you use the `-m128bit-long-double' switch, the
     structures and arrays containing `long double' will change their
     size as well as function calling convention for function taking
     `long double' will be modified.

`-m96bit-long-double'
     Set the size of `long double' to 96 bits as required by the i386
     application binary interface.  This is the default.

`-msvr3-shlib'
`-mno-svr3-shlib'
     Control whether GCC places uninitialized local variables into the
     `bss' or `data' segments.  `-msvr3-shlib' places them into `bss'.
     These options are meaningful only on System V Release 3.

`-mrtd'
     Use a different function-calling convention, in which functions
     that take a fixed number of arguments return with the `ret' NUM
     instruction, which pops their arguments while returning.  This
     saves one instruction in the caller since there is no need to pop
     the arguments there.

     You can specify that an individual function is called with this
     calling sequence with the function attribute `stdcall'.  You can
     also override the `-mrtd' option by using the function attribute
     `cdecl'.  *Note Function Attributes::.

     *Warning:* this calling convention is incompatible with the one
     normally used on Unix, so you cannot use it if you need to call
     libraries compiled with the Unix compiler.

     Also, you must provide function prototypes for all functions that
     take variable numbers of arguments (including `printf'); otherwise
     incorrect code will be generated for calls to those functions.

     In addition, seriously incorrect code will result if you call a
     function with too many arguments.  (Normally, extra arguments are
     harmlessly ignored.)

`-mregparm=NUM'
     Control how many registers are used to pass integer arguments.  By
     default, no registers are used to pass arguments, and at most 3
     registers can be used.  You can control this behavior for a
     specific function by using the function attribute `regparm'.
     *Note Function Attributes::.

     *Warning:* if you use this switch, and NUM is nonzero, then you
     must build all modules with the same value, including any
     libraries.  This includes the system libraries and startup modules.

`-mpreferred-stack-boundary=NUM'
     Attempt to keep the stack boundary aligned to a 2 raised to NUM
     byte boundary.  If `-mpreferred-stack-boundary' is not specified,
     the default is 4 (16 bytes or 128 bits), except when optimizing
     for code size (`-Os'), in which case the default is the minimum
     correct alignment (4 bytes for x86, and 8 bytes for x86-64).

     On Pentium and PentiumPro, `double' and `long double' values
     should be aligned to an 8 byte boundary (see `-malign-double') or
     suffer significant run time performance penalties.  On Pentium
     III, the Streaming SIMD Extension (SSE) data type `__m128' suffers
     similar penalties if it is not 16 byte aligned.

     To ensure proper alignment of this values on the stack, the stack
     boundary must be as aligned as that required by any value stored
     on the stack.  Further, every function must be generated such that
     it keeps the stack aligned.  Thus calling a function compiled with
     a higher preferred stack boundary from a function compiled with a
     lower preferred stack boundary will most likely misalign the
     stack.  It is recommended that libraries that use callbacks always
     use the default setting.

     This extra alignment does consume extra stack space, and generally
     increases code size.  Code that is sensitive to stack space usage,
     such as embedded systems and operating system kernels, may want to
     reduce the preferred alignment to `-mpreferred-stack-boundary=2'.

`-mmmx'
`-mno-mmx'

`-msse'
`-mno-sse'

`-msse2'
`-mno-sse2'

`-m3dnow'
`-mno-3dnow'
     These switches enable or disable the use of built-in functions
     that allow direct access to the MMX, SSE and 3Dnow extensions of
     the instruction set.

     *Note X86 Built-in Functions::, for details of the functions
     enabled and disabled by these switches.

     To have SSE/SSE2 instructions generated automatically from
     floating-point code, see `-mfpmath=sse'.

`-mpush-args'
`-mno-push-args'
     Use PUSH operations to store outgoing parameters.  This method is
     shorter and usually equally fast as method using SUB/MOV
     operations and is enabled by default.  In some cases disabling it
     may improve performance because of improved scheduling and reduced
     dependencies.

`-maccumulate-outgoing-args'
     If enabled, the maximum amount of space required for outgoing
     arguments will be computed in the function prologue.  This is
     faster on most modern CPUs because of reduced dependencies,
     improved scheduling and reduced stack usage when preferred stack
     boundary is not equal to 2.  The drawback is a notable increase in
     code size.  This switch implies `-mno-push-args'.

`-mthreads'
     Support thread-safe exception handling on `Mingw32'.  Code that
     relies on thread-safe exception handling must compile and link all
     code with the `-mthreads' option.  When compiling, `-mthreads'
     defines `-D_MT'; when linking, it links in a special thread helper
     library `-lmingwthrd' which cleans up per thread exception
     handling data.

`-mno-align-stringops'
     Do not align destination of inlined string operations.  This
     switch reduces code size and improves performance in case the
     destination is already aligned, but gcc don't know about it.

`-minline-all-stringops'
     By default GCC inlines string operations only when destination is
     known to be aligned at least to 4 byte boundary.  This enables
     more inlining, increase code size, but may improve performance of
     code that depends on fast memcpy, strlen and memset for short
     lengths.

`-momit-leaf-frame-pointer'
     Don't keep the frame pointer in a register for leaf functions.
     This avoids the instructions to save, set up and restore frame
     pointers and makes an extra register available in leaf functions.
     The option `-fomit-frame-pointer' removes the frame pointer for
     all functions which might make debugging harder.

   These `-m' switches are supported in addition to the above on AMD
x86-64 processors in 64-bit environments.

`-m32'
`-m64'
     Generate code for a 32-bit or 64-bit environment.  The 32-bit
     environment sets int, long and pointer to 32 bits and generates
     code that runs on any i386 system.  The 64-bit environment sets
     int to 32 bits and long and pointer to 64 bits and generates code
     for AMD's x86-64 architecture.

`-mno-red-zone'
     Do not use a so called red zone for x86-64 code.  The red zone is
     mandated by the x86-64 ABI, it is a 128-byte area beyond the
     location of the stack pointer that will not be modified by signal
     or interrupt handlers and therefore can be used for temporary data
     without adjusting the stack pointer.  The flag `-mno-red-zone'
     disables this red zone.

`-mcmodel=small'
     Generate code for the small code model: the program and its
     symbols must be linked in the lower 2 GB of the address space.
     Pointers are 64 bits.  Programs can be statically or dynamically
     linked.  This is the default code model.

`-mcmodel=kernel'
     Generate code for the kernel code model.  The kernel runs in the
     negative 2 GB of the address space.  This model has to be used for
     Linux kernel code.

`-mcmodel=medium'
     Generate code for the medium model: The program is linked in the
     lower 2 GB of the address space but symbols can be located
     anywhere in the address space.  Programs can be statically or
     dynamically linked, but building of shared libraries are not
     supported with the medium model.

`-mcmodel=large'
     Generate code for the large model: This model makes no assumptions
     about addresses and sizes of sections.  Currently GCC does not
     implement this model.


File: gcc.info,  Node: HPPA Options,  Next: Intel 960 Options,  Prev: i386 and x86-64 Options,  Up: Submodel Options

HPPA Options
------------

   These `-m' options are defined for the HPPA family of computers:

`-march=ARCHITECTURE-TYPE'
     Generate code for the specified architecture.  The choices for
     ARCHITECTURE-TYPE are `1.0' for PA 1.0, `1.1' for PA 1.1, and
     `2.0' for PA 2.0 processors.  Refer to `/usr/lib/sched.models' on
     an HP-UX system to determine the proper architecture option for
     your machine.  Code compiled for lower numbered architectures will
     run on higher numbered architectures, but not the other way around.

     PA 2.0 support currently requires gas snapshot 19990413 or later.
     The next release of binutils (current is 2.9.1) will probably
     contain PA 2.0 support.

`-mpa-risc-1-0'
`-mpa-risc-1-1'
`-mpa-risc-2-0'
     Synonyms for `-march=1.0', `-march=1.1', and `-march=2.0'
     respectively.

`-mbig-switch'
     Generate code suitable for big switch tables.  Use this option
     only if the assembler/linker complain about out of range branches
     within a switch table.

`-mjump-in-delay'
     Fill delay slots of function calls with unconditional jump
     instructions by modifying the return pointer for the function call
     to be the target of the conditional jump.

`-mdisable-fpregs'
     Prevent floating point registers from being used in any manner.
     This is necessary for compiling kernels which perform lazy context
     switching of floating point registers.  If you use this option and
     attempt to perform floating point operations, the compiler will
     abort.

`-mdisable-indexing'
     Prevent the compiler from using indexing address modes.  This
     avoids some rather obscure problems when compiling MIG generated
     code under MACH.

`-mno-space-regs'
     Generate code that assumes the target has no space registers.
     This allows GCC to generate faster indirect calls and use unscaled
     index address modes.

     Such code is suitable for level 0 PA systems and kernels.

`-mfast-indirect-calls'
     Generate code that assumes calls never cross space boundaries.
     This allows GCC to emit code which performs faster indirect calls.

     This option will not work in the presence of shared libraries or
     nested functions.

`-mlong-load-store'
     Generate 3-instruction load and store sequences as sometimes
     required by the HP-UX 10 linker.  This is equivalent to the `+k'
     option to the HP compilers.

`-mportable-runtime'
     Use the portable calling conventions proposed by HP for ELF
     systems.

`-mgas'
     Enable the use of assembler directives only GAS understands.

`-mschedule=CPU-TYPE'
     Schedule code according to the constraints for the machine type
     CPU-TYPE.  The choices for CPU-TYPE are `700' `7100', `7100LC',
     `7200', and `8000'.  Refer to `/usr/lib/sched.models' on an HP-UX
     system to determine the proper scheduling option for your machine.

`-mlinker-opt'
     Enable the optimization pass in the HPUX linker.  Note this makes
     symbolic debugging impossible.  It also triggers a bug in the HPUX
     8 and HPUX 9 linkers in which they give bogus error messages when
     linking some programs.

`-msoft-float'
     Generate output containing library calls for floating point.
     *Warning:* the requisite libraries are not available for all HPPA
     targets.  Normally the facilities of the machine's usual C
     compiler are used, but this cannot be done directly in
     cross-compilation.  You must make your own arrangements to provide
     suitable library functions for cross-compilation.  The embedded
     target `hppa1.1-*-pro' does provide software floating point
     support.

     `-msoft-float' changes the calling convention in the output file;
     therefore, it is only useful if you compile _all_ of a program with
     this option.  In particular, you need to compile `libgcc.a', the
     library that comes with GCC, with `-msoft-float' in order for this
     to work.


File: gcc.info,  Node: Intel 960 Options,  Next: DEC Alpha Options,  Prev: HPPA Options,  Up: Submodel Options

Intel 960 Options
-----------------

   These `-m' options are defined for the Intel 960 implementations:

`-mCPU-TYPE'
     Assume the defaults for the machine type CPU-TYPE for some of the
     other options, including instruction scheduling, floating point
     support, and addressing modes.  The choices for CPU-TYPE are `ka',
     `kb', `mc', `ca', `cf', `sa', and `sb'.  The default is `kb'.

`-mnumerics'
`-msoft-float'
     The `-mnumerics' option indicates that the processor does support
     floating-point instructions.  The `-msoft-float' option indicates
     that floating-point support should not be assumed.

`-mleaf-procedures'
`-mno-leaf-procedures'
     Do (or do not) attempt to alter leaf procedures to be callable
     with the `bal' instruction as well as `call'.  This will result in
     more efficient code for explicit calls when the `bal' instruction
     can be substituted by the assembler or linker, but less efficient
     code in other cases, such as calls via function pointers, or using
     a linker that doesn't support this optimization.

`-mtail-call'
`-mno-tail-call'
     Do (or do not) make additional attempts (beyond those of the
     machine-independent portions of the compiler) to optimize
     tail-recursive calls into branches.  You may not want to do this
     because the detection of cases where this is not valid is not
     totally complete.  The default is `-mno-tail-call'.

`-mcomplex-addr'
`-mno-complex-addr'
     Assume (or do not assume) that the use of a complex addressing
     mode is a win on this implementation of the i960.  Complex
     addressing modes may not be worthwhile on the K-series, but they
     definitely are on the C-series.  The default is currently
     `-mcomplex-addr' for all processors except the CB and CC.

`-mcode-align'
`-mno-code-align'
     Align code to 8-byte boundaries for faster fetching (or don't
     bother).  Currently turned on by default for C-series
     implementations only.

`-mic-compat'
`-mic2.0-compat'
`-mic3.0-compat'
     Enable compatibility with iC960 v2.0 or v3.0.

`-masm-compat'
`-mintel-asm'
     Enable compatibility with the iC960 assembler.

`-mstrict-align'
`-mno-strict-align'
     Do not permit (do permit) unaligned accesses.

`-mold-align'
     Enable structure-alignment compatibility with Intel's gcc release
     version 1.3 (based on gcc 1.37).  This option implies
     `-mstrict-align'.

`-mlong-double-64'
     Implement type `long double' as 64-bit floating point numbers.
     Without the option `long double' is implemented by 80-bit floating
     point numbers.  The only reason we have it because there is no
     128-bit `long double' support in `fp-bit.c' yet.  So it is only
     useful for people using soft-float targets.  Otherwise, we should
     recommend against use of it.


File: gcc.info,  Node: DEC Alpha Options,  Next: DEC Alpha/VMS Options,  Prev: Intel 960 Options,  Up: Submodel Options

DEC Alpha Options
-----------------

   These `-m' options are defined for the DEC Alpha implementations:

`-mno-soft-float'
`-msoft-float'
     Use (do not use) the hardware floating-point instructions for
     floating-point operations.  When `-msoft-float' is specified,
     functions in `libgcc.a' will be used to perform floating-point
     operations.  Unless they are replaced by routines that emulate the
     floating-point operations, or compiled in such a way as to call
     such emulations routines, these routines will issue floating-point
     operations.   If you are compiling for an Alpha without
     floating-point operations, you must ensure that the library is
     built so as not to call them.

     Note that Alpha implementations without floating-point operations
     are required to have floating-point registers.

`-mfp-reg'
`-mno-fp-regs'
     Generate code that uses (does not use) the floating-point register
     set.  `-mno-fp-regs' implies `-msoft-float'.  If the floating-point
     register set is not used, floating point operands are passed in
     integer registers as if they were integers and floating-point
     results are passed in `$0' instead of `$f0'.  This is a
     non-standard calling sequence, so any function with a
     floating-point argument or return value called by code compiled
     with `-mno-fp-regs' must also be compiled with that option.

     A typical use of this option is building a kernel that does not
     use, and hence need not save and restore, any floating-point
     registers.

`-mieee'
     The Alpha architecture implements floating-point hardware
     optimized for maximum performance.  It is mostly compliant with
     the IEEE floating point standard.  However, for full compliance,
     software assistance is required.  This option generates code fully
     IEEE compliant code _except_ that the INEXACT-FLAG is not
     maintained (see below).  If this option is turned on, the
     preprocessor macro `_IEEE_FP' is defined during compilation.  The
     resulting code is less efficient but is able to correctly support
     denormalized numbers and exceptional IEEE values such as
     not-a-number and plus/minus infinity.  Other Alpha compilers call
     this option `-ieee_with_no_inexact'.

`-mieee-with-inexact'
     This is like `-mieee' except the generated code also maintains the
     IEEE INEXACT-FLAG.  Turning on this option causes the generated
     code to implement fully-compliant IEEE math.  In addition to
     `_IEEE_FP', `_IEEE_FP_EXACT' is defined as a preprocessor macro.
     On some Alpha implementations the resulting code may execute
     significantly slower than the code generated by default.  Since
     there is very little code that depends on the INEXACT-FLAG, you
     should normally not specify this option.  Other Alpha compilers
     call this option `-ieee_with_inexact'.

`-mfp-trap-mode=TRAP-MODE'
     This option controls what floating-point related traps are enabled.
     Other Alpha compilers call this option `-fptm TRAP-MODE'.  The
     trap mode can be set to one of four values:

    `n'
          This is the default (normal) setting.  The only traps that
          are enabled are the ones that cannot be disabled in software
          (e.g., division by zero trap).

    `u'
          In addition to the traps enabled by `n', underflow traps are
          enabled as well.

    `su'
          Like `su', but the instructions are marked to be safe for
          software completion (see Alpha architecture manual for
          details).

    `sui'
          Like `su', but inexact traps are enabled as well.

`-mfp-rounding-mode=ROUNDING-MODE'
     Selects the IEEE rounding mode.  Other Alpha compilers call this
     option `-fprm ROUNDING-MODE'.  The ROUNDING-MODE can be one of:

    `n'
          Normal IEEE rounding mode.  Floating point numbers are
          rounded towards the nearest machine number or towards the
          even machine number in case of a tie.

    `m'
          Round towards minus infinity.

    `c'
          Chopped rounding mode.  Floating point numbers are rounded
          towards zero.

    `d'
          Dynamic rounding mode.  A field in the floating point control
          register (FPCR, see Alpha architecture reference manual)
          controls the rounding mode in effect.  The C library
          initializes this register for rounding towards plus infinity.
          Thus, unless your program modifies the FPCR, `d' corresponds
          to round towards plus infinity.

`-mtrap-precision=TRAP-PRECISION'
     In the Alpha architecture, floating point traps are imprecise.
     This means without software assistance it is impossible to recover
     from a floating trap and program execution normally needs to be
     terminated.  GCC can generate code that can assist operating
     system trap handlers in determining the exact location that caused
     a floating point trap.  Depending on the requirements of an
     application, different levels of precisions can be selected:

    `p'
          Program precision.  This option is the default and means a
          trap handler can only identify which program caused a
          floating point exception.

    `f'
          Function precision.  The trap handler can determine the
          function that caused a floating point exception.

    `i'
          Instruction precision.  The trap handler can determine the
          exact instruction that caused a floating point exception.

     Other Alpha compilers provide the equivalent options called
     `-scope_safe' and `-resumption_safe'.

`-mieee-conformant'
     This option marks the generated code as IEEE conformant.  You must
     not use this option unless you also specify `-mtrap-precision=i'
     and either `-mfp-trap-mode=su' or `-mfp-trap-mode=sui'.  Its only
     effect is to emit the line `.eflag 48' in the function prologue of
     the generated assembly file.  Under DEC Unix, this has the effect
     that IEEE-conformant math library routines will be linked in.

`-mbuild-constants'
     Normally GCC examines a 32- or 64-bit integer constant to see if
     it can construct it from smaller constants in two or three
     instructions.  If it cannot, it will output the constant as a
     literal and generate code to load it from the data segment at
     runtime.

     Use this option to require GCC to construct _all_ integer constants
     using code, even if it takes more instructions (the maximum is
     six).

     You would typically use this option to build a shared library
     dynamic loader.  Itself a shared library, it must relocate itself
     in memory before it can find the variables and constants in its
     own data segment.

`-malpha-as'
`-mgas'
     Select whether to generate code to be assembled by the
     vendor-supplied assembler (`-malpha-as') or by the GNU assembler
     `-mgas'.

`-mbwx'
`-mno-bwx'
`-mcix'
`-mno-cix'
`-mfix'
`-mno-fix'
`-mmax'
`-mno-max'
     Indicate whether GCC should generate code to use the optional BWX,
     CIX, FIX and MAX instruction sets.  The default is to use the
     instruction sets supported by the CPU type specified via `-mcpu='
     option or that of the CPU on which GCC was built if none was
     specified.

`-mfloat-vax'
`-mfloat-ieee'
     Generate code that uses (does not use) VAX F and G floating point
     arithmetic instead of IEEE single and double precision.

`-mexplicit-relocs'
`-mno-explicit-relocs'
     Older Alpha assemblers provided no way to generate symbol
     relocations except via assembler macros.  Use of these macros does
     not allow optimial instruction scheduling.  GNU binutils as of
     version 2.12 supports a new syntax that allows the compiler to
     explicitly mark which relocations should apply to which
     instructions.  This option is mostly useful for debugging, as GCC
     detects the capabilities of the assembler when it is built and
     sets the default accordingly.

`-msmall-data'
`-mlarge-data'
     When `-mexplicit-relocs' is in effect, static data is accessed via
     "gp-relative" relocations.  When `-msmall-data' is used, objects 8
     bytes long or smaller are placed in a "small data area" (the
     `.sdata' and `.sbss' sections) and are accessed via 16-bit
     relocations off of the `$gp' register.  This limits the size of
     the small data area to 64KB, but allows the variables to be
     directly accessed via a single instruction.

     The default is `-mlarge-data'.  With this option the data area is
     limited to just below 2GB.  Programs that require more than 2GB of
     data must use `malloc' or `mmap' to allocate the data in the heap
     instead of in the program's data segment.

     When generating code for shared libraries, `-fpic' implies
     `-msmall-data' and `-fPIC' implies `-mlarge-data'.

`-mcpu=CPU_TYPE'
     Set the instruction set and instruction scheduling parameters for
     machine type CPU_TYPE.  You can specify either the `EV' style name
     or the corresponding chip number.  GCC supports scheduling
     parameters for the EV4, EV5 and EV6 family of processors and will
     choose the default values for the instruction set from the
     processor you specify.  If you do not specify a processor type,
     GCC will default to the processor on which the compiler was built.

     Supported values for CPU_TYPE are

    `ev4'

    `ev45'
    `21064'
          Schedules as an EV4 and has no instruction set extensions.

    `ev5'
    `21164'
          Schedules as an EV5 and has no instruction set extensions.

    `ev56'
    `21164a'
          Schedules as an EV5 and supports the BWX extension.

    `pca56'
    `21164pc'
    `21164PC'
          Schedules as an EV5 and supports the BWX and MAX extensions.

    `ev6'
    `21264'
          Schedules as an EV6 and supports the BWX, FIX, and MAX
          extensions.

    `ev67'

    `21264a'
          Schedules as an EV6 and supports the BWX, CIX, FIX, and MAX
          extensions.

`-mtune=CPU_TYPE'
     Set only the instruction scheduling parameters for machine type
     CPU_TYPE.  The instruction set is not changed.

`-mmemory-latency=TIME'
     Sets the latency the scheduler should assume for typical memory
     references as seen by the application.  This number is highly
     dependent on the memory access patterns used by the application
     and the size of the external cache on the machine.

     Valid options for TIME are

    `NUMBER'
          A decimal number representing clock cycles.

    `L1'
    `L2'
    `L3'
    `main'
          The compiler contains estimates of the number of clock cycles
          for "typical" EV4 & EV5 hardware for the Level 1, 2 & 3 caches
          (also called Dcache, Scache, and Bcache), as well as to main
          memory.  Note that L3 is only valid for EV5.


File: gcc.info,  Node: DEC Alpha/VMS Options,  Next: Clipper Options,  Prev: DEC Alpha Options,  Up: Submodel Options

DEC Alpha/VMS Options
---------------------

   These `-m' options are defined for the DEC Alpha/VMS implementations:

`-mvms-return-codes'
     Return VMS condition codes from main.  The default is to return
     POSIX style condition (e.g. error) codes.


File: gcc.info,  Node: Clipper Options,  Next: H8/300 Options,  Prev: DEC Alpha/VMS Options,  Up: Submodel Options

Clipper Options
---------------

   These `-m' options are defined for the Clipper implementations:

`-mc300'
     Produce code for a C300 Clipper processor.  This is the default.

`-mc400'
     Produce code for a C400 Clipper processor, i.e. use floating point
     registers f8-f15.


File: gcc.info,  Node: H8/300 Options,  Next: SH Options,  Prev: Clipper Options,  Up: Submodel Options

H8/300 Options
--------------

   These `-m' options are defined for the H8/300 implementations:

`-mrelax'
     Shorten some address references at link time, when possible; uses
     the linker option `-relax'.  *Note `ld' and the H8/300:
     (ld.info)H8/300, for a fuller description.

`-mh'
     Generate code for the H8/300H.

`-ms'
     Generate code for the H8/S.

`-ms2600'
     Generate code for the H8/S2600.  This switch must be used with
     `-ms'.

`-mint32'
     Make `int' data 32 bits by default.

`-malign-300'
     On the H8/300H and H8/S, use the same alignment rules as for the
     H8/300.  The default for the H8/300H and H8/S is to align longs
     and floats on 4 byte boundaries.  `-malign-300' causes them to be
     aligned on 2 byte boundaries.  This option has no effect on the
     H8/300.


File: gcc.info,  Node: SH Options,  Next: System V Options,  Prev: H8/300 Options,  Up: Submodel Options

SH Options
----------

   These `-m' options are defined for the SH implementations:

`-m1'
     Generate code for the SH1.

`-m2'
     Generate code for the SH2.

`-m3'
     Generate code for the SH3.

`-m3e'
     Generate code for the SH3e.

`-m4-nofpu'
     Generate code for the SH4 without a floating-point unit.

`-m4-single-only'
     Generate code for the SH4 with a floating-point unit that only
     supports single-precision arithmetic.

`-m4-single'
     Generate code for the SH4 assuming the floating-point unit is in
     single-precision mode by default.

`-m4'
     Generate code for the SH4.

`-mb'
     Compile code for the processor in big endian mode.

`-ml'
     Compile code for the processor in little endian mode.

`-mdalign'
     Align doubles at 64-bit boundaries.  Note that this changes the
     calling conventions, and thus some functions from the standard C
     library will not work unless you recompile it first with
     `-mdalign'.

`-mrelax'
     Shorten some address references at link time, when possible; uses
     the linker option `-relax'.

`-mbigtable'
     Use 32-bit offsets in `switch' tables.  The default is to use
     16-bit offsets.

`-mfmovd'
     Enable the use of the instruction `fmovd'.

`-mhitachi'
     Comply with the calling conventions defined by Hitachi.

`-mnomacsave'
     Mark the `MAC' register as call-clobbered, even if `-mhitachi' is
     given.

`-mieee'
     Increase IEEE-compliance of floating-point code.

`-misize'
     Dump instruction size and location in the assembly code.

`-mpadstruct'
     This option is deprecated.  It pads structures to multiple of 4
     bytes, which is incompatible with the SH ABI.

`-mspace'
     Optimize for space instead of speed.  Implied by `-Os'.

`-mprefergot'
     When generating position-independent code, emit function calls
     using the Global Offset Table instead of the Procedure Linkage
     Table.

`-musermode'
     Generate a library function call to invalidate instruction cache
     entries, after fixing up a trampoline.  This library function call
     doesn't assume it can write to the whole memory address space.
     This is the default when the target is `sh-*-linux*'.


File: gcc.info,  Node: System V Options,  Next: TMS320C3x/C4x Options,  Prev: SH Options,  Up: Submodel Options

Options for System V
--------------------

   These additional options are available on System V Release 4 for
compatibility with other compilers on those systems:

`-G'
     Create a shared object.  It is recommended that `-symbolic' or
     `-shared' be used instead.

`-Qy'
     Identify the versions of each tool used by the compiler, in a
     `.ident' assembler directive in the output.

`-Qn'
     Refrain from adding `.ident' directives to the output file (this is
     the default).

`-YP,DIRS'
     Search the directories DIRS, and no others, for libraries
     specified with `-l'.

`-Ym,DIR'
     Look in the directory DIR to find the M4 preprocessor.  The
     assembler uses this option.

