InS_StArT
PE2ODI.COM
1.65                                    
^Xircom Pocket Ethernet Adapter II,PE2ODI.COM,IEM
?Installation for the Xircom Pocket Ethernet Adapter II.
*OIEM(FRAME) Frame type
?The latest ODI Specification uses Ethernet_802.2 as the default frame type.  If your network requires something other than Ethernet_802.2, then make sure to specify the correct frame type.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIEM() Force Non-Bidirectional Mode
?Select the NON keyword only if you wish to force non-bidirectional mode.
NON
InS_EnD

