
                      SILPHEED VERSION 2.2 


SUBJECT:  VOLUME CONTROL

        SILPHEED version 2.2 has a volume control feature for several
        music driver types. The driver types for which volume control 
        has been implemented are:

                ROLAND MT32/MT-100 SOUND MODULE
                IBM MUSIC FEATURE CARD
                AD LIB MUSIC SYNTHESIZER CARD
                PCJR
                TANDY 1000 SERIES

        
        
        The keys used for volume control are the following:

                Volume Up   press the =(+) key

                Volume down press the -(_) key

        Press the appropriate key and hold until the desired volume 
        has been achieved.
