The Amateur Radio Project - Measurements

# Measurements

### Question 24 of 32

A sinusoidal voltage is correctly applied to an oscilloscope but the trace is too small. To enlarge the height of this trace, adjustment should be made to the control marked

1. X-shift
2. timebase (time/cm)
3. vertical amplifier (V/cm)
4. trigger level

1 | 2 | 3 | 4

Back |

page (tq2324)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details