The Amateur Radio Project - Practical resistors

# Practical resistors

### Question 6 of 6

A 68 resistor is in parallel with an 82 resistor. The combination is connected across a 6V supply. The rating of the 68 resistor and 82 resistor should be respectively

1. 1 W, 0.5 W
2. 1 W, 0.25W
3. 0.5W, 1 W
4. 0.5W, 0.5 W

1 | 2 | 3 | 4

Back |

page (tq0406)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details