The Amateur Radio Project - Simple alternating current circuits

# Simple alternating current circuits

### Question 6 of 14

A coil of negligible resistance has an inductance of 0.5H. It is connected across a 6V, 50Hz supply. The power dissipated in the coil will be

1. 15.7W
2. 2.62W
3. 38mW
4. zero

1 | 2 | 3 | 4

Back |

page (tq0806)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details