The Amateur Radio Project - Measurements

# Measurements

### Question 12 of 32

A moving coil multimeter of sensitivity 2000/V is set to ‘DC 20V’, and connected across terminals A and B in Fig. 23.1. The reading on the multimeter will be

1. 20V
2. 15V
3. 10V
4. 12V

1 | 2 | 3 | 4

Back |

page (tq2312)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details