The Amateur Radio Project - Receivers

# Receivers

### Question 10 of 22

A superheterodyne receiver is tuned to 7.1MHz and is receiving image interference from 8.03MHz. The local oscillator frequency and intermediate frequency will be respectively

1. 465kHz, 7.565MHz
2. 6.635MHz, 7.565kHz
3. 7.565MHz, 465kHz
4. 8.495MHz, 465kHz

1 | 2 | 3 | 4

Back |

page (tq2210)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details