The Amateur Radio Project - Operating procedures and practices

# Operating procedures and practices

### Question 15 of 21

A repeater can normally be accessed with a toneburst of

1. 1.75MHz for 500ms
2. 1.75kHz for 500ms
3. 1.75kHz for 5s
4. 1.75Hz for 50ms

1 | 2 | 3 | 4

Back |

page (tq2515)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details