The Amateur Radio Project - Resonance and its applications

# Resonance and its applications

### Question 5 of 16

A coil of inductance 125mH and resistance 2 is connected in series with a 2F capacitor. The resonant frequency of the circuit will be approximately

1. 320Hz
2. 640Hz
3. 1kHz
4. 2kHz

1 | 2 | 3 | 4

Back |

page (tq1005)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details