The Amateur Radio Project - Current, voltage and resistance

# Current, voltage and resistance

### Question 10 of 10

A battery has an open-circuit voltage of 24V. When delivering a load current of 2A its terminal voltage falls to 20 V. The internal resistance of the battery is

1. 12
2. 10
3. 6
4. 2

1 | 2 | 3 | 4

Back |

page (tq0110)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details