# Practical resistors

Resistors take many forms, dependent upon their power rating and use. They are manufactured to preferred ohmic values and power ratings, and will normally have a tolerance of 5%, 10% or 20%; closer tolerances are available for special purposes. A tolerance means its actual value can be above or below its quoted value.

Questions

page (t04)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details