The Amateur Radio Project - Transformers

# Transformers

### Question 2 of 8

The ratio of primary to secondary turns on a step-down transformer is 15:1. When 240V is applied to the primary winding, the secondary will have a terminal voltage of

1. 3600V
2. 256V
3. 16V
4. 4V

1 | 2 | 3 | 4

Back |

page (tq1102)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details