The Amateur Radio Project - Amplifiers

# Amplifiers

### Question 4 of 18

Some distortion normally occurs in class A amplification. This is because

1. the applied signal is changing
2. the zero bias only produces pulses at the output
3. the load resistance is non-linear
4. of the non-linearity of the transistor characteristic

1 | 2 | 3 | 4

Back |

page (tq1504)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details