# Measurements

## Multi-range meters

Many commercial multi-range meters are available, in both digital and analogue form. These consist of a number of voltage multipliers and current shunts, an instrument rectifier and current transformer, all of which are switched to provide a large number of DC and AC voltage and current ranges on a high-sensitivity meter.

A typical analogue Multi-Meter

A typical digital LCD Multi-Meter

Back | Index | Next