# Transmitter interference

### Explanation of question 5

With single sideband transmission, an AF bandwidth of 3kHz will produce an RF bandwidth of

1. 6kHz
2. 3kHz
3. 1.5kHz
4. 0.75kHz

The answer is :- 2 A single sideband transmission will have a bandwidth equal to the highest modulating frequency.

BACK

page (tq2405ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details