The Amateur Radio Project - F.M., A.M. and S.S.B. transmitters

# F.M., A.M. and S.S.B. transmitters

### Question 15 of 24

A frequency mixer circuit is supplied with two frequencies, f1 = 3.5MHz and f2 = 465kHz. A frequency which CANNOT appear at the output

1 | 2 | 3 | 4

Back |

page (tq1815)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details