The Amateur Radio Project - F.M., A.M. and S.S.B. transmitters

# F.M., A.M. and S.S.B. transmitters

### Question 8 of 24

A double-sideband AM transmitter has a carrier frequency of 14.3MHz and the highest audio modulating frequency is 3kHz. The bandwidth will be

1. 14 - 14.6MHz
2. 14.294 - 14.306MHz
3. 14.297 - 14.303MHz
4. 14.2985 - 14.3015MHz

1 | 2 | 3 | 4

Back |

page (tq1808)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details