The Amateur Radio Project - Resonance and its applications

# Resonance and its applications

### Question 4 of 16

A series circuit is resonant at a frequency of 4kHz. If the resistance of the circuit is doubled, the resonant frequency will be

1. 1kHz
2. 2kHz
3. 4kHz
4. 8kHz

1 | 2 | 3 | 4

Back |

page (tq1004)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details