The Amateur Radio Project - Measurements

# Measurements

### Question 23 of 32

- i An oscilloscope can only display a sine wave
- ii Vertical deflection of the electron beam of an oscilloscope is controlled by a voltage on the X-plates

1. i and ii are both true
2. i is true but ii is false
3. i is false but ii is true
4. i and ii are both false

1 | 2 | 3 | 4

Back |

page (tq2323)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details